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;;U Local Area Connection s annsion 5

soacsmu.acuk § Local Area Connection Properties =
Broadcom NetLink (TM) Gigabit ...

AOME - Zctero) Networing
Patition... Standalone

Interet Protocol Version 4 (ICP/IPvd) Propertes

General [ altermate Configuration

You can get I settings assigned automatially i your network supports
this capabiity. Otherwise, you need to ask your network adminstrator
for the appropriate P settngs.

© Obtain an IP address automaticaly
© Use the foloing I address:

1P address:

Subnet mask:

Default gateway:

® Obtain DI server address automaticaly
© Use the foloning DNS server addresses:
Preferred DIS server:

Alternate DS server:

[ validate settings upon exit
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Organize Disable this network device  Diagnose this connection  Rename this connection  View status of this connection  Change settings of this connection
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; Local Area Connection § Local Area Connection Status
Broadcom NetLink (TM) Gigabit ... Network Connection Details

o Netwat Conecton et
Property Valve

Connectionspecific DN~ soac smu ac.uk

Desciption Broadcom NetLink (TM) Gigabt Ethemet
Physical Address 8428.28.964D37

'DHCP Enabled Yes

P4 Address 19216827.218

P4 Subnet Mask 255.255.255.0

Lease Obtained 11 December 2015 14:22:07

Lesse Bpres 17 January 2152 20:5858

IPv4 Defaui Gateway 192168272

1Pv4 DHCP Server 192.16827.1

IPv4 DN Server 192.16827.1

1Pv4 WINS Server

NetBIOS over Tepip En.. Yes

Linkocal 1PV Address  fe8D:d5202533b849.0548%11

1Pv6 Defauk Gateway

1Pv6 DNS Server
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Options

Connection Settings B .

Configure Prosies to Access the Internet
© Noproxy
© Auto-detect proxy settings for this network
©) Use system prosy settings
© Manual proxy configuration:
HITP Proxys 193628855
Useths prowy server
SSLProgy (193628855
ETP Proy: 193628855
'SOCKS Host: | 193.62.88.55
SOCKSW @ SOCKS¥S
No Prosy for:

Port:

forall protocols

Port:
Pot:
Port:

st

Iocalhost, 127,001

Eample: mozilla.org, .net.nz, 192.168.1.0/24
© Automatic proxy configuration URL:
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