  ip                          Global IP configuration subcommands
  ipc                         Configure IPC system
  ipv6                        Global IPv6 configuration commands
  kron                        Kron interval Facility
  l2                          Layer 2
  lacp                        LACP configuration
  li-view                     LI View
  license                     license boot config commands
  line                        Configure a terminal line
  link                        Enable Link State Tracking feature
  lldp                        Global LLDP configuration subcommands
  location                    Global location configuration commands
  logging                     Modify message logging facilities
  login                       Enable secure login checking
  mab                         MAC Authentication Bypass Global Configuration
                              Commands
  mac                         Global MAC configuration subcommands
  macro                       Macro configuration
  map-class                   Configure static map class
  map-list                    Configure static map list
  memory                      Configure memory management
  mls                         mls global commands
  monitor                     Monitoring different system events
  network-policy              Network Policy
  nmsp                        NMSP configuration commands
  no                          Negate a command or set its defaults
  ntp                         Configure NTP
  parameter-map               Configure Parameter Map
  parser                      Configure parser
  passthru-domain-list        Domain name's associated with FQDN name
  pnp                         Configure PNP
  policy-map                  Configure Policy Map
  port-channel                EtherChannel configuration
  port-security               Security related command
  power                       Power configure
  priority-list               Build a priority list
  privilege                   Command privilege parameters
  process                     Configure process
  process-max-time            Maximum time for process to run before
                              voluntarily relinquishing processor
  psp                         Enable PSP
  qos                         Global QoS configuration subcommands
  queue-list                  Build a custom queue list
  regexp                      regexp commands
  rep                         Resilient Ethernet Protocol characteristics
  resource                    Configure Resource settings
  rmon                        Remote Monitoring
  router                      Enable a routing process
  sasl                        Configure SASL
  scheduler                   Scheduler parameters
  scripting                   Configure options for scripting languages
  service                     Modify use of network based services
  service-policy              Configure Global CPL Service Policy
  service-template            Configure a service-template/identity policy
  setup                       Configure setup options
  sflow                       change sFlow global configuration
  shell                       Configure shell command
  shutdown                    Shutdown system elements
  snmp                        Modify non engine SNMP parameters
  snmp-server                 Modify SNMP engine parameters
  source                      Get config from another source
  spanning-tree               Spanning Tree Subsystem
  stack-mac                   Global stack mac-address feature configurations
  stackmaker                  Specify stack name and add its member
  stacks                      Configure stacks
  standby                     Global HSRP configuration commands
  switch                      Config commands for the switches in the stack
  system                      Set the system configuration
  tacacs-server               Modify TACACS query parameters
  template                    Select a template to configure
  tftp-server                 Provide TFTP service for netload requests
  time-range                  Define time range entries
  udld                        Configure global UDLD setting
  user-name                   Establish User Name Authentication
  username                    Establish User Name Authentication
  vlan                        Vlan commands
  vtp                         Configure global VTP state
  wsma                        Configure Web Services Management Agents

S1(config)#exit
S1#
*Aug 21 14:05:14.471: %SYS-5-CONFIG_I: Configured from console by console
S1#en
S1#conf t
Enter configuration commands, one per line.  End with CNTL/Z.
S1(config)#exit
S1#e
*Aug 21 14:05:33.766: %SYS-5-CONFIG_I: Configured from console by consol^Z
S1#
S1#ex

































S1 con0 is now available





Press RETURN to get started.


S1>
S1>en
Password:
S1#conf t
Enter configuration commands, one per line.  End with CNTL/Z.
S1(config)#exit
S1#
*Aug 21 14:06:05.027: %SYS-5-CONFIG_I: Configured from console by console?
Exec commands:
  access-enable    Create a temporary Access-List entry
  access-profile   Apply user-profile to interface
  access-template  Create a temporary Access-List entry
  archive          manage archive files
  authentication   Authentication options for eEdge
  beep             Blocks Extensible Exchange Protocol commands
  bulkstat         Bulkstat exec commands
  calendar         Manage the hardware calendar
  call-home        Call-Home commands
  cd               Change current directory
  clear            Reset functions
  clock            Manage the system clock
  cns              CNS agents
  configure        Enter configuration mode
  connect          Open a terminal connection
  copy             Copy from one file to another
  crypto           Encryption related commands.
  debug            Debugging functions (see also 'undebug')
  delete           Delete a file
  device           device classifier
  diagnostic       Diagnostic commands
  dir              List files on a filesystem
  disable          Turn off privileged commands
  disconnect       Disconnect an existing network connection
  do-exec          Mode-independent "do-exec" prefix support
  dot1x            IEEE 802.1X Exec Commands
  eap              EAP Exec Commands
  enable           Turn on privileged commands
  erase            Erase a filesystem
  ethernet         Ethernet parameters
  exit             Exit from the EXEC
  format           Format a filesystem
  help             Description of the interactive help system
  if-mgr           IF-MGR operations
  ip               Global IP commands
  lock             Lock the terminal
  logging          Handles logging operations
  login            Log in as a particular user
  logout           Exit from the EXEC
  macro            Exec level macro commands
  mkdir            Create new directory
  monitor          Monitoring different system events
  more             Display the contents of a file
  name-connection  Name an existing network connection

S1#login cisco
         ^
% Invalid input detected at '^' marker.

S1#login ?
  <cr>

S1#?
Exec commands:
  access-enable    Create a temporary Access-List entry
  access-profile   Apply user-profile to interface
  access-template  Create a temporary Access-List entry
  archive          manage archive files
  authentication   Authentication options for eEdge
  beep             Blocks Extensible Exchange Protocol commands
  bulkstat         Bulkstat exec commands
  calendar         Manage the hardware calendar
  call-home        Call-Home commands
  cd               Change current directory
  clear            Reset functions
  clock            Manage the system clock
  cns              CNS agents
  configure        Enter configuration mode
  connect          Open a terminal connection
  copy             Copy from one file to another
  crypto           Encryption related commands.
  debug            Debugging functions (see also 'undebug')
  delete           Delete a file
  device           device classifier
  diagnostic       Diagnostic commands
  dir              List files on a filesystem
  disable          Turn off privileged commands
  disconnect       Disconnect an existing network connection
  do-exec          Mode-independent "do-exec" prefix support
  dot1x            IEEE 802.1X Exec Commands
  eap              EAP Exec Commands
  enable           Turn on privileged commands
  erase            Erase a filesystem
  ethernet         Ethernet parameters
  exit             Exit from the EXEC
  format           Format a filesystem
  help             Description of the interactive help system
  if-mgr           IF-MGR operations
  ip               Global IP commands
  lock             Lock the terminal
  logging          Handles logging operations
  login            Log in as a particular user
  logout           Exit from the EXEC
  macro            Exec level macro commands
  mkdir            Create new directory
  monitor          Monitoring different system events
  more             Display the contents of a file
  name-connection  Name an existing network connection
  no               Disable debugging functions
  ping             Send echo messages
  pnpa             PnP agent
  port-channel     lag auto persistent
  pwd              Display current working directory
  release          Release a resource
  reload           Halt and perform a cold restart
  remote           Remote procedures
  rename           Rename a file
  renew            Renew a resource
  rep              Resilient Ethernet Protocol Exec Commands
  resume           Resume an active network connection
  rmdir            Remove existing directory
  routing-context  Routing Context
  rsh              Execute a remote command
  send             Send a message to other tty lines
  session          Run command on member switch
  set              Set system parameter (not config)
  setup            Run the SETUP command facility
  show             Show running system information
  software         Software commands
  spec-file        format spec file commands
  ssh              Open a secure shell client connection
  staging          execute boot stage parameters
  switch           Switch-specific commands
  systat           Display information about terminal lines
  tclquit          Quit Tool Command Language shell
  tclsh            Tool Command Language shell
  telnet           Open a telnet connection
  terminal         Set terminal line parameters
  test             Test subsystems, memory, and interfaces
  traceroute       Trace route to destination
  tunnel           Open a tunnel connection
  udld             UDLD protocol commands
  undebug          Disable debugging functions (see also 'debug')
  upgrade          Upgrade commands
  verify           Verify a file
  vtp              Configure global VTP state
  where            List active connections
  write            Write running configuration to memory, network, or terminal

S1#setup ?
  <cr>

S1#setup


         --- System Configuration Dialog ---

Continue with configuration dialog? [yes/no]: n
S1#set?
set  setup

S1#set ?
  memory  set memory parameters
  trace   Set trace options

S1#login
Username: cisco
Password:
% Login invalid

S1#
S1#login
Username: cisco
Password:
% Login invalid

S1#en login
      ^
% Invalid input detected at '^' marker.

S1#en login?
% Unrecognized command
S1#en loginexi
      ^
% Invalid input detected at '^' marker.

S1#en?
enable

S1#en
S1#conf t
Enter configuration commands, one per line.  End with CNTL/Z.
S1(config)#?
Configure commands:
  aaa                         Authentication, Authorization and Accounting.
  access-list                 Add an access list entry
  access-session              Access Sesion Global Configuration Commands
  alias                       Create command alias
  archive                     Archive the configuration
  arp                         Set a static ARP entry
  authentication              Auth Manager Global Configuration Commands
  auto                        Configure Automation
  autoconf                    Configure autoconf
  banner                      Define a login banner
  beep                        Configure BEEP (Blocks Extensible Exchange
                              Protocol)
  boot                        Modify system boot parameters
  buffers                     Adjust system buffer pool parameters
  bulkstat                    Bulkstat Application
  call-home                   Enter call-home configuration mode
  captive-portal-bypass       Enable Captive portal bypass for apple devices
  cdp                         Global CDP configuration subcommands
  cfg-mode                    Enter configuration mode
  cisp                        Set CISP parameters
  class-map                   Configure CPL Class Map

S1(config)#en?
enable  end

S1(config)#enenable ?
% Unrecognized command
S1(config)#enab?
enable

S1(config)#enab ?
  algorithm-type  Algorithm to use for hashing the plaintext 'enable' secret
  last-resort     Define enable action if no TACACS servers respond
  masked-secret   secret input will be masked on screen and will be converted
                  to type 9 by default
  password        Assign the privileged level password (MAX of 25 characters)
  secret          Assign the privileged level secret (MAX of 25 characters)
  use-tacacs      Use TACACS to check enable passwords

S1(config)#enab secret cisco123
The enable secret you have chosen is the same as your enable password.
This is not recommended.  Re-enter the enable secret.

S1(config)#enab secret Cisco123
S1(config)#ena ?
  algorithm-type  Algorithm to use for hashing the plaintext 'enable' secret
  last-resort     Define enable action if no TACACS servers respond
  masked-secret   secret input will be masked on screen and will be converted
                  to type 9 by default
  password        Assign the privileged level password (MAX of 25 characters)
  secret          Assign the privileged level secret (MAX of 25 characters)
  use-tacacs      Use TACACS to check enable passwords

S1(config)#?
Configure commands:
  aaa                         Authentication, Authorization and Accounting.
  access-list                 Add an access list entry
  access-session              Access Sesion Global Configuration Commands
  alias                       Create command alias
  archive                     Archive the configuration
  arp                         Set a static ARP entry
  authentication              Auth Manager Global Configuration Commands
  auto                        Configure Automation
  autoconf                    Configure autoconf
  banner                      Define a login banner
  beep                        Configure BEEP (Blocks Extensible Exchange
                              Protocol)
  boot                        Modify system boot parameters
  buffers                     Adjust system buffer pool parameters
  bulkstat                    Bulkstat Application
  call-home                   Enter call-home configuration mode
  captive-portal-bypass       Enable Captive portal bypass for apple devices
  cdp                         Global CDP configuration subcommands
  cfg-mode                    Enter configuration mode
  cisp                        Set CISP parameters
  class-map                   Configure CPL Class Map
  clock                       Configure time-of-day clock
  cns                         CNS agents
  configuration               Configuration access
  crypto                      Encryption module
  default                     Set a command to its defaults
  default-value               Default character-bits values
  define                      interface range macro definition
  device                      device classifier configuration
  device-sensor               IOS Sensor Commands
  diagnostic                  Configure diagnostic information
  do-exec                     To run exec commands in config mode
  dot1x                       IEEE 802.1X Global Configuration Commands
  downward-compatible-config  Generate a configuration compatible with older
                              software
  dying-gasp                  Dying Gasp configuration commands
  eap                         EAP Global Configuration Commands
  enable                      Modify enable password parameters
  end                         Exit from configure mode
  epm                         EPM Global Configuration Commands
  errdisable                  Error disable
  ethernet                    Ethernet configuration
  exception                   Exception handling
  exit                        Exit from configure mode
  fallback                    Fallback configuration commands
  file                        Adjust file system parameters
  fips                        FIPS config
  format                      Format the output
  global-address-family       Enter address-family base routing topology mode
  help                        Description of the interactive help system
  hostname                    Set system's network name
  hw-module                   Control of individual components in the system
  id-manager                  ID Pool Manager
  identity                    Identity Configuration Commands
  interface                   Select an interface to configure
  ip                          Global IP configuration subcommands
  ipc                         Configure IPC system
  ipv6                        Global IPv6 configuration commands
  kron                        Kron interval Facility
  l2                          Layer 2
  lacp                        LACP configuration
  li-view                     LI View
  license                     license boot config commands
  line                        Configure a terminal line
  link                        Enable Link State Tracking feature
  lldp                        Global LLDP configuration subcommands
  location                    Global location configuration commands
  logging                     Modify message logging facilities
  login                       Enable secure login checking
  mab                         MAC Authentication Bypass Global Configuration
                              Commands
  mac                         Global MAC configuration subcommands
  macro                       Macro configuration
  map-class                   Configure static map class
  map-list                    Configure static map list
  memory                      Configure memory management
  mls                         mls global commands
  monitor                     Monitoring different system events
  network-policy              Network Policy
  nmsp                        NMSP configuration commands
  no                          Negate a command or set its defaults
  ntp                         Configure NTP
  parameter-map               Configure Parameter Map
  parser                      Configure parser
  passthru-domain-list        Domain name's associated with FQDN name
  pnp                         Configure PNP
  policy-map                  Configure Policy Map
  port-channel                EtherChannel configuration
  port-security               Security related command
  power                       Power configure

S1(config)#port-cha
S1(config)#port-channel ?
  auto  LACP auto for the system

S1(config)#port-channel
% Incomplete command.

S1(config)#int range g1/0/1
S1(config-if-range)#port-channel 1
                      ^
% Invalid input detected at '^' marker.

S1(config-if-range)#exit
S1(config)#port-channel 1
                        ^
% Invalid input detected at '^' marker.

S1(config)#port-channel
% Incomplete command.

S1(config)#exit
S1#
*Aug 21 14:19:34.014: %SYS-5-CONFIG_I: Configured from console by console?
Exec commands:
  access-enable    Create a temporary Access-List entry
  access-profile   Apply user-profile to interface
  access-template  Create a temporary Access-List entry
  archive          manage archive files
  authentication   Authentication options for eEdge
  beep             Blocks Extensible Exchange Protocol commands
  bulkstat         Bulkstat exec commands
  calendar         Manage the hardware calendar
  call-home        Call-Home commands
  cd               Change current directory
  clear            Reset functions
  clock            Manage the system clock
  cns              CNS agents
  configure        Enter configuration mode
  connect          Open a terminal connection
  copy             Copy from one file to another
  crypto           Encryption related commands.
  debug            Debugging functions (see also 'undebug')
  delete           Delete a file
  device           device classifier
  diagnostic       Diagnostic commands
Press RETURN for another line, SPACE for another page, anything else to quit
  dir              List files on a filesystem
  disable          Turn off privileged commands
  disconnect       Disconnect an existing network connection
  do-exec          Mode-independent "do-exec" prefix support
  dot1x            IEEE 802.1X Exec Commands
  eap              EAP Exec Commands
  enable           Turn on privileged commands
  erase            Erase a filesystem
  ethernet         Ethernet parameters
  exit             Exit from the EXEC
  format           Format a filesystem
  help             Description of the interactive help system
  if-mgr           IF-MGR operations
  ip               Global IP commands
  lock             Lock the terminal
  logging          Handles logging operations
  login            Log in as a particular user
  logout           Exit from the EXEC
  macro            Exec level macro commands
  mkdir            Create new directory
  monitor          Monitoring different system events
  more             Display the contents of a file
  name-connection  Name an existing network connection
  no               Disable debugging functions
  ping             Send echo messages
  pnpa             PnP agent
  port-channel     lag auto persistent
  pwd              Display current working directory
  release          Release a resource
  reload           Halt and perform a cold restart
  remote           Remote procedures
  rename           Rename a file
  renew            Renew a resource
  rep              Resilient Ethernet Protocol Exec Commands
  resume           Resume an active network connection
  rmdir            Remove existing directory
  routing-context  Routing Context
  rsh              Execute a remote command
  send             Send a message to other tty lines
  session          Run command on member switch
  set              Set system parameter (not config)
  setup            Run the SETUP command facility
  show             Show running system information
  software         Software commands
  spec-file        format spec file commands
  ssh              Open a secure shell client connection
  staging          execute boot stage parameters
  switch           Switch-specific commands
  systat           Display information about terminal lines
  tclquit          Quit Tool Command Language shell
  tclsh            Tool Command Language shell
  telnet           Open a telnet connection
  terminal         Set terminal line parameters
  test             Test subsystems, memory, and interfaces
  traceroute       Trace route to destination
  tunnel           Open a tunnel connection
  udld             UDLD protocol commands
  undebug          Disable debugging functions (see also 'debug')
  upgrade          Upgrade commands
  verify           Verify a file
  vtp              Configure global VTP state
  where            List active connections
  write            Write running configuration to memory, network, or terminal

S1#
R1>en
R1#en?
enable

R1#en
R1#enable ?
  <0-15>  Enable level
  view    Set into the existing view
  <cr>    <cr>

R1#enable
R1#?
Exec commands:
  access-profile   Apply user-profile to interface
  access-session   Access-session options for eEdge
  app-hosting      Application hosting
  archive          manage archive files
  attach           Connect to a module's console
  authentication   Authentication options for eEdge
  auto             Exec level Automation
  beep             Blocks Extensible Exchange Protocol commands
  bfe              For manual emergency modes setting
  bulkstat         Bulkstat exec commands
  call-home        Call-Home commands
  cd               Change current directory
  clear            Reset functions
  clock            Manage the system clock
  cns              CNS agents
  configure        Enter configuration mode
  connect          Open a terminal connection
  controller-mode  controller-mode service
  copy             Copy from one file to another
  crypto           Encryption related commands.
  cts              Cisco Trusted Security Exec Commands
  debug            Debugging functions (see also 'undebug')
  delete           Delete a file
  diagnostic       Diagnostic commands
  dir              List files on a filesystem
  disable          Turn off privileged commands
  disconnect       Disconnect an existing network connection
  dns              DNS Protocol commands
  do-exec          Mode-independent "do-exec" prefix support
  dot1x            IEEE 802.1X Exec Commands
  eap              EAP Exec Commands
  enable           Turn on privileged commands
  erase            Erase a filesystem
  ethernet         Ethernet parameters
  event            Event related commands
  exit             Exit from the EXEC
  factory-reset    Factory Reset command
  format           Format a filesystem
  fsck             Filesystem check
  guestshell       Request a guestshell
  help             Description of the interactive help system
  hw-module        Apply command to specific hardware component
  if-mgr           IF-MGR operations
  install          Install command
 --More--
S1#en
S1#crypto ?
  key  Key related commands.
  pki  Public Key components

S1#crypto key?
key

S1#crypto key ?
  lock    Lock a keypair.
  unlock  Unlock a keypair.

S1#?
Exec commands:
  access-enable    Create a temporary Access-List entry
  access-profile   Apply user-profile to interface
  access-template  Create a temporary Access-List entry
  archive          manage archive files
  authentication   Authentication options for eEdge
  beep             Blocks Extensible Exchange Protocol commands
  bulkstat         Bulkstat exec commands
  calendar         Manage the hardware calendar
  call-home        Call-Home commands
  cd               Change current directory
  clear            Reset functions
  clock            Manage the system clock
  cns              CNS agents
  configure        Enter configuration mode
  connect          Open a terminal connection
  copy             Copy from one file to another
  crypto           Encryption related commands.
  debug            Debugging functions (see also 'undebug')
  delete           Delete a file
  device           device classifier
  diagnostic       Diagnostic commands
  dir              List files on a filesystem
  disable          Turn off privileged commands
  disconnect       Disconnect an existing network connection
  do-exec          Mode-independent "do-exec" prefix support
  dot1x            IEEE 802.1X Exec Commands
  eap              EAP Exec Commands
  enable           Turn on privileged commands
  erase            Erase a filesystem
  ethernet         Ethernet parameters
  exit             Exit from the EXEC
  format           Format a filesystem
  help             Description of the interactive help system
  if-mgr           IF-MGR operations
  ip               Global IP commands
  lock             Lock the terminal
  logging          Handles logging operations
  login            Log in as a particular user
  logout           Exit from the EXEC
  macro            Exec level macro commands
  mkdir            Create new directory
  monitor          Monitoring different system events
  more             Display the contents of a file
  name-connection  Name an existing network connection
  no               Disable debugging functions
  ping             Send echo messages
  pnpa             PnP agent
  port-channel     lag auto persistent
  pwd              Display current working directory
  release          Release a resource
  reload           Halt and perform a cold restart
  remote           Remote procedures
  rename           Rename a file
  renew            Renew a resource
  rep              Resilient Ethernet Protocol Exec Commands
  resume           Resume an active network connection
  rmdir            Remove existing directory
  routing-context  Routing Context
  rsh              Execute a remote command
  send             Send a message to other tty lines
  session          Run command on member switch
  set              Set system parameter (not config)
  setup            Run the SETUP command facility
  show             Show running system information
  software         Software commands
  spec-file        format spec file commands
  ssh              Open a secure shell client connection
  staging          execute boot stage parameters
  switch           Switch-specific commands
  systat           Display information about terminal lines
  tclquit          Quit Tool Command Language shell
  tclsh            Tool Command Language shell
  telnet           Open a telnet connection
  terminal         Set terminal line parameters
  test             Test subsystems, memory, and interfaces
  traceroute       Trace route to destination
  tunnel           Open a tunnel connection
  udld             UDLD protocol commands
  undebug          Disable debugging functions (see also 'debug')
  upgrade          Upgrade commands
  verify           Verify a file
  vtp              Configure global VTP state
  where            List active connections
  write            Write running configuration to memory, network, or terminal

S1#en pass
S1#en passw
S1#conf t
Enter configuration commands, one per line.  End with CNTL/Z.
S1(config)#pass
S1(config)#paassw
S1(config)#paassword ?
% Unrecognized command
S1(config)#passw
S1(config)#passw ?
% Unrecognized command
S  ip               IP SLA Exec Command
  isdn             Run an ISDN EXEC command on an ISDN interface
  issu             issu commands
  license          Smart licensing Commands
  lock             Lock the terminal
  logging          Handles logging operations
  login            Log in as a particular user
  logout           Exit from the EXEC
  maintenance      Maintenance mode
  microcode        microcode commands
  mkdir            Create new directory
  mlacp            mLACP EXEC commands
  monitor          Monitoring different system events
  more             Display the contents of a file
  mrinfo           Request neighbor and version information from a multicast
                   router
  mrm              IP Multicast Routing Monitor Test
  mstat            Show statistics after multiple multicast traceroutes
  mtrace           Trace reverse multicast path from destination to source
  name-connection  Name an existing network connection
  nat64            NAT64 commands
  network-clock    Network clock
  no               Disable debugging functions
  partition        Partition a filesystem
  ping             Send echo messages
  pnpa             PnP agent
  port-channel     lag auto persistent
  ppp              Start IETF Point-to-Point Protocol (PPP)
  pwd              Display current working directory
  redundancy       Redundancy Facility (RF) exec commands
  release          Release a resource
  reload           Halt and perform a cold restart
  rename           Rename a file
  renew            Renew a resource
  request          Request an action
  restart          Restart Connection/Interface
  resume           Resume an active network connection
  rlogin           Open an rlogin connection
  rmdir            Remove existing directory
  routing-context  Routing Context
  rsh              Execute a remote command
  send             Send a message to other tty lines
  service          IOS integrated service enablement
  set              Set system parameter (not config)
  setup            Run the SETUP command facility
  sga-internal     Cisco Trusted Security Exec Commands
  show             Show running system information
  slip             Start Serial-line IP (SLIP)
  snmp             snmp commands
  spec-file        format spec file commands
  ssh              Open a secure shell client connection
  sslproxy         SSLPROXY Exec Commands
  start-chat       Start a chat-script on a line
  systat           Display information about terminal lines
  tclquit          Quit Tool Command Language shell
  tclsh            Tool Command Language shell
  telnet           Open a telnet connection
  terminal         Set terminal line parameters
  test             Test subsystems, memory, and interfaces
  traceroute       Trace route to destination
  tunnel           Open a tunnel connection
  ucse             UCSE server
  udld             UDLD protocol commands
  undebug          Disable debugging functions (see also 'debug')
  upgrade          Upgrade commands
  verify           Verify a file
  virtual-service  Virtual service and infrastructure related commands
  vtp              Configure global VTP state
  where            List active connections
  which-route      Do OSI route table lookup and display results
  who              who
  write            Write running configuration to memory, network, or terminal
  xprofile         Profile operations

R1#ena secret cisco123
       ^
% Invalid input detected at '^' marker.

R1#enable
R1#enable
R1#enable ?
  <0-15>  Enable level
  view    Set into the existing view
  <cr>    <cr>

R1#enable
R1#conf t
Enter configuration commands, one per line.  End with CNTL/Z.
R1(config)#enable username cisco
                     ^
% Invalid input detected at '^' marker.

R1(config)#enable secret cisco123
R1(config)#enable ?
  algorithm-type  Algorithm to use for hashing the plaintext 'enable' secret
  last-resort     Define enable action if no TACACS servers respond
  masked-secret   secret input will be masked on screen and will be converted
                  to type 9 by default
  password        Assign the privileged level password (MAX of 25 characters)
  secret          Assign the privileged level secret (MAX of 25 characters)
  use-tacacs      Use TACACS to check enable passwords

R1(config)#encryp
R1(config)#encryp
             ^
% Invalid input detected at '^' marker.

R1(config)#cry?
crypto

R1(config)#cry ?
  RSA-key-pair  RSA key pair
  key           Long term key operations
  pki           Public Key components
  provisioning  Secure Device Provisioning
  wui           Crypto HTTP configuration interfaces

R1(config)#cry rsa
R1(config)#cry rsa-key-pair
% Incomplete command.

R1(config)#cry rsa-key-pair
R1(config)#cry rsa-key-pair ?
  WORD  Key pair name

R1(config)#cry rsa-key-pair cisco123
% Incomplete command.

R1(config)#cry rsa-key-pair word
% Incomplete command.

R1(config)#cry rsa-key-pair w
R1(config)#cry rsa-key-pair
R1(config)#cry rsa-key-pair 1024
% Incomplete command.

R1(config)#exit
R1#
*Aug 21 14:33:39.637: %SYS-5-CONFIG_I: Configured from console by console
R1#sh run
Building configuration...

Current configuration : 6026 bytes
!
! Last configuration change at 14:33:39 UTC Wed Aug 21 2024
!
version 17.9
service timestamps debug datetime msec
service timestamps log datetime msec
! Call-home is enabled by Smart-Licensing.
service call-home
platform qfp utilization monitor load 80
platform punt-keepalive disable-kernel-core
!
hostname R1
!
boot-start-marker
boot-end-marker
!
!
no aaa new-model
!
!
!
!
!
!
!
!
!
!
login on-success log
!
!
!
!
!
!
!
subscriber templating
vtp version 1
multilink bundle-name authenticated
!
!
!
crypto pki trustpoint TP-self-signed-3644520442
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-3644520442
 revocation-check none
 rsakeypair TP-self-signed-3644520442
!
crypto pki trustpoint SLA-TrustPoint
 enrollment pkcs12
 revocation-check crl
!
!
crypto pki certificate chain TP-self-signed-3644520442
 certificate self-signed 01
  30820330 30820218 A0030201 02020101 300D0609 2A864886 F70D0101 05050030
  31312F30 2D060355 04031326 494F532D 53656C66 2D536967 6E65642D 43657274
  69666963 6174652D 33363434 35323034 3432301E 170D3234 30383231 31333132
  34325A17 0D333430 38323131 33313234 325A3031 312F302D 06035504 03132649
  4F532D53 656C662D 5369676E 65642D43 65727469 66696361 74652D33 36343435
  32303434 32308201 22300D06 092A8648 86F70D01 01010500 0382010F 00308201
  0A028201 0100B415 107F4B8C 24EEF361 9BFF6614 218941CB 1FCAB32D E2FC61D5
  0E4DE56E 4333734C 8A68667F 5D84E8D8 8A185398 67DAAAEB DBDC4C5C 6DC558B8
  E21E7207 7ABCC810 440DDDAC 1EA6D096 841963C5 38B7D795 44E8022C DC7690BE
  D342BBC0 631B3AEB 77A63D8B 80DBB371 643D5805 93C1C4DB 58ADB1E8 4535C928
  B258ACE3 D949CF60 03F910A8 DD46F2D3 E4582563 2A42F71E 8D9047B1 1FDBA593
  F2A86847 5694D592 D1B17C43 FAF4D13B 3789AD15 446201CE BCCC5DEE D0ED1679
  DC327BFC CD2AD1E4 13D7362A 705CD8EC B837ABD0 52772AD4 54F583AA 06F84CA2
  1173378F 4BCFE024 EF1934EA 269AE405 EEE902D4 F55EC0BE 38BF9C5D 4A2F7D79
  887683AF 9A0B0203 010001A3 53305130 0F060355 1D130101 FF040530 030101FF
  301F0603 551D2304 18301680 14F90B1A 9BC90E21 855CC38C C07A334F 1B65435C
  DC301D06 03551D0E 04160414 F90B1A9B C90E2185 5CC38CC0 7A334F1B 65435CDC
  300D0609 2A864886 F70D0101 05050003 82010100 5669C128 525C407E C40B0473
  A79A3501 1D07B099 8B765B42 BE6B45BD D97B4E91 0BE73E61 7C7B70C2 B2D7B77A
  7483BD0D 97CBD359 2D3ED74A 143B3141 371ACA3C AF6FB949 8B4275E6 E1686089
  534A7A3E 0AC6EBC2 94BB4ED7 24FBC74D D0214116 F1274A0D F8FF2B7B 4FCBE079
  B6A39F44 C8EF1B08 BDE723AE 27DE5B49 286A8218 776D61FB 358069D6 E6BEB248
  B7597833 0935FF9D 31368BE8 1D49B5D7 DDD08F39 8FDB6DD5 30BF074F 79E02E41
  2605E197 50BDE09D E31224CF 0F6AEF7D 06AB814F 36859896 50D55B2F 7F1E62CA
  25BF8FEA 017D071F 5EA6550B 81D5F26A 9628F29B 98B76A9B B6D74602 30AC3330
  E8A5D8B2 64A44CA9 B8C450EB 5B876B42 954DE9E8
        quit
crypto pki certificate chain SLA-TrustPoint
 certificate ca 01
  30820321 30820209 A0030201 02020101 300D0609 2A864886 F70D0101 0B050030
  32310E30 0C060355 040A1305 43697363 6F312030 1E060355 04031317 43697363
  6F204C69 63656E73 696E6720 526F6F74 20434130 1E170D31 33303533 30313934
  3834375A 170D3338 30353330 31393438 34375A30 32310E30 0C060355 040A1305
  43697363 6F312030 1E060355 04031317 43697363 6F204C69 63656E73 696E6720
  526F6F74 20434130 82012230 0D06092A 864886F7 0D010101 05000382 010F0030
  82010A02 82010100 A6BCBD96 131E05F7 145EA72C 2CD686E6 17222EA1 F1EFF64D
  CBB4C798 212AA147 C655D8D7 9471380D 8711441E 1AAF071A 9CAE6388 8A38E520
  1C394D78 462EF239 C659F715 B98C0A59 5BBB5CBD 0CFEBEA3 700A8BF7 D8F256EE
  4AA4E80D DB6FD1C9 60B1FD18 FFC69C96 6FA68957 A2617DE7 104FDC5F EA2956AC
  7390A3EB 2B5436AD C847A2C5 DAB553EB 69A9A535 58E9F3E3 C0BD23CF 58BD7188
  68E69491 20F320E7 948E71D7 AE3BCC84 F10684C7 4BC8E00F 539BA42B 42C68BB7
  C7479096 B4CB2D62 EA2F505D C7B062A4 6811D95B E8250FC4 5D5D5FB8 8F27D191
  C55F0D76 61F9A4CD 3D992327 A8BB03BD 4E6D7069 7CBADF8B DF5F4368 95135E44
  DFC7C6CF 04DD7FD1 02030100 01A34230 40300E06 03551D0F 0101FF04 04030201
  06300F06 03551D13 0101FF04 05300301 01FF301D 0603551D 0E041604 1449DC85
  4B3D31E5 1B3E6A17 606AF333 3D3B4C73 E8300D06 092A8648 86F70D01 010B0500
  03820101 00507F24 D3932A66 86025D9F E838AE5C 6D4DF6B0 49631C78 240DA905
  604EDCDE FF4FED2B 77FC460E CD636FDB DD44681E 3A5673AB 9093D3B1 6C9E3D8B
  D98987BF E40CBD9E 1AECA0C2 2189BB5C 8FA85686 CD98B646 5575B146 8DFC66A8
  467A3DF4 4D565700 6ADF0F0D CF835015 3C04FF7C 21E878AC 11BA9CD2 55A9232C
  7CA7B7E6 C1AF74F6 152E99B7 B1FCF9BB E973DE7F 5BDDEB86 C71E3B49 1765308B
  5FB0DA06 B92AFE7F 494E8A9E 07B85737 F3A58BE1 1A48A229 C37C1E69 39F08678
  80DDCD16 D6BACECA EEBC7CF9 8428787B 35202CDC 60E4616A B623CDBD 230E3AFB
  418616A9 4093E049 4D10AB75 27E86F73 932E35B5 8862FDAE 0275156F 719BB2F0
  D697DF7F 28
        quit
!
!
license udi pid C8200L-1N-4T sn FCZ2818R0Q9
memory free low-watermark processor 62972
!
diagnostic bootup level minimal
!
spanning-tree extend system-id
!
enable secret 9 $9$CWJH3yMtBsmSJ.$JuNmvudjJXaO9hRtQ4w7HbK78uKxj73L0vB0K8.haKE
!
!
redundancy
 mode none
!
!
!
!
!
!
!
!
interface GigabitEthernet0/0/0
 no ip address
 shutdown
 negotiation auto
!
interface GigabitEthernet0/0/1
 no ip address
 shutdown
 negotiation auto
!
interface GigabitEthernet0/0/2
 no ip address
 shutdown
 negotiation auto
!
interface GigabitEthernet0/0/3
 no ip address
 shutdown
 negotiation auto
!
interface Serial0/1/0
 no ip address
 shutdown
!
interface Serial0/1/1
 no ip address
 shutdown
!
ip http server
ip http authentication local
ip http secure-server
ip forward-protocol nd
!
!
!
!
!
!
control-plane
!
!
line con 0
 stopbits 1
line aux 0
line vty 0 4
 login
 transport input ssh
line vty 5 14
 login
 transport input ssh
!
call-home
 ! If contact email address in call-home is configured as sch-smart-licensing@cisco.com
 ! the email address configured in Cisco Smart License Portal will be used as contact email address to send SCH notifications.
 contact-email-addr sch-smart-licensing@cisco.com
 profile "CiscoTAC-1"
  active
  destination transport-method http
!
!
!
!
!
!
end

R1#sh ip int br
Interface              IP-Address      OK? Method Status                Protocol
GigabitEthernet0/0/0   unassigned      YES unset  administratively down down
GigabitEthernet0/0/1   unassigned      YES unset  administratively down down
GigabitEthernet0/0/2   unassigned      YES unset  administratively down down
GigabitEthernet0/0/3   unassigned      YES unset  administratively down down
Serial0/1/0            unassigned      YES unset  administratively down down
Serial0/1/1            unassigned      YES unset  administratively down down
R1#
S1(config)#ex
% Ambiguous command:  "ex"
S1(config)#exi
S1#
*Aug 21 14:36:45.861: %SYS-5-CONFIG_I: Configured from console by consolesh ru
Building configuration...

Current configuration : 1636 bytes
!
! Last configuration change at 14:36:45 UTC Wed Aug 21 2024
!
version 15.2
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname S1
!
boot-start-marker
boot-end-marker
!
enable secret 9 $9$GGtOPUBP6GxM.Z$d2Txn6pb8B5Kzac9Ls96ON34ms6aP1DgA.AuGc72RoY
enable password cisco123
!
username cisco
no aaa new-model
switch 1 provision c1000-24t-4g-l
system mtu routing 1500
!
!
!
!
!
!
!
!
!
!
spanning-tree mode rapid-pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
!
!
!
interface GigabitEthernet1/0/1
!
interface GigabitEthernet1/0/2
!
interface GigabitEthernet1/0/3
!
interface GigabitEthernet1/0/4
!
interface GigabitEthernet1/0/5
!
interface GigabitEthernet1/0/6
!
interface GigabitEthernet1/0/7
!
interface GigabitEthernet1/0/8
!
interface GigabitEthernet1/0/9
!
interface GigabitEthernet1/0/10
!
interface GigabitEthernet1/0/11
!
interface GigabitEthernet1/0/12
!
interface GigabitEthernet1/0/13
!
interface GigabitEthernet1/0/14
!
interface GigabitEthernet1/0/15
!
interface GigabitEthernet1/0/16
!
interface GigabitEthernet1/0/17
!
interface GigabitEthernet1/0/18
!
interface GigabitEthernet1/0/19
!
interface GigabitEthernet1/0/20
!
interface GigabitEthernet1/0/21
!
interface GigabitEthernet1/0/22
!
interface GigabitEthernet1/0/23
!
interface GigabitEthernet1/0/24
!
interface GigabitEthernet1/0/25
!
interface GigabitEthernet1/0/26
!
interface GigabitEthernet1/0/27
!
interface GigabitEthernet1/0/28
!
interface Vlan1
 no ip address
!
ip http server
ip http secure-server
!
!
!
!
line con 0
line vty 5 15
!
end

S1#sh ip int b
Interface              IP-Address      OK? Method Status                Protocol
Vlan1                  unassigned      YES unset  up                    up
GigabitEthernet1/0/1   unassigned      YES unset  up                    up
GigabitEthernet1/0/2   unassigned      YES unset  up                    up
GigabitEthernet1/0/3   unassigned      YES unset  down                  down
GigabitEthernet1/0/4   unassigned      YES unset  down                  down
GigabitEthernet1/0/5   unassigned      YES unset  down                  down
GigabitEthernet1/0/6   unassigned      YES unset  up                    up
GigabitEthernet1/0/7   unassigned      YES unset  down                  down
GigabitEthernet1/0/8   unassigned      YES unset  down                  down
GigabitEthernet1/0/9   unassigned      YES unset  down                  down
GigabitEthernet1/0/10  unassigned      YES unset  down                  down
GigabitEthernet1/0/11  unassigned      YES unset  down                  down
GigabitEthernet1/0/12  unassigned      YES unset  down                  down
GigabitEthernet1/0/13  unassigned      YES unset  down                  down
GigabitEthernet1/0/14  unassigned      YES unset  down                  down
GigabitEthernet1/0/15  unassigned      YES unset  down                  down
GigabitEthernet1/0/16  unassigned      YES unset  down                  down
GigabitEthernet1/0/17  unassigned      YES unset  down                  down
GigabitEthernet1/0/18  unassigned      YES unset  down                  down
GigabitEthernet1/0/19  unassigned      YES unset  down                  down
GigabitEthernet1/0/20  unassigned      YES unset  down                  down
GigabitEthernet1/0/21  unassigned      YES unset  down                  down
GigabitEthernet1/0/22  unassigned      YES unset  down                  down
GigabitEthernet1/0/23  unassigned      YES unset  down                  down
GigabitEthernet1/0/24  unassigned      YES unset  down                  down
GigabitEthernet1/0/25  unassigned      YES unset  down                  down
GigabitEthernet1/0/26  unassigned      YES unset  down                  down
GigabitEthernet1/0/27  unassigned      YES unset  down                  down
GigabitEthernet1/0/28  unassigned      YES unset  down                  down
S1#sh vl
S1#sh vlan b

VLAN Name                             Status    Ports
---- -------------------------------- --------- -------------------------------
1    default                          active    Gi1/0/1, Gi1/0/2, Gi1/0/3
                                                Gi1/0/4, Gi1/0/5, Gi1/0/6
                                                Gi1/0/7, Gi1/0/8, Gi1/0/9
                                                Gi1/0/10, Gi1/0/11, Gi1/0/12
                                                Gi1/0/13, Gi1/0/14, Gi1/0/15
                                                Gi1/0/16, Gi1/0/17, Gi1/0/18
                                                Gi1/0/19, Gi1/0/20, Gi1/0/21
                                                Gi1/0/22, Gi1/0/23, Gi1/0/24
                                                Gi1/0/25, Gi1/0/26, Gi1/0/27
                                                Gi1/0/28
10   Operations                       active
20   CarPark                          active
99   Management                       active
1000 Native                           active
1002 fddi-default                     act/unsup
1003 token-ring-default               act/unsup
1004 fddinet-default                  act/unsup
1005 trnet-default                    act/unsup
S1#
S2>en
S2#conf t
Enter configuration commands, one per line.  End with CNTL/Z.
S2(config)#ena secr cisco123
S2(config)#exit
S2#
*Aug 21 14:39:00.704: %SYS-5-CONFIG_I: Configured from console by consolesh run
Building configuration...

Current configuration : 1606 bytes
!
! Last configuration change at 14:39:00 UTC Wed Aug 21 2024
!
version 15.2
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname S2
!
boot-start-marker
boot-end-marker
!
enable secret 9 $9$sG86uTEHQ0oYTJ$9f0QXJpLvb.B4SQok/034o0EFHgZ1YbDaiffeiKtCBo
!
no aaa new-model
switch 1 provision c1000-24t-4g-l
system mtu routing 1500
!
!
!
!
!
!
!
!
!
!
spanning-tree mode rapid-pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
!
!
!
interface GigabitEthernet1/0/1
!
interface GigabitEthernet1/0/2
!
interface GigabitEthernet1/0/3
!
interface GigabitEthernet1/0/4
!
interface GigabitEthernet1/0/5
!
interface GigabitEthernet1/0/6
!
interface GigabitEthernet1/0/7
!
interface GigabitEthernet1/0/8
!
interface GigabitEthernet1/0/9
!
interface GigabitEthernet1/0/10
!
interface GigabitEthernet1/0/11
!
interface GigabitEthernet1/0/12
!
interface GigabitEthernet1/0/13
!
interface GigabitEthernet1/0/14
!
interface GigabitEthernet1/0/15
!
interface GigabitEthernet1/0/16
!
interface GigabitEthernet1/0/17
!
interface GigabitEthernet1/0/18
!
interface GigabitEthernet1/0/19
!
interface GigabitEthernet1/0/20
!
interface GigabitEthernet1/0/21
!
interface GigabitEthernet1/0/22
!
interface GigabitEthernet1/0/23
!
interface GigabitEthernet1/0/24
!
interface GigabitEthernet1/0/25
!
interface GigabitEthernet1/0/26
!
interface GigabitEthernet1/0/27
!
interface GigabitEthernet1/0/28
!
interface Vlan1
 no ip address
 shutdown
!
ip http server
ip http secure-server
!
!
!
!
line con 0
line vty 5 15
!
end

S2#sh ip int br
Interface              IP-Address      OK? Method Status                Protocol
Vlan1                  unassigned      YES unset  administratively down down
GigabitEthernet1/0/1   unassigned      YES unset  up                    up
GigabitEthernet1/0/2   unassigned      YES unset  up                    up
GigabitEthernet1/0/3   unassigned      YES unset  down                  down
GigabitEthernet1/0/4   unassigned      YES unset  down                  down
GigabitEthernet1/0/5   unassigned      YES unset  down                  down
GigabitEthernet1/0/6   unassigned      YES unset  down                  down
GigabitEthernet1/0/7   unassigned      YES unset  down                  down
GigabitEthernet1/0/8   unassigned      YES unset  down                  down
GigabitEthernet1/0/9   unassigned      YES unset  down                  down
GigabitEthernet1/0/10  unassigned      YES unset  down                  down
GigabitEthernet1/0/11  unassigned      YES unset  down                  down
GigabitEthernet1/0/12  unassigned      YES unset  down                  down
GigabitEthernet1/0/13  unassigned      YES unset  down                  down
GigabitEthernet1/0/14  unassigned      YES unset  down                  down
GigabitEthernet1/0/15  unassigned      YES unset  down                  down
GigabitEthernet1/0/16  unassigned      YES unset  down                  down
GigabitEthernet1/0/17  unassigned      YES unset  down                  down
GigabitEthernet1/0/18  unassigned      YES unset  up                    up
GigabitEthernet1/0/19  unassigned      YES unset  down                  down
GigabitEthernet1/0/20  unassigned      YES unset  down                  down
GigabitEthernet1/0/21  unassigned      YES unset  down                  down
GigabitEthernet1/0/22  unassigned      YES unset  down                  down
GigabitEthernet1/0/23  unassigned      YES unset  down                  down
GigabitEthernet1/0/24  unassigned      YES unset  down                  down
GigabitEthernet1/0/25  unassigned      YES unset  down                  down
GigabitEthernet1/0/26  unassigned      YES unset  down                  down
GigabitEthernet1/0/27  unassigned      YES unset  down                  down
GigabitEthernet1/0/28  unassigned      YES unset  down                  down
S2#sh vl
S2#sh vlan b

VLAN Name                             Status    Ports
---- -------------------------------- --------- -------------------------------
1    default                          active    Gi1/0/1, Gi1/0/2, Gi1/0/3
                                                Gi1/0/4, Gi1/0/5, Gi1/0/6
                                                Gi1/0/7, Gi1/0/8, Gi1/0/9
                                                Gi1/0/10, Gi1/0/11, Gi1/0/12
                                                Gi1/0/13, Gi1/0/14, Gi1/0/15
                                                Gi1/0/16, Gi1/0/17, Gi1/0/18
                                                Gi1/0/19, Gi1/0/20, Gi1/0/21
                                                Gi1/0/22, Gi1/0/23, Gi1/0/24
                                                Gi1/0/25, Gi1/0/26, Gi1/0/27
                                                Gi1/0/28
7    London                           active
9    S1                               active
1002 fddi-default                     act/unsup
1003 token-ring-default               act/unsup
1004 fddinet-default                  act/unsup
1005 trnet-default                    act/unsup
S2#vlan datab
    ^
% Invalid input detected at '^' marker.

S2#conf t
Enter configuration commands, one per line.  End with CNTL/Z.
S2(config)#vlan da
S2(config)#vlan da?
WORD

S2(config)#vlan da ?
  <cr>

S2(config)#vlan data
Command rejected: Bad VLAN list - character #1 is a non-numeric
character ('d').
S2(config)#no vlan 7
S2(config)#no vlan 9
S2(config)#no vlan 1
%Default VLAN 1 may not be deleted.
S2(config)#no vlan range 1002-1005
                         ^
% Invalid input detected at '^' marker.

S2(config)#no vlan 1002-1005
%Default VLAN 1002 may not be deleted.
%Default VLAN 1003 may not be deleted.
%Default VLAN 1004 may not be deleted.
%Default VLAN 1005 may not be deleted.
S2(config)#vlan 22
S2(config-vlan)#name student
S2(config-vlan)#
S2(config-vlan)#vlan 23
S2(config-vlan)#name teacher
S2(config-vlan)#vlan 24
S2(config-vlan)#name management
S2(config-vlan)#vlan 25
S2(config-vlan)#name library
S2(config-vlan)#vlan 26
S2(config-vlan)#name native
S2(config-vlan)#vlan 24
S2(config-vlan)#ip add 192.168.110.3
                ^
% Invalid input detected at '^' marker.

S2(config-vlan)#?
VLAN configuration commands:
  are           Maximum number of All Route Explorer hops for this VLAN (or
                zero if none specified)
  backupcrf     Backup CRF mode of the VLAN
  bridge        Bridging characteristics of the VLAN
  exit          Apply changes, bump revision number, and exit mode
  media         Media type of the VLAN
  mtu           VLAN Maximum Transmission Unit
  name          Ascii name of the VLAN
  no            Negate a command or set its defaults
  parent        ID number of the Parent VLAN of FDDI or Token Ring type VLANs
  private-vlan  Configure a private VLAN
  ring          Ring number of FDDI or Token Ring type VLANs
  said          IEEE 802.10 SAID
  shutdown      Shutdown VLAN switching
  state         Operational state of the VLAN
  ste           Maximum number of Spanning Tree Explorer hops for this VLAN (or
                zero if none specified)
  stp           Spanning tree characteristics of the VLAN
  tb-vlan1      ID number of the first translational VLAN for this VLAN (or
                zero if none)
  tb-vlan2      ID number of the second translational VLAN for this VLAN (or
                zero if none)

S2(config-vlan)#ex
S2(config)#int vlan 22-26 no sh
                      ^
% Invalid input detected at '^' marker.

S2(config)##
*Aug 21 14:53:15.077: %LINEPROTO-5-UPDOWN: Line protocol on Interface Vlan22, changed state to dowint vlan 22-26 no sh
*Aug 21 14:53:17.076: %LINK-5-CHANGED: Interface Vlan22, changed state to aint vlan 22-26 no sh
                      ^
% Invalid input detected at '^' marker.

S2(config)#sh vl brie
              ^
% Invalid input detected at '^' marker.

S2(config)#sh vl brie
S2(config)#sh vl brie
S2(config)#sh vlan brie
              ^
% Invalid input detected at '^' marker.

S2(config)#exit
S2#
*Aug 21 14:54:07.934: %SYS-5-CONFIG_I: Configured from console by consolevlan datab
    ^
% Invalid input detected at '^' marker.

S2#sh vlan b

VLAN Name                             Status    Ports
---- -------------------------------- --------- -------------------------------
1    default                          active    Gi1/0/1, Gi1/0/2, Gi1/0/3
                                                Gi1/0/4, Gi1/0/5, Gi1/0/6
                                                Gi1/0/7, Gi1/0/8, Gi1/0/9
                                                Gi1/0/10, Gi1/0/11, Gi1/0/12
                                                Gi1/0/13, Gi1/0/14, Gi1/0/15
                                                Gi1/0/16, Gi1/0/17, Gi1/0/18
                                                Gi1/0/19, Gi1/0/20, Gi1/0/21
                                                Gi1/0/22, Gi1/0/23, Gi1/0/24
                                                Gi1/0/25, Gi1/0/26, Gi1/0/27
                                                Gi1/0/28
22   student                          active
23   teacher                          active
24   management                       active
25   library                          active
26   native                           active
1002 fddi-default                     act/unsup
1003 token-ring-default               act/unsup
1004 fddinet-default                  act/unsup
1005 trnet-default                    act/unsup
S2#conf t
Enter configuration commands, one per line.  End with CNTL/Z.
S2(config)#int g1/0/18
S2(config-if)#switchport acc
S2(config-if)#switchport access trun
S2(config-if)#switchport access trunk
                                ^
% Invalid input detected at '^' marker.

S2(config-if)#switchport mode trunk
S2(config-if)#
*Aug 21 14:55:54.873: %LINEPROTO-5-UPDOWN: Line protocol on Interface GigabitEthernet1/0/18, changed state to downswitchport mode trunk
*Aug 21 14:55:57.939: %LINEPROTO-5-UPDOWN: Line protocol on Interface GigabitEthernet1/0/18                S2(config-if)#switchport mode trunk
S2(config-if)#switchport trunk access vlan 23
                                ^
% Invalid input detected at '^' marker.

S2(config-if)#switchport trunk ?
  allowed  Set allowed VLAN characteristics when interface is in trunking mode
  native   Set trunking native characteristics when interface is in trunking
           mode
  pruning  Set pruning VLAN characteristics when interface is in trunking mode

S2(config-if)#switchport trunk allowed ?
  vlan  Set allowed VLANs when interface is in trunking mode

S2(config-if)#switchport trunk allowed vlan 23
S2(config-if)#vlan 26
S2(config-vlan)#?
VLAN configuration commands:
  are           Maximum number of All Route Explorer hops for this VLAN (or
                zero if none specified)
  backupcrf     Backup CRF mode of the VLAN
  bridge        Bridging characteristics of the VLAN
  exit          Apply changes, bump revision number, and exit mode
  media         Media type of the VLAN
  mtu           VLAN Maximum Transmission Unit
  name          Ascii name of the VLAN
  no            Negate a command or set its defaults
  parent        ID number of the Parent VLAN of FDDI or Token Ring type VLANs
  private-vlan  Configure a private VLAN
  ring          Ring number of FDDI or Token Ring type VLANs
  said          IEEE 802.10 SAID
  shutdown      Shutdown VLAN switching
  state         Operational state of the VLAN
  ste           Maximum number of Spanning Tree Explorer hops for this VLAN (or
                zero if none specified)
  stp           Spanning tree characteristics of the VLAN
  tb-vlan1      ID number of the first translational VLAN for this VLAN (or
                zero if none)
  tb-vlan2      ID number of the second translational VLAN for this VLAN (or
                zero if none)

S2(config-vlan)#end
S2#
*Aug 21 14:58:58.830: %SYS-5-CONFIG_I: Configured from console by console
S2#sh vlan bri

VLAN Name                             Status    Ports
---- -------------------------------- --------- -------------------------------
1    default                          active    Gi1/0/1, Gi1/0/2, Gi1/0/3
                                                Gi1/0/4, Gi1/0/5, Gi1/0/6
                                                Gi1/0/7, Gi1/0/8, Gi1/0/9
                                                Gi1/0/10, Gi1/0/11, Gi1/0/12
                                                Gi1/0/13, Gi1/0/14, Gi1/0/15
                                                Gi1/0/16, Gi1/0/17, Gi1/0/19
                                                Gi1/0/20, Gi1/0/21, Gi1/0/22
                                                Gi1/0/23, Gi1/0/24, Gi1/0/25
                                                Gi1/0/26, Gi1/0/27, Gi1/0/28
22   student                          active
23   teacher                          active
24   management                       active
25   library                          active
26   native                           active
1002 fddi-default                     act/unsup
1003 token-ring-default               act/unsup
1004 fddinet-default                  act/unsup
1005 trnet-default                    act/unsup
S2#sh ip int bri
Interface              IP-Address      OK? Method Status                Protocol
Vlan1                  unassigned      YES unset  administratively down down
GigabitEthernet1/0/1   unassigned      YES unset  up                    up
GigabitEthernet1/0/2   unassigned      YES unset  up                    up
GigabitEthernet1/0/3   unassigned      YES unset  down                  down
GigabitEthernet1/0/4   unassigned      YES unset  down                  down
GigabitEthernet1/0/5   unassigned      YES unset  down                  down
GigabitEthernet1/0/6   unassigned      YES unset  down                  down
GigabitEthernet1/0/7   unassigned      YES unset  down                  down
GigabitEthernet1/0/8   unassigned      YES unset  down                  down
GigabitEthernet1/0/9   unassigned      YES unset  down                  down
GigabitEthernet1/0/10  unassigned      YES unset  down                  down
GigabitEthernet1/0/11  unassigned      YES unset  down                  down
GigabitEthernet1/0/12  unassigned      YES unset  down                  down
GigabitEthernet1/0/13  unassigned      YES unset  down                  down
GigabitEthernet1/0/14  unassigned      YES unset  down                  down
GigabitEthernet1/0/15  unassigned      YES unset  down                  down
GigabitEthernet1/0/16  unassigned      YES unset  down                  down
GigabitEthernet1/0/17  unassigned      YES unset  down                  down
GigabitEthernet1/0/18  unassigned      YES unset  up                    up
GigabitEthernet1/0/19  unassigned      YES unset  down                  down
GigabitEthernet1/0/20  unassigned      YES unset  down                  down
GigabitEthernet1/0/21  unassigned      YES unset  down                  down
GigabitEthernet1/0/22  unassigned      YES unset  down                  down
GigabitEthernet1/0/23  unassigned      YES unset  down                  down
GigabitEthernet1/0/24  unassigned      YES unset  down                  down
GigabitEthernet1/0/25  unassigned      YES unset  down                  down
GigabitEthernet1/0/26  unassigned      YES unset  down                  down
GigabitEthernet1/0/27  unassigned      YES unset  down                  down
GigabitEthernet1/0/28  unassigned      YES unset  down                  down
S2#sh run
Building configuration...

Current configuration : 1663 bytes
!
! Last configuration change at 14:58:58 UTC Wed Aug 21 2024
!
version 15.2
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname S2
!
boot-start-marker
boot-end-marker
!
enable secret 9 $9$sG86uTEHQ0oYTJ$9f0QXJpLvb.B4SQok/034o0EFHgZ1YbDaiffeiKtCBo
!
no aaa new-model
switch 1 provision c1000-24t-4g-l
system mtu routing 1500
!
!
!
!
!
!
!
!
!
!
spanning-tree mode rapid-pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
!
!
!
interface GigabitEthernet1/0/1
!
interface GigabitEthernet1/0/2
!
interface GigabitEthernet1/0/3
!
interface GigabitEthernet1/0/4
!
interface GigabitEthernet1/0/5
!
interface GigabitEthernet1/0/6
!
interface GigabitEthernet1/0/7
!
interface GigabitEthernet1/0/8
!
interface GigabitEthernet1/0/9
!
interface GigabitEthernet1/0/10
!
interface GigabitEthernet1/0/11
!
interface GigabitEthernet1/0/12
!
interface GigabitEthernet1/0/13
!
interface GigabitEthernet1/0/14
!
interface GigabitEthernet1/0/15
!
interface GigabitEthernet1/0/16
!
interface GigabitEthernet1/0/17
!
interface GigabitEthernet1/0/18
 switchport trunk allowed vlan 23
 switchport mode trunk
!
interface GigabitEthernet1/0/19
!
interface GigabitEthernet1/0/20
!
interface GigabitEthernet1/0/21
!
interface GigabitEthernet1/0/22
!
interface GigabitEthernet1/0/23
!
interface GigabitEthernet1/0/24
!
interface GigabitEthernet1/0/25
!
interface GigabitEthernet1/0/26
!
interface GigabitEthernet1/0/27
!
interface GigabitEthernet1/0/28
!
interface Vlan1
 no ip address
 shutdown
!
ip http server
ip http secure-server
!
!
!
!
line con 0
line vty 5 15
!
end

S2#
S1>
S1>
S1>
S1>sh vlan b

VLAN Name                             Status    Ports
---- -------------------------------- --------- -------------------------------
1    default                          active    Gi1/0/1, Gi1/0/2, Gi1/0/3
                                                Gi1/0/4, Gi1/0/5, Gi1/0/6
                                                Gi1/0/7, Gi1/0/8, Gi1/0/9
                                                Gi1/0/10, Gi1/0/11, Gi1/0/12
                                                Gi1/0/13, Gi1/0/14, Gi1/0/15
                                                Gi1/0/16, Gi1/0/17, Gi1/0/18
                                                Gi1/0/19, Gi1/0/20, Gi1/0/21
                                                Gi1/0/22, Gi1/0/23, Gi1/0/24
                                                Gi1/0/25, Gi1/0/26, Gi1/0/27
                                                Gi1/0/28
10   Operations                       active
20   CarPark                          active
99   Management                       active
1000 Native                           active
1002 fddi-default                     act/unsup
1003 token-ring-default               act/unsup
1004 fddinet-default                  act/unsup
1005 trnet-default                    act/unsup
S1>conf t
      ^
% Invalid input detected at '^' marker.

S1>en
Password:
Password:
S1#conf t
Enter configuration commands, one per line.  End with CNTL/Z.
S1(config)#no vlan 10
S1(config)#no vlan 20
S1(config)#no vlan 99
S1(config)#no vlan 100
S1(config)#no vlan 1000
S1(config)#vlan 22
S1(config-vlan)#name student
S1(config-vlan)#vlan 23
S1(config-vlan)#name teacher
S1(config-vlan)#vlan 24
S1(config-vlan)#name management
S1(config-vlan)#vlan 25
S1(config-vlan)#name library
S1(config-vlan)#vlan 26
S1(config-vlan)#name native
S1(config-vlan)#exit
S1(config)#int vlan 23
S1(config-if)#
*Aug 21 15:04:00.369: %LINEPROTO-5-UPDOWN: Line protocol on Interface Vlan23, changed state to downexit
S1(config)#int g1/0/6
S1(config-if)#switchport mode
S1(config-if)#switchport mode tr
S1(config-if)#switchport mode trunk
S1(config-if)#sw
S1(config-if)#switchport trunk
S1(config-if)#switchport trunk all
S1(config-if)#switchport trunk allowed  vlan 22
S1(config-if)#no sh
S1(config-if)#exit
S1(config)#exit
S1#sh
*Aug 21 15:05:16.295: %SYS-5-CONFIG_I: Configured from console by console vl br

VLAN Name                             Status    Ports
---- -------------------------------- --------- -------------------------------
1    default                          active    Gi1/0/1, Gi1/0/2, Gi1/0/3
                                                Gi1/0/4, Gi1/0/5, Gi1/0/6
                                                Gi1/0/7, Gi1/0/8, Gi1/0/9
                                                Gi1/0/10, Gi1/0/11, Gi1/0/12
                                                Gi1/0/13, Gi1/0/14, Gi1/0/15
                                                Gi1/0/16, Gi1/0/17, Gi1/0/18
                                                Gi1/0/19, Gi1/0/20, Gi1/0/21
                                                Gi1/0/22, Gi1/0/23, Gi1/0/24
                                                Gi1/0/25, Gi1/0/26, Gi1/0/27
                                                Gi1/0/28
22   student                          active
23   teacher                          active
24   management                       active
25   library                          active
26   native                           active
1002 fddi-default                     act/unsup
1003 token-ring-default               act/unsup
1004 fddinet-default                  act/unsup
1005 trnet-default                    act/unsup
S1#sh ip int br
Interface              IP-Address      OK? Method Status                Protocol
Vlan1                  unassigned      YES unset  up                    up
Vlan23                 unassigned      YES unset  up                    down
GigabitEthernet1/0/1   unassigned      YES unset  up                    up
GigabitEthernet1/0/2   unassigned      YES unset  up                    up
GigabitEthernet1/0/3   unassigned      YES unset  down                  down
GigabitEthernet1/0/4   unassigned      YES unset  down                  down
GigabitEthernet1/0/5   unassigned      YES unset  down                  down
GigabitEthernet1/0/6   unassigned      YES unset  down                  down
GigabitEthernet1/0/7   unassigned      YES unset  down                  down
GigabitEthernet1/0/8   unassigned      YES unset  down                  down
GigabitEthernet1/0/9   unassigned      YES unset  down                  down
GigabitEthernet1/0/10  unassigned      YES unset  down                  down
GigabitEthernet1/0/11  unassigned      YES unset  down                  down
GigabitEthernet1/0/12  unassigned      YES unset  down                  down
GigabitEthernet1/0/13  unassigned      YES unset  down                  down
GigabitEthernet1/0/14  unassigned      YES unset  down                  down
GigabitEthernet1/0/15  unassigned      YES unset  down                  down
GigabitEthernet1/0/16  unassigned      YES unset  down                  down
GigabitEthernet1/0/17  unassigned      YES unset  down                  down
GigabitEthernet1/0/18  unassigned      YES unset  down                  down
GigabitEthernet1/0/19  unassigned      YES unset  down                  down

S1#h run
help run
     ^
% Invalid input detected at '^' marker.

S1#sh run
Building configuration...

Current configuration : 1727 bytes
!
! Last configuration change at 15:05:16 UTC Wed Aug 21 2024
!
version 15.2
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname S1
!
boot-start-marker
boot-end-marker
!
enable secret 9 $9$GGtOPUBP6GxM.Z$d2Txn6pb8B5Kzac9Ls96ON34ms6aP1DgA.AuGc72RoY
enable password cisco123
!
username cisco
no aaa new-model
switch 1 provision c1000-24t-4g-l
system mtu routing 1500
!
!
!
!
!
!
!
!
!
!
spanning-tree mode rapid-pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
!
!
!
interface GigabitEthernet1/0/1
!
interface GigabitEthernet1/0/2
!
interface GigabitEthernet1/0/3
!
interface GigabitEthernet1/0/4
!
interface GigabitEthernet1/0/5
!
interface GigabitEthernet1/0/6
 switchport trunk allowed vlan 22
 switchport mode trunk
!
interface GigabitEthernet1/0/7
!
interface GigabitEthernet1/0/8
!
interface GigabitEthernet1/0/9
!
interface GigabitEthernet1/0/10
!
interface GigabitEthernet1/0/11
!
interface GigabitEthernet1/0/12
!
interface GigabitEthernet1/0/13
!
interface GigabitEthernet1/0/14
!
interface GigabitEthernet1/0/15
!
interface GigabitEthernet1/0/16
!
interface GigabitEthernet1/0/17
!
interface GigabitEthernet1/0/18
!
interface GigabitEthernet1/0/19
!
interface GigabitEthernet1/0/20
!
interface GigabitEthernet1/0/21
!
interface GigabitEthernet1/0/22
!
interface GigabitEthernet1/0/23
!
interface GigabitEthernet1/0/24
!
interface GigabitEthernet1/0/25
!
interface GigabitEthernet1/0/26
!
interface GigabitEthernet1/0/27
!
interface GigabitEthernet1/0/28
!
interface Vlan1
 no ip address
!
interface Vlan23
 no ip address
!
ip http server
ip http secure-server
!
!
!
!
line con 0
line vty 5 15
!
end

S1#
