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Router>en
Router#config t
Enter configuration commands, one per line.  End with CNTL/Z.
Router(config)#hostname R1
R1(config)#enable secret class
R1(config)#line con 0
R1(config-line)#password cisco
R1(config-line)#login
R1(config-line)#exit
R1(config)#line vty 0 15
R1(config-line)#password cisco
R1(config-line)#login
R1(config-line)#exit
R1(config)#service password-encryption
R1(config)#banner motd # "Unauthorized access is prohibited" #
R1(config)#interface g0/0
R1(config-if)#ip address 172.16.10.1 255.255.255.0
R1(config-if)#no shutdown
R1(config-if)#
*Aug 19 12:23:52.112: %LINK-3-UPDOWN: Interface GigabitEthernet0/0, changed state to down
*Aug 19 12:23:55.980: %LINK-3-UPDOWN: Interface GigabitEthernet0/0, changed state to up
*Aug 19 12:23:56.980: %LINEPROTO-5-UPDOWN: Line protocol on Interface GigabitEthernet0/0, changed state to up
R1(config-if)#ex
R1(config)#interface g0/1
R1(config-if)#ip address 172.16.11.1 255.255.255.0
R1(config-if)#no shutdown
R1(config-if)#
*Aug 19 12:25:21.900: %LINK-3-UPDOWN: Interface GigabitEthernet0/1, changed state to down
*Aug 19 12:25:23.980: %LINK-3-UPDOWN: Interface GigabitEthernet0/1, changed state to up
*Aug 19 12:25:24.980: %LINEPROTO-5-UPDOWN: Line protocol on Interface GigabitEthernet0/1, changed state to up

*Aug 19 12:35:20.651: %SYS-5-CONFIG_I: Configured from console by console "Unauthorized access is prohibited"

 "Unauthorized access is prohibited"

User Access Verification

Password:
Password:
R1>en
Password:
Password:
R1#sh run
Building configuration...

Current configuration : 1415 bytes
!
! Last configuration change at 12:35:20 UTC Mon Aug 19 2019
!
version 15.4
service timestamps debug datetime msec
service timestamps log datetime msec
service password-encryption
!
hostname R1
!
boot-start-marker
boot-end-marker
!
!
enable secret 5 $1$QbU7$inNn.bm3GflAS6aMpgOnl/
!
no aaa new-model
no ip domain lookup
ip cef
no ipv6 cef
multilink bundle-name authenticated
!
!
cts logging verbose
!
!
license udi pid CISCO2901/K9 sn FCZ1930C0VQ
!
!
!
redundancy
!
!
!
!
!
!
interface Embedded-Service-Engine0/0
 no ip address
 shutdown
!
interface GigabitEthernet0/0
 ip address 172.16.10.1 255.255.255.0
 duplex auto
 speed auto
!
interface GigabitEthernet0/1
 ip address 172.16.11.1 255.255.255.0
 duplex auto
 speed auto
!
interface Serial0/0/0
 no ip address
 shutdown
 clock rate 2000000
!
interface Serial0/0/1
 no ip address
 shutdown
 clock rate 2000000
!
ip forward-protocol nd
!
no ip http server
no ip http secure-server
!
!
!
!
!
control-plane
!
!
banner motd ^C "Unauthorized access is prohibited" ^C
!
line con 0
 password 7 060506324F41
 login
line aux 0
line 2
 no activation-character
 no exec
 transport preferred none
 transport output pad telnet rlogin lapb-ta mop udptn v120 ssh
 stopbits 1
line vty 0 4
 password 7 0822455D0A16
 login
 transport input none
line vty 5 15
 password 7 0822455D0A16
 login
 transport input none
!
scheduler allocate 20000 1000
!
end

R1#sh ip int brief
Interface                  IP-Address      OK? Method Status                Protocol
Embedded-Service-Engine0/0 unassigned      YES unset  administratively down down
GigabitEthernet0/0         172.16.10.1     YES manual up                    up
GigabitEthernet0/1         172.16.11.1     YES manual up                    up
Serial0/0/0                unassigned      YES unset  administratively down down
Serial0/0/1                unassigned      YES unset  administratively down down
R1#




Switch>en

Switch#config t
Enter configuration commands, one per line.  End with CNTL/Z.
Switch(config)#hostname S1
S1(config)#no ip domain-lookup
S1(config)#banner motd # "Access not authorized" #
S1(config)#interface vlan1
S1(config-if)#ip address 172.16.11.10 255.255.255.0
% Nameserver entry 192.168.214.34 does not exist
% Nameserver entry 192.168.214.38 does not exist

S1(config-if)#no shutdown
S1(config-if)#ip address 172.16.11.10 255.255.255.0
S1(config-if)#no shutdown
S1(config-if)#exit
S1(config)#exit
S1#sh
*Mar 11 20:23:32.891: %SYS-5-CONFIG_I: Configured from console by consoleip
% Incomplete command.

S1#sh ip interface brief
Interface              IP-Address      OK? Method Status                Protocol
Vlan1                  172.16.11.10    YES manual up                    up
FastEthernet0/1        unassigned      YES unset  down                  down
FastEthernet0/2        unassigned      YES unset  down                  down
FastEthernet0/3        unassigned      YES unset  down                  down
FastEthernet0/4        unassigned      YES unset  down                  down
FastEthernet0/5        unassigned      YES unset  up                    up
FastEthernet0/6        unassigned      YES unset  up                    up
FastEthernet0/7        unassigned      YES unset  down                  down
FastEthernet0/8        unassigned      YES unset  down                  down
FastEthernet0/9        unassigned      YES unset  down                  down
FastEthernet0/10       unassigned      YES unset  down                  down
FastEthernet0/11       unassigned      YES unset  down                  down
FastEthernet0/12       unassigned      YES unset  down                  down
FastEthernet0/13       unassigned      YES unset  down                  down
FastEthernet0/14       unassigned      YES unset  down                  down
FastEthernet0/15       unassigned      YES unset  down                  down
FastEthernet0/16       unassigned      YES unset  down                  down
FastEthernet0/17       unassigned      YES unset  down                  down
FastEthernet0/18       unassigned      YES unset  down                  down
FastEthernet0/19       unassigned      YES unset  down                  down
FastEthernet0/20       unassigned      YES unset  down                  down
FastEthernet0/21       unassigned      YES unset  down                  down
FastEthernet0/22       unassigned      YES unset  down                  down
FastEthernet0/23       unassigned      YES unset  down                  down
FastEthernet0/24       unassigned      YES unset  down                  down
GigabitEthernet0/1     unassigned      YES unset  down                  down
GigabitEthernet0/2     unassigned      YES unset  down                  down
S1#config t
Enter configuration commands, one per line.  End with CNTL/Z.
S1(config)#ip?
ip  ipc

S1(config)#ip gat?
% Unrecognized command
S1(config)#ip g?
gdp  gratuitous-arps

S1(config)#ip de?
default-gateway  device

S1(config)#ip de
S1(config)#ip de
S1(config)#ip default-gateway
% Incomplete command.

S1(config)#ip default-gateway device
                              ^
% Invalid input detected at '^' marker.

S1(config)#ip default-gateway 172.16.11.1
S1(config)#ex
% Ambiguous command:  "ex"
S1(config)#exit
S1#s
*Mar 11 20:27:38.635: %SYS-5-CONFIG_I: Configured from console by consoleh
% Type "show ?" for a list of subcommands
S1#sh ip interface brief
Interface              IP-Address      OK? Method Status                Protocol
Vlan1                  172.16.11.10    YES manual up                    up
FastEthernet0/1        unassigned      YES unset  down                  down
FastEthernet0/2        unassigned      YES unset  down                  down
FastEthernet0/3        unassigned      YES unset  down                  down
FastEthernet0/4        unassigned      YES unset  down                  down
FastEthernet0/5        unassigned      YES unset  up                    up
FastEthernet0/6        unassigned      YES unset  up                    up
FastEthernet0/7        unassigned      YES unset  down                  down
FastEthernet0/8        unassigned      YES unset  down                  down
FastEthernet0/9        unassigned      YES unset  down                  down
FastEthernet0/10       unassigned      YES unset  down                  down
FastEthernet0/11       unassigned      YES unset  down                  down
FastEthernet0/12       unassigned      YES unset  down                  down
FastEthernet0/13       unassigned      YES unset  down                  down
FastEthernet0/14       unassigned      YES unset  down                  down
FastEthernet0/15       unassigned      YES unset  down                  down
FastEthernet0/16       unassigned      YES unset  down                  down
FastEthernet0/17       unassigned      YES unset  down                  down
FastEthernet0/18       unassigned      YES unset  down                  down
FastEthernet0/19       unassigned      YES unset  down                  down
FastEthernet0/20       unassigned      YES unset  down                  down
FastEthernet0/21       unassigned      YES unset  down                  down
FastEthernet0/22       unassigned      YES unset  down                  down
FastEthernet0/23       unassigned      YES unset  down                  down
FastEthernet0/24       unassigned      YES unset  down                  down
GigabitEthernet0/1     unassigned      YES unset  down                  down
GigabitEthernet0/2     unassigned      YES unset  down                  down
S1#ip de?
% Unrecognized command
S1#config t
Enter configuration commands, one per line.  End with CNTL/Z.
S1(config)#ip default-gateway
% Incomplete command.

S1(config)#ip default-gateway 172.16.11.1
S1(config)#line vty 0 15
S1(config-line)#password cisco
S1(config-line)#login
S1(config-line)#exit
S1(config)#exit
S1#sh
*Mar 11 20:30:52.421: %SYS-5-CONFIG_I: Configured from console by consoleow run
Building configuration...

Current configuration : 1454 bytes
!
! Last configuration change at 20:30:52 UTC Thu Mar 11 1993
!
version 15.0
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname S1
!
boot-start-marker
boot-end-marker
!
!
no aaa new-model
system mtu routing 1500
!
!
no ip domain-lookup
!
!
!
!
!
!
!
!
spanning-tree mode pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
!
!
!
interface FastEthernet0/1
!
interface FastEthernet0/2
!
interface FastEthernet0/3
!
interface FastEthernet0/4
!
interface FastEthernet0/5
!
interface FastEthernet0/6
!
interface FastEthernet0/7
!
interface FastEthernet0/8
!
interface FastEthernet0/9
!
interface FastEthernet0/10
!
interface FastEthernet0/11
!
interface FastEthernet0/12
!
interface FastEthernet0/13
!
interface FastEthernet0/14
!
interface FastEthernet0/15
!
interface FastEthernet0/16
!
interface FastEthernet0/17
!
interface FastEthernet0/18
!
interface FastEthernet0/19
!
interface FastEthernet0/20
!
interface FastEthernet0/21
!
interface FastEthernet0/22
!
interface FastEthernet0/23
!
interface FastEthernet0/24
!
interface GigabitEthernet0/1
!
interface GigabitEthernet0/2
!
interface Vlan1
 ip address 172.16.11.10 255.255.255.0
!
ip default-gateway 172.16.11.1
ip http server
ip http secure-server
!
banner motd ^C "Access not authorized" ^C
!
line con 0
line vty 0 4
 password cisco
 login
line vty 5 15
 password cisco
 login
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mmand Prompt

Hicrosoft Windows [Version 16.6.17134.956]
(c) 2018 Microsoft Corporation. All rights reserved

C: \Users\Admin>ping 172.16.16.254

Pinging 172.16.16.254 with 32 bytes of data:
Reply from 172.16.16.254: bytes-32 time<ims TTL=127
Reply from 172.16.16.254: bytes=32 time=ims
Reply from 172.16.16.254: bytes=32 time=ims
Reply from 172.16.16.254: bytes-32 time=ims TTL-127

Ping statistics for 172.16.16.254:

Packets: Sent - 4, Received - 4, Lost = @ (8% loss)
lApproximate round trip times in milli-seconds:
Minimun = ems, Maximum - ims, Average = ems

C:\Users\Admin>
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Command Prompt

(C:\Users\Adnin>ipconfig /all

Windows TP Configuration

Host Name . . . © e . ... . : DESKTOP-3HOLFT:
Primary Dns Suffix

Node Type . . . S e YD

Ip Routing Enabled. . . . . . . . : Mo

WINS Proxy Enabled. . . . . ... :No

Ethernet adapter Ethernet:

Connection-specific DNS Suffix .

Description . . . . . .. ... .: Realtek PCle GBE Family Controller
Physical Address. 9C-5C-8E-94-88-CE

DHCP Enabled.
Autoconfiguration Enabled .
Link-local IPv6 Address .
1Pv4 Address.

Subnet Mask .

Default Gateway . .16.11.1

DHCPYV6 TAID . S e AIRGTIAD

DHCPV6 Client DUID. . . . . . . . : ©0-81-60-61-22-F3-38-DA-9C-5C-8E-94-88-CE
DNS Servers . %1

463e:c60d: bbd: 337b%9 (Preferred)
.16.11.254(Preferred)
.255.255.6

fec6:0:0: FFFF::3%1
NetBIOS over Tcpip. . . . . . . . : Enabled

C:\Users\Admin>
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:\Users\Admin>ipconfig /all

Windows IP Configuration

Host Name . . . ... ... .: OVALCISCO-e4
Primary Dns Suffix’

Node Type . . . Hybrid

Ip Routing Enabled. aozssads O

WINS Proxy Enabled. . . . . ... :No

Ethernet adapter Local Area Connection:

Connection-specific DNS Suffix
Description .

Physical Address.

DHCP Enabled.
Autoconfiguration Enabled
Link-local IPv6 Address .
1Pv4 Address.

Subnet Mask .

Default Gateway .

DHCPY6 TATD .

DHCPY6 Client DUID.

DNS Servers .

: Realtek PCIe GBE Family Controller
9C-5C-8E-94-85-F1

9C06:5531:1164:651b%17 (Preferred)
172.16.16.254(Preferred)

: 255.255.255.6

172.16.16.1

245128334

: 60-61-00-01-1E-CC-BC-E7-9C-5C-8E-94-85-F1

NetBIOS over Tcpip.

C:\Users\Admin>




