Martin Darzins: Student ID 1909722
TASK 1
[image: ]
Step 7a – Ipconfig 192.168.1.10
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7b – ping 192.168.1.11
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Step 8a – Ipconfig 192.168.1.11
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8b – ping 192.168.1.10
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TASK 2
Step 5 – Home laptop is Automatically configured via Wi-Fi
Step 7 - MAD’s Home Laptop – ipconfig /all
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Step 8 – ping www.google.com
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Step 9 – tracert www.google.com
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Microsoft Windows [Version 10.0.19041.508]
(c) 2626 Microsoft Corporation. All rights reserved.

:\Users\Martin>ipconfig /all

iindows IP Configuration

Host Name . . . DESKTOP-BTK5196
Primary Dns Suffix’

Node Type . . Hybrid

Ip Routing Enabled. No

WINS Proxy Enabled No

DNS SuFfix Search List. lan

thernet adapter Ethernet:

Media State . Media disconnected
Connection-specific DS Suffix

Description . e Realtek PCIe GbE Family Controller
Physical Address. 30-F9-ED-AQ-BF -BF

DHCP Enabled. Yes

Autoconfiguration Enabled . Yes
ethernet adapter VirtualBox Host-Only Network:

Connection-specific DNS Suffix

Description . VirtualBox Host-Only Ethernet Adapter
Physical Address. 0A-00-27-00-00-67
DHCP Enabled.

Autoconfiguration Enabled .
Link-local IPv6 Address .
1Pv4 Address.

Subnet Mask .

Default Gateway .

1C74:b48: Feb7%7 (Preferred)
192.168.56.1(Preferred)
255.255.255.6

DHCPV6 TAID . . 755630119
DHCPV6 Client DUID. ©0-01-60-01-20- 8¢ -AB-4£-30-FO-ED-A-BF-BF
DNS Servers . :

NetBIOS over Tcpip.
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wireless LAN adapter Local Area Connection* 11:

Media State .
Connection-specific DS Suffix
Description . e
Physical Address.

DHCP Enabled. .
Autoconfiguration Enabled .

: Media disconnected

Microsoft Wi-Fi Direct Virtual Adapter #3

: 3E-77-E6-DC-E7-83

ves

: Yes

wireless LAN adapter Local Area Connection* 12:

Media State .

Connection-specific DNS Suffix

Description .
Physical Address.

DHCP Enabled. .
Autoconfiguration Enabled .

wireless LAN adapter WiFi

Connection-specific DNS Suffix
Description . e
Physical Address.

DHCP Enabled. .
Autoconfiguration Enabled .
1Ipv6 Address. .
Temporary Ipv6 Address.
Link-local IPv6 Address .

1Pv4 Address.

Subnet Mask .

Lease Obtained.

Lease Expires .

Default Gateway .

DHCP Server .
DHCPV6 TAID . .
DHCPV6 Client DUID.
DNS Servers . . . .
NetBIOS over Tcpip.

: Media disconnected

Microsoft Wi-Fi Direct Virtual Adapter #4

: 3E-77-E6-DC-EF-83

No

: Yes

: lan

Broadcom 862.11n Network Adapter
3C-77-E6-DC-E7-83

: Yes

: fdaa:bbcc:ddee:0:7477:5b8: cc38:351(Preferred)

Fego: :317d:11a5: e7e3:1dbc%9 (Preferred)
192.168.1.14(Preferred)

: 255.255.255.0

01 October 2020 09:42:06
02 October 2020 13:24:07

: fes0::36db:ocFF:fefa:bca3no

192.168.1.1
192.168.1.1

: 540833766

00-61-00-01-20-8E-A8-4E-30-FO-ED-AD-BF -BF
192.168.1.1
Enabled

Connection-specific DNS Suffix Search List :

lan
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Ethernet adapter Bluetooth Network Connection:

Media State . . . : Media disconnected
Connection-specific DS Suffix

Description . e Bluetooth Device (Personal Area Network)
Physical Address. : 3C-77-E6-DC-E7-84

DHCP Enabled. . Yes

Autoconfiguration Enabled . : Yes
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Microsoft Windows [Version 10.0.19041.508]
(c) 2026 Microsoft Corporation. All rights reserved.

:\Users\Martin>ping ww.google. com

Pinging w.google. con [172.217.169.4] with 32 bytes of data:
Reply from 172.217.
Reply from 172.217.
Reply from 172.217.169.4: bytes=32 time=3gms TTL-118
Reply from 172.217.169.4: bytes=32 time=4oms TTL-118

Ping statistics for 172.217.160.4:

Packets: Sent = 4, Received = 4, Lost = @ (8% loss),
Approximate round trip times in milli-seconds:

Minimum = 24ms, Maximum = 49ms, Average = 34ms
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C:\Users\Martin>tracert www.

Tracing route to www.google.

over a maximum of 36 hops:
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ttrouter [192.168.1.1]
Request timed out.
ae52-nere@1.nec.as13285.net [78.144.1.9]
ae52-5Cr161. th.as13285.net [78.144.1.8]
72.14.209.16

209.85.248.229

209.85.241.93

1hr25526-1n-F4.1€106.net [172.217.169.4]
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152.168.1.10
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C:\>ping 192.1€8.1.11

Pinging 152.168.1.11 with 32 bytes of data:

Reply from 152.163.1.11: byces:
Reply from 152 163 1 11: byces:
Reply from 152 163 1 11: byces:
Reply from 152.163 1 11: byves=:

2 vime=lms TTL-128
2 vime<lms TTL-128
2 vime=lms TTL-128
2 vime<lms TTL-128

Ping stavisties for 192.168.1.11:
Packets: Sent = 3, Received = 4, Lost = 0 (0% loss),
Bpprosimate round trip vimes in milli-seconds
Minimm = Ons, Maximm = lms, Average = Oms
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Packet Tracer BC Command Line 1.0
C:\>ipeontiy

FastEthernet0 Connection: (default port)

Connection-specific DNS Suffix

152.168.1.11
2552852550
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C:\>ping 152.168.1.10

Pinging 152.168.1.10 with 32 byves of data:

Reply from 152.163.1.10
Reply from 152 163 1 10:
Reply from 152 163 1 10
Reply from 152 163 1 10:

cimemlms TTI-128
cime=ams TTL-128
cime=lms TTL-128
cime<lms TTL-128

Ping scavistics for 152.168.1.10
Packets: Sent = 3, Received = 4, Lost = 0 (0% loss),
Bpproximate round trip times in milli-seconds:
Minimm = Ons, Maximm = 3ms, Average = lms





