Recap IPV4 Addressing
a) For the following IP addresses deduce the network ID and Broadacast address

(i) 192.168.10.253 /24
(ii) 192.168.10.253 /25
(iii) 192.168.10.253 /26
(iv) 192.168.10.253 /27
(v) 192.168.10.253 /30
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Recap -OSPF
Work in groups of 3

1. Use Cisco Real Devices to implement the given Topology
2. Design and assign IPV4 Addresses to topology devices and links
3. Configure  Single Area OSPF
RID for R1 is 1.1.1.1
RID for R2 is 2.2.2.2
RID for R3  is 3.3.3.3
RID for  R4 is 4.4.4.4.
4. Make  sure PCs can ping each other
5. Identify DR, BDR and Drothers
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