Portfolio 2 : Task 1 (Network Test)
SD-C
IPCONFIG /ALL: Confirm the IP address matches the topology provided.
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ping 192.168.1.10: Must be successful.
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ping 192.168.2.1: Must be successful.
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ping 192.168.2.10: Must be successful.
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L-CD
ip address: Confirm the IP address matches the topology provided. [image: A screenshot of a computer screen
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ping 192.168.1.10: Must be successful.
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ping 192.168.1.1: Must be successful.
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192.168.2.10
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