	Device
	Issue
	Action

	HUB
	Did not have IP NAT INSIDE configuration set on device
	telnet from pc1 to branch-1 router and telnet from there to hub where configuration can be set on serial0/1/0 interface

	Factory router
	Interface g0/0/1 is down causing pc3 to not be able to ping internet server
	telnet from pc2 to factory router where interface g0/0/1 can be brought online

	Factory router
	PC3 cannot be pinged by other devices, OSPF config missing on factory router
	telnet from PC2 to factory router where missing ospf config can be added

	PC5
	PC5 cannot ping anything
	Correct default gateway sourced and added to PC5 IP config

	Branch-2
	PC6 & 7 cannot ping internet server
	S0/1/0 interface is not configured correctly, needs IP address added



