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PC-A ipconfig and ping to pc-b
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PC-B ipconfig and ping to pc-a
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R1 configuration using “show running-configration” command
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SWICH configuration with “show running-config” command. 
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