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 	Lab 3: Design and Configure IPv4 Network 
 
 
 	Kindly note that the step by step instruction for this lab is  demonstrated during the tutorial session. After completing the lab, you 
have to submit both the packet tracer file and the document via moodle Objectives n.kaliyamurthy@uwtsd.ac.uk
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Task 1: Determine and Calculate IPv4 Address Subnetting 
Task 2: Calculate VLSM Subnetting 
Task 3: Build a Network and configure End and Intermediate devices Required Resources 
· 1 PC (Windows with Internet access) 
· Optional: IPv4 address calculator 
· Packet Tracer (Latest version) 
[image: ]ABC Corporation is a small business company which has an existing network which requires some modifications. Based on the requirements, you are expected to subnet the network and configure the devices. Do Variable Length Subnet Masking. You are asked to use IP Addressing Scheme:   
 
 
 
 
 
 
 
Fill the tables with appropriate information/ details. 
	
	Subnet as per the Requirement 
	

	Specification 
	Network: A 
	Network: B 
	Network: C 

	Network Address 
	 192.168.100.0
	 192.168.100.96
	192.168.100.64 

	Subnet Mask 
	 255.255.255.192
	 255.255.255.252
	255.255.255.224

	No. of asked hosts/subnet 
	50 
	2 
	20 

	No. of usable hosts/ subnet 
	 62
	 2
	 30

	First Usable Host (FUH) 
	 192.168.100.1
	 192.168.100.97
	 192.168.100.65

	Last Usable Host  (LUH) 
	 192.168.100.62
	 192.168.100.98
	 192.168.100.94

	Broadcast Address 
	 192.168.100.63
	 192.168.100.99
	 192.168.100.95

	
	Addressing Table 
	

	Device 
	Requirement 
	IP address 
	Subnet Mask 
	Gateway 

	PC1  
	1st Usable Host 
Network: A 
	 192.168.100.1
	255.255.255.192 
	192.168.100.62 

	Laptop1  
	2nd Usable Host 
Network: A 
	 192.168.100.2
	255.255.255.192 
	192.168.100.62 

	PC2  
	1st Usable Host 
Network: B 
	 192.168.100.97
	 255.255.255.252
	192.168.100.98 

	PC3 
	1st Usable Host 
Network: C 
	 192.168.100.65
	 255.255.255.224
	192.168.100.94 

	Laptop0 
	2nd Usable Host 
Network: C 
	 192.168.100.66
	255.255.255.224 
	[bookmark: _GoBack]192.168.100.94 

	RAI G0/0/0 
	Last Usable 
Host             
Network: A 
	 192.168.100.62
	 255.255.255.192
	N/A 

	RIBC G0/0/1 
	Last Usable 
Host 
Network: B 
	 192.168.100.98
	255.255.255.252 
	N/A 

	RIBC G0/0/0 
	Last Usable 
Host 
Network: C 
	 192.168.100.94
	255.255.255.224 
	N/A 


Create the below Topology
 
 

Initialize the Device and configure step by step:  
1. Initialize ALL the Switches.  
2. Delete the Old VLan Database in ALL the Switches (S0, S1 & S2) and reload. 
3. Check the Switches with appropriate command to find Old VLan Database is deleted. 
Write down the above command here: show vlan brief
4. Configure all the End devices (Hosts) with appropriate IP Address, Subnet Mask and Default Gateway.  
5. Assign host names as per the topology for all intermediate devices.  
6. Set a minimum length for passwords as 7 in all routers.  
7. Assign Encrypted Privileged Passwords for all routers. (Set as ciscoebl)
8. Configure Console Connection: Set password for RAI Console as ciscocon.   
9. Configure Line Connection and allow only Telnet Access for RAI:  
Total 5 Lines, Password for Line Connection is ciscovty.  
10. Encrypt all the Clear Text Passwords for all routers. 
11. Create a Banner (MOTD) for all routers "ONLY AUTHORISED ACCESS".  
12. Based on the Addressing Table derived by you at IPv4 Addressing Scheme Part, Configure the G0/0/0, G0/0/1 for RIBC and G0/0/0 Interface of Router RAI and activate the interface with appropriate IP Address. Add Descriptions suitable to the Topology. 
13. Disable DNS Lookup in Router RAI.  
14. Configure Domain Name as www.advancednetworking.com  
Configure 
all the switches
:
 
 

15. Assign Names as per the Label for Switches.  
16. Shut down all unused ports in switches. 
17. Ping Test from all Hosts to confirm the working Network. Troubleshoot if needed.  
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