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	Contract Name:
	Single two story detached building with loft

	Method Statement Title:
	Pouring Concrete

	Activity Start Date on Site:
	06/05/2020

	
	Signature:
	D.matthews

	Method Statement 

Prepared by: 
	Dylan Matthews
	Date:
	25/04/2020


	Title:
	Two Storey detached building with loft excavation method

	
	

	Risk Assessment
	 See Risk Assessment  Hazards and Control Measures as Attached. 

	Scope of Works
	This method statement outlines the proposals for the work activities associated with:

Pouring Concrete
The purpose of this method statement is to explain the proper procedure on how to prepare and cast slab on grade or any horizontal element or member including fixation of steel reinforcement, MEP embedment’s, fixing of shutter etc. without injuries.

	Plant & Equipment
	Concrete Pump

Concrete Mixer

Mini truck

Bob cat

Concrete vibrators

Wheel borrow

Slump tray

Slump cone and other associated tools

Rubber hammer

	Methodology
	Concrete pouring 

· The concrete mixer must be stopped at the check point for the inspection of slump test and to obtain sample cubes for test.

· One set of cubes shall be taken every 50 cubic meter concrete, each set consist of 6 cubes, 3 cubes to be tested on 7th days and 3 cubes to be tested for 28th days.

· Extra three cubes can be made for re-checking if in case circumstances may happen.

· Unload the concrete within 90 minutes from the batching plant loading time.

· Compact the concrete properly by using mechanical vibrators, extra vibrator shall be available in case of any shortage or mechanical problems.

· Use approved hardener material after casting concrete when required. Make sure applications shall be as per manufacturer’s recommendation.

· Use the power float for the smooth finish surface purpose. Store extra power float near the casting area in case of any mechanical malfunctioning.

· Cure the casted area properly with covering concrete with hessian cloth and polythene sheet on top but before placing the concrete wet the hessian with water.

· Cure the concrete by spraying water three times per day for a period of 7 days.

· The casted area or member shall be protected by placing barricade to prevent plants and machineries damaged the concrete.

· Concrete pour card shall be filled by Quality Engineer and to be submitted to the Engineer including concrete delivery notes, this task will be done whenever required.

· Concrete cube test report shall be submitted to the Engineer



	First Aid  &  PPE
	PPE
Mandatory 

· Safety Helmet EN397

· High Visibility Jacket or Vest 

· Safety Footwear 

· Gloves 

All works shall comply with safety procedure or instruction set out in project safety plan and municipality rules and regulations.

Basic PPE to be worn by all staff and laborers.

Trained operator and banksman would be engaged to control or operate heavy equipment machine.

Provide sufficient lighting whenever night casting.
 

	Environment
	Spill kits will be readily available during works so any spillages can be contained and dealt with.

	Emergency  Procedures
	· All personnel to sign in/out when leaving site.

· Assembly point at site access gate

· Nearest A&E Hospital: 
Morriston Hospital 
· Report all accidents/incidents to site supervisor immediately so it can be recorded.

· In the event of a spillage contain the area using a spill Kit and report to the site supervisor immediately.

· Spill kits are sited in site compound.



