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[bookmark: _GoBack]Project Description

CABAT CONSULTING Ltd are pleased to present this construction phase plan and statement for the proposed development off Kings Road, Swansea, the new University Atrium ‘Glyndwr’.

A brief description would describe the development which is to be carried out in one phase consisting of a steel frame super-structure, a mixture of brick & block cavity insulated walls, composite cladding and a green wall. Internal timber SIP’s panels to the floors and walls with a timber trussed flat roof structure, Aluminium & UPVC windows and doors with solar PV panels.  

Various external finishes to each elevation of the building including recycled composite cladding along with a clay facing brick to the external walls. The roof will have a single ply membrane to the flat roof and EDPM covering. 
Internally, supporting steel with SIP’s partitions, dry walls and paint finished walls to each room on each floor.

There will car parking to the external of the buildings complete with hard and soft landscaped areas 

[bookmark: _Toc39000521]Programme Details

Please refer to the programme for further details.
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	Date

	Issue of Pre-Construction Information to Principal Contractor
	02/04/2020

	Time allocated by Client for the planning and preparation of the construction work
	4 weeks 

	Start of construction phase
	2020

	Duration
	85 Weeks 

	Last date for contractors (including Principal Contractor) to submit final information for Health & Safety File
	20/03/2020

	
	



[bookmark: _Toc39000523]Key Role Holders
	Title
	Address Details
	Contact Details

	Client
	UWTSD, 
1 KINGS ROAD
SWANSEA
SA1 8PH

	Name: 
Tel:
Fax:
E-mail:
Mobile:
	Allan Nantel
01792493696

Alan.nantel@uwtsd.ac.uk

	Client
	As Above
	Name: 
Tel:
Fax:
E-mail:
Mobile:
	Juan Ferriz-Papi
01792493696

Juan.ferris-papi@uwtsd.ac.uk

	Principal Designer
	CABAT CONSULTING LTD
CRWYS STREET
SWANSEA 
SA1 9JU
	Name: 
Tel:
Fax:
E-mail:
Mobile:
	Chris Abat


cabat.consult@designtech.co.uk
07814963517


	Architect
	As Above
	Name: 
Tel:
Fax:
E-mail:
Mobile:
	Tracy King


1403139@student.uwtsd.ac.uk
07817924932


	Civil Engineer
	As Above
	Name: 
Tel:
Fax:
E-mail:
Mobile:
	Cerys Cole


P151440@student.uwtsd.ac.uk
07816210410

	Construction Manager
	As Above
	Name: 
Tel:
Fax:
E-mail:
Mobile:
	Adam Meyrick


1706760@student.uwtsd.ac.uk
07469217247

	Quantity Surveyor
	[bookmark: _Toc35281034][bookmark: _Toc35282237][bookmark: _Toc39000524]As Above
	Name: 
Tel:
Fax:
E-mail:
Mobile:
	Bethan Stroud


1702210@student.uwtsd.ac.uk
07783415165

	Building Surveyor
	[bookmark: _Toc35281035][bookmark: _Toc35282238][bookmark: _Toc39000525]As Above
	Name: 
Tel:
Fax:
E-mail:
Mobile:
	Alex Morgan


@student.uwtsd.ac.uk
07488290440




[bookmark: _Toc39000526]Health and Safety Goals

This project will be managed and controlled in such a way as to minimise risks to employees, contractors, occupiers of Kings Road, members of the public and any other person who may be affected by the preparation and/or construction works planned to take place.

We will also take all reasonable measures to minimise the effects our activities (and those of our contractors) will have on the environment.

[bookmark: _Toc39000527]Monitoring and Review

· On-site activities will be monitored on an ongoing basis by our Site Manager.  The Site Manager will also record weekly safety checks, this will be overseen by the Contracts Manager in addition to our internal Health and Safety Dept. We will carry out weekly inspections and audits highlighting both areas which require improvement and good practice.
· Contractors are required to provide adequate supervision and monitoring of their works and will, during site meetings, be requested to report on health and safety standards being achieved. Sub-contractor method statements will detail the contractor’s arrangements for monitoring and review.
· Regular health and safety review meetings will be held throughout the contract (during contract review meetings) and notes will be taken. Particular attention will be paid to the changes that occur as the project progresses and the measures necessary to ensure that health and safety is properly managed.

[bookmark: _Toc39000528]On-Site Liaison

· The senior supervisor for each contractor will be nominated as the Liaison Officer for that contractor and will be identified with a Black Safety hat.

· The Site Manager will act as the liaison between project organisations and personnel, and neighbouring buildings occupiers/management.

[bookmark: _Toc39000529]Consultation with the workforce

· The workforce will be encouraged to consult with site management at every opportunity (i.e. during inductions, briefings, toolbox talks and other site meetings including DCM).

· An ‘open door’ policy is in place.  All site operatives are able (and encouraged) to approach site management with their queries and observations.
· If sub-contractors bring to site any personnel who may not consider English to be their first language, the Site Manager will consider whether special measures will be necessary to ensure they can be provided with suitable and sufficient information, instruction, training and supervision.
· Daily consultation meetings are held every morning in the site office to discuss the hazards of the day.
[bookmark: _Toc39000530]Arrangements for the Exchange of Design Information

· Design information will be exchanged during our meetings with the Designers.
· As deemed necessary by the nature of any design changes, we will distribute design information to the Client, Principal Designer and our sub-contractors via the most appropriate means.
· Records of issue will be retained.
· Should a design change warrant a review of working methods, our and our sub-contractors risk assessments and method statements will be amended, with information being conveyed to the workforce via toolbox talk.

[bookmark: _Toc39000531]Selection and Control of Sub-Contractors

· Sub-contractors appointed by us will be selected after consideration of previous experience on similar types of projects and evidence of organisational capability. 
· Where sub-contractors are involved in design work, their names will be forwarded to the Principal Designer.
· All sub-contractors will provide the Site Manager with risk assessments and, where necessary, method statements relating to their site operations. The Site Manager will check this documentation and ensure it is relevant and comprehensive, together with evidence of relevant training of individuals allocated to the project, before allowing work by that contractor to commence.
[bookmark: _Toc39000532]Arrangements for Exchange of Health & Safety Information

· The senior person from each organisation on site is responsible for ensuring that health and safety information is exchanged between themselves, the principal contractor and other site contractors.
· The Site Manager will be responsible for coordinating the exchange of information.


Site Security

· We will install 2m high security fencing/hoarding to all boundaries. Where possible we will erect suitable permanent site boundaries early into the programme.  Where necessary, additional localised temporary fencing will be provided around the work areas. Work areas and means of access/egress will be as agreed with the Client and Principal Designer.  
· The site and the compound area will be left in a secure state at the end of each working day.  
· All equipment and materials will be safely stored when not in use.  During working hours, regular monitoring of the site will take place to ensure that no unauthorised persons are present within the work areas.
· It has been agreed that security personnel will be required with a minimum of two security officers patrolling the site from the hours of 1600 – 0600 hrs. The duration of the security cover will be reviewed on 13/08/20.
[bookmark: _Toc39000533]Site Inductions

· All site personnel will receive site inductions on the morning of their first day on site and before being permitted to commence work on site. 
· The content of the site inductions will be as detailed on the induction schedule, but specific to this particular site.
· Site visitors (delivery personnel etc.) will receive inductions covering those topics relevant to their activities.
· Where necessary, measures will be taken to ensure that foreign workers receive suitable inductions.
On-Site Training
· In addition to site inductions, all sub-contractors are required to provide their personnel with on-site training. This can take the form of toolbox talks, method statement and risk assessment briefings, and any other training that may be necessary to ensure that they can carry out their tasks safely.
[bookmark: _Toc39000534]Welfare & Hygiene

· Welfare facilities will be provided from day one of the construction phase, consisting of toilet, washing (with hot water) and drying facilities and space for making meals. 

·  All facilities will comply with the requirements of CDM 2015 (Schedule 2).  

· Operatives will be instructed to use the facilities in an appropriate manner and to assist in keeping them clean and tidy.

· Sub-contractors are required to provide an appointed person and first aid kit for treating minor injuries. 

· The site first aid post is located in the site office.  The First Aider/Appointed Person for the site is TBC during the initial enabling works followed by TBC during the main build. 

· Welfare, hygiene and first aid arrangements will be communicated to all personnel during site inductions.

[bookmark: _Toc39000535]RIDDOR Procedures

· We will ensure that all contractors are aware of the reporting procedures for accidents and dangerous occurrences, as detailed in RIDDOR 2013, and as per the reporting procedures stated in our company safety policy. 
· All accidents and incidents will be reported to the Site Manager at the earliest opportunity and recording in our site accident book.
· Although a period of within 15 days is specified for over 7 day injuries for submitting Forms 2508(Rev) online to the HSE, the Site Manager will require sight of any report as soon as sufficient details of the accident/ DO are available.
· Details will be forwarded to the CABAT CONSULTING LTD Health and Safety Department at the earliest opportunity.
[bookmark: _Toc39000536]Production & Approval of Safety Documentation

· Risk assessments will be carried out by contractors for all activities. These will be provided to the Site Manager before work starts on site. Once they have been checked, then work may proceed, subject to all identified control measures being in place.  
· Where the risk assessment identifies the need for a written method statement to be prepared, this will also be handed to the Site Manager in good time to allow it to be reviewed before site operations commence.  In this instance, method statements will be provided for the following activities;
















	Work Activity:
	Method Statement to be provided by:

	Ground Remediation 
	Remediation Contractor 

	Earth works 
	Ground-worker 

	Excavations 
	Ground-worker

	Temporary Ground Shoring 
	Shoring Contractor / Ground worker 

	Permanent Driven Piles
	Piling Contractor

	Drainage (Inc Diversions) 
	Ground-worker

	SIPs Panel erection
	SIP’s Contractor

	Brick & Block work 
	Brick laying Contractor 

	Steel frame erection 
	Steel Frame Contractor 

	Scaffold 
	Contractor 

	Tarmac 
	Contractor 

	Flat roof 
	EDPM Contractor 

	Windows & Doors 
	Contractor 

	Dry lining 
	SIPs Contractor 

	Electrical 
	Contractor 

	MVHR
	Contractor

	Mechanical 
	Contractor 

	Fencing 
	Contractor 

	Landscaping 
	Contractor 

	Decoration 
	Contractor 

	Flooring 
	Contractor 

	Green Wall erection 
	Green Services contractor

	Solar PV erection
	PV Contractor

	Rainwater Harvesting
	Contractor



All personnel identified as exposed to the identified risks will receive information and training, to allow them to carry out their work safely. Records of this will be kept by the employer (e.g. method statement and risk assessment sign-off sections).
Where reference is made to existing procedures, arrangements and systems of work, they will be available on site for reference.
[bookmark: _Toc39000537]Site Rules

The site rules are displayed on the “Site Rules” poster in the site office. These will be 
adhered to at all times.  Additional site specific rules will include the following:

· Site parking and access
· Rules for site visitors
· Use of mobile phones
· Restricted areas of the site
· Rules associated with site hazards, e.g. restrictions of use for highly flammable substances or hot works on sites, etc.

All personnel will also be informed of the site rules during their site induction training.  
Hard copies of the site rules will be displayed on site for reference.  If deemed 
necessary, arrangements will be made for translation of site rules for foreign workers.
	
[bookmark: _Toc39000538]Fire Safety

· We will prepare a fire risk assessment of the construction work and implement fire safety policies, procedures and records to demonstrate compliance with our duties under the Construction (Design and Management) Regulations 2015 [Regulations 29-32] and the Fire Safety Order 2005.
· Hot works will be avoided where possible through selection of alternative materials or work methods.
· We acknowledge that there is a high risk of fire on construction sites during the construction period.  During the design stage we will ensure that a site specific risk assessment is carried out to determine the suitability of the use of timber SIPs for the project (in accordance with the guidance). 
· Once the suitability of the design of the steel frame has been confirmed, we will prepare a specific fire risk assessment for the construction site.  The primary purpose of the site fire risk assessment is to address fire safety management, means of escape, means of warning of fire, firefighting equipment, structural fire precautions (including compartmentation) for the construction site work. The findings from the risk assessment will be the basis for the development of the site, fire management plan, which will be appended to the Construction Phase Plan. 
· The construction works will be planned and programmed to allow early installation of the fire compartmentation. This will include early installation of fire barriers, enclosure of compartmentation walls and protective means of escape, and enclosing ground floor and other areas at risk of arson.
· Where possible we will install the permanent means of fire detection / fighting facilities to provide protection during the construction phase. Alternatively, we will install a temporary site system.
· We will discuss with the steel framed designer / manufacturer possible design measures to minimise the risk of fire, for example fire retardant treatment of the timber.  
· We will ensure our site security measures take account of the fire risks associated with arson.
· The above measures will be incorporated into our site fire management plan.

Emergency Procedures

· The Emergency Procedures Poster that includes key contact telephone numbers will be displayed in site office. 

· Fire Action Notices will be displayed at locations on the site as determined by the fire risk assessment.  As part of the site induction all personnel will be informed of the means of raising the alarm if a fire occurs.

[bookmark: _Toc39000539]Action in event of a fire

In the event of a fire, the Site Manager or his deputy will follow the following procedure:  

Raise the alarm (Using existing call points or temporary audible warning device – as identified by the Site Fire Risk Assessment)

· Ensure that all personnel have evacuated the site and made their way to the designated Assembly Point and carry out a roll call.

· Establish the precise location and extent of the fire

· If necessary, call the Fire and Rescue Service, giving the following information as appropriate:  

· Full address of site (including any access restrictions)
· Extent of fire
· If any persons are not accounted for
· Presence and location of hazardous, flammable or explosive substances

· The person who telephones the emergency services will remain on the line until the operator specifically instructs that all necessary information has been received and understood

· Ensure that a responsible person is designated to meet the Fire and Rescue Service on their arrival in order to direct them to the emergency and provide any other requested information, such as the location of service isolation points and last known location of any missing persons

· Contact head office  

Based on the findings of the fire risk assessment trained staff may attempt to fight the fire with the fire extinguishers provided, when;

· It is deemed safe to do so;
· Such action would contain or extinguish the fire;
· It is likely to have a direct and immediate effect in protecting life.

As determine by the fire risk assessment we will supply fire extinguishers that will be located at suitable fire points on the site.  All operatives will receive information about the nature, location and use of extinguishers during their site induction training.  

Fire and emergency procedures will be monitored and reviewed as the contract progresses.  As determined by the fire risk assessment the emergency procedure will be tested by evacuation exercises.  Records of these will be retained.  

[bookmark: _Toc39000540]Management of Temporary Works

We will ensure that all hazards and risks associated with temporary works on this site are controlled by the implement of our company Temporary Works procedures.

· A Temporary Works Co-ordinator and Supervisor will be appointed for this project. 
· Temporary works on this project are likely to include Scaffolding; Propping; Edge Protection; Formwork (Shuttering); Trench Supports; Temporary Roofs; Hoarding; Signage; Temporary Pedestrian access; Loading Bays; Safety Netting; Tower Crane Bases; Piling Rig Bases; Hoists; Cofferdams; etc.  Refer to Temporary Works Register for full details.
· Details of Temporary Works Designers will be forwarded to the Principal Designer upon their appointment.
[bookmark: _Toc39000541]Protection of occupied or neighbouring areas

· Consideration will be given to this during the planning and management of the works, to minimise risk to health of safety on these non-construction personnel, in addition to minimising disruption and nuisance.  The Site Manager will liaise with the Client / occupiers on a regular basis.
· The site traffic management plan will take account of arrangements for co-ordinating any conflict with traffic movements to the occupied area of the site and neighbouring residential and university properties. Temporary access to the University parking facility will be required for the duration of the project, the entrance/exit will be approximately 100 metres South of the site entrance.  
[bookmark: _Toc39000542]Waste

· Waste will be collected and placed into suitable receptacles.  There is limited space for delivery and siting of skips, so where possible, waste material will be removed off site on a daily basis.
· The Site Manager will ensure regular collections of waste materials.  Licensed waste carriers will be used as required.  Waste collections will be planned in line with our traffic management arrangements and be timed to minimise disruption and risk to non construction personnel.

[bookmark: _Toc39000543]Traffic Management & Deliveries

· Access to the construction site will be made via Union Street, Suitable vehicles will be selected to take account of the access route.  Banksmen will be used to oversee the movement of construction vehicles into and out of the site.
· Before commencement of operations, signs will be erected which warn all non-construction personnel of the works in progress.  The signage will make clear segregation of construction traffic routes and members of the public.
· Temporary barriers and / or a watchman will be used as appropriate to ensure that non-construction personnel do not access any hazardous areas which may be temporarily created outside the site or in occupied / shared areas (for example, during loading and unloading at roadside).
· As soon as the construction phase commences, the Site Manager will prepare a traffic management plan.  The plan will also detail the provision of segregated pedestrian route to and within the site. 
· Roads will, so far as is reasonably practicable, be kept free from mud and cleaned on a regular basis, if deemed necessary.
· Deliveries of materials and plant for use on site will be controlled according to the nature of items to be delivered, the type of delivery vehicle and the location of the proposed works (provide details).  All suppliers/sub contractors will be advised of the access and delivery arrangements and restrictions.
· All deliveries and construction related traffic movements will be planned to avoid the busy or high risk periods.  The Client will be consulted to avoid any overlap with their deliveries, etc.
· Banksmen and watchmen will be employed at all times where loading or unloading of vehicles takes place in areas near those with public or shared access.


Specific measures for works involving particular risks

(Including those required by CDM 2015 Regulation 12(2) / Schedule)


[bookmark: _Toc39000544]Excavation work and groundworks, etc.

· Together with our groundworks sub contractor, we are familiar with all aspects of excavation work connected with this project.  Full information regarding the ground contamination will be obtained prior to commencement the works on site.  A specific risk assessment and method statement will be prepared for work with ground contaminants.
· The Site Manager will ensure that suitable and sufficient risk assessments (and method statements where appropriate) have been carried out for all work activities.  Existing generic assessments will be utilised, modified as appropriate for the particular activity in question.
· Support of excavations will be managed in line with our site temporary works procedure.  We will inform the Principal Designer of any temporary works designers we appoint.





[bookmark: _Toc39000545]Falling from height

· Work at height is unavoidable. The Site Manager will supervise all this work and will determine, in consultation with contractors, which methods of access and protection from falls are to be used for each operation.  The following equipment will be provided as necessary:-

	(a)	Timber pole ladders
	(b)	Step-ladders
	(c)	Tube & fitting scaffolding 
	(d)	Mobile tower scaffolding 
(c) Podium platforms
(d) Crash decks
(e) Purpose built access equipment (such as pulpit steps)
(f) Air bags
(g) Safety Netting
(h) Mobile Elevated Work Platforms (MEWPs)

· Access for work at height will be planned taking into account the hierarchy of access as set out within TG20:13 i.e. with preference to use of staircases over ladder access.
· Stepladders will be used only as intended (i.e. not as pole ladders) and be Class 1. Class 3 (domestic) ladders will not be brought to site.  Ladders and stepladders will only be used for access or as a workplace after the Site Manager has assessed the matter and determined that no suitable alternative is available.  Where their use is necessary, it will only be permitted if three points of contact can be maintained (i.e. at least one hand will be holding the ladder at all times).
· All ladders will be correctly secured or footed when in use and extend at least 1.05m past their landing point.  Ladders will be set at an angle of 75 degrees (1 in 4).
· All tube & fitting scaffolding will be erected and maintained by our recognised contractors in accordance with SG4:15, and will conform to BS EN 12811-1, TG20:13 and the Work at Height Regulations 2005.
· Where there is a risk of falls of materials on to the occupied areas / public routes below, the scaffolding will incorporate suitable measures to prevent falls of materials, etc. below, e.g. fan hoarding, close boarding, debris netting, etc.
· Where required, a lifting point for a hoist will be designed in by the scaffolding contractors.  
· The Site Manager (or scaffolding contractor) will carry out all statutory inspections (weekly or more frequently) of the independent scaffolding as required by the Regulations.  Records of inspections will be retained in the scaffold inspection register on site.
· Additionally, the scaffolding will be inspected on a daily basis by the Site Manager to ensure that the structures are safe for use.  Any concerns will be notified to the scaffolders and addressed prior to anyone being permitted onto the scaffolding.
· Podium platforms may be used by contractors, provided they are, at all times, founded on a firm, level surface and be fully boarded to at least 600mm at all times. Overhang will be less than 150mm. Purpose designed systems, such as the Safestand Access System can be used. 
· Mobile scaffold towers will be used in preference to podium platforms and / or ladders wherever reasonably practicable.
· Suitable edge protection (permanent or temporary) will be provided at all levels to prevent risk of falls from height.
· All roofing works will be undertaken in accordance with the guidance contained in the HSE publication, HSG33 - 'Health and Safety in Roofwork'.

[bookmark: _Toc39000546]Assembly or dismantling heavy prefabricated components

· Risk Assessments and Method Statement will be prepared by our sub contractors prior to the commencement of steelwork erection operations.
· Steel frame sections will be delivered to site via Lorries and unloaded by competent persons, either directly to the erection area or stored in a safe and orderly manner.  Fall prevention measures for the unloading of Lorries and erection of the Steel Frame will be detailed in the sub-contractor’s risk assessment and method statement.

Dismantling or demolition of prefabricated components

· Suitable mechanical aids will be selected in the delivering and installed of these heavy components.  
· A lifting plan will be prepared and the steel frame contractor, a competent appointed person.   A contract lift will be arranged for the following lifting operations: 

To be advised after contract begins

1. Main Scaffold erecting 
	2. Steel Frame erecting 
3. Roof Tiling  
4. Plasterboard & Internal fit out 
5. Waste disposal 

· Localised lifting operations (e.g. using lorry mounted cranes for unloading) can be carried out without a plan. However, all crane operators must be competent, trained and certificated.
· The Temporary Works Co-ordinator will be consulted to discuss the TW requirements for these activities, e.g. ensuring adequate capacity of ground for the loading of lifting equipment, use of temporary supports during the erection or dismantling process, etc.

[bookmark: _Toc39000547]Manual Handling

· Wherever reasonably practicable, manual handling will be avoided and mechanical methods used.
· Any remaining manual handling operations will be assessed by the Site Manager.  A lifting practice poster will be displayed in the site accommodation.
· Full procedures for assessing manual handling tasks and ensuring safety during manual handling operations are contained within company safety documentation. These will be adhered to at all times by the employees and sub contractors.
· As, where reasonably practicable, mechanical devices will be used for handling heavy loads, the Site Manager will ensure that sufficient mechanical equipment is available at all times (e.g. trolleys, wheel barrows, genie lifts, etc.), with particular consideration of movement of materials from delivery to point of use.  

[bookmark: _Toc39000548]Noise & Vibration

· Noise will be controlled by using modern machinery, maintained in good condition and where practicable fitted with sound deadening devices. Personal protective equipment will also be used where necessary.
· Should any work be necessary which may involve exposure by operatives to levels of vibration above the daily exposure limit or action values (ELV or EAV), a separate and specific assessment will be carried out. Work activities which could result in site operatives high levels of vibration include use of power tools, scabbling, etc.
· Persons will not be exposed to levels of vibration above the daily maximum recommended level of 2.5m/s/s. Work methods will be planned and equipment selected to minimise risks associated with hand and whole body vibration.  

[bookmark: _Toc39000549]Other Significant Health and Safety Risks

· Where these are identified as the project progresses, risk assessments will be carried out to determine all necessary control measures.
[bookmark: _Toc39000550]Construction Methods

· Cabat Consultancy Ltd, as the main contractor will comply with all construction methods established within the method statement and will maintain compliance with all parties involved with the project.
[bookmark: _Toc39000551]The Health and Safety File

[bookmark: _Toc39000552]Layout & Format

· As agreed with the Client and Principal Designer document.  Whilst a Principal Designer is appointed, it is the Principal Designer’s duty to prepare and update the Health and Safety File.  

· The content of the Health and Safety File will follow the requirements of Appendix 4 of CDM 2015.


[bookmark: _Toc39000553]ADDITIONAL SITE SAFETY DOCUMENTATION

The Site Manager will ensure that the following documentation is available on site;  

A.	Site Induction Schedule

B.	Site Rules

C.	Risk Assessment and Method Statement Schedule
	Job Specific Risk Assessments and Method Statements
Job Specific Risk Assessments and Method Statements – Sub Contractors 

D.	Traffic Management Plan & Site Drawings

E.	Safety Inspection Reports
	Site Manager’s Weekly Checklists
	
F.	Records of Statutory Inspections 
(Scaffold/Excavation/Lifting & Plant/Electrical/Other)

G.	Blank / Completed Toolbox Talks

H.	Training Certificates / Plant Operators Licences
	Project Specific Training Record Form	

I.	Services Information 
	Drawings and correspondence from utility and other service providers

J.	PPE Issue Register

K.	Accident & Incident Report Form

L.	Insurances 

M.	Pre-Construction Information 

N.	Site Fire Risk Assessment & Management Plan

O.	Temporary Works Register



End of document
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