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Ms =          kg  ( to be found prior to test )
Musf =  38 kg /wheel   
Musr = 42 kg/wheel  	
CG height for sprung mass  =  0.299m (verify  accuracy when determining weight transfer by wheel deflection )	
Wheelbase 	2.351m	
Rolling radius 0.275 m ( Typical figure – each tyre type  will be slightly different )
Front spring rate 350 lb/in
Rear spring rate 170 lb/in
Ratio of  wheel  travel to spring travel  1.97
Ratio of  wheel  travel to pot travel   1.622
Rear Suspension leverage of wheel to spring = 1.0
Velocity  ratio of damper wheel to pot = 1.0	
	 

