Task 1: Network Test
 submission


S-DC connectivity 

Ipconfig/all
[image: A screenshot of a computer screen

Description automatically generated]








Ping 192.168.1.10
[image: A computer screen shot of a black screen

Description automatically generated]

Ping 192.168.2.1
[image: A screenshot of a computer

Description automatically generated]

L-DC connectivity

Ip address
[image: A screenshot of a computer

Description automatically generated]

Ping 192.168.1.10
[image: A screenshot of a computer

Description automatically generated]


Ping 192.168.1.1
[image: A screenshot of a computer

Description automatically generated]
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dministrator: Command Prompt

DHCP Server . 10.0.2.2
DHCPV6 IAID . L. ... ... : 101187623

DHCPV6 Client DUID. . . . . . . . : 00-81-@0-01-30-66-31-06-08-00-27-1A-80-9D
DNS Servers .

127.0.6.1
NetBIOS over Tcpip. . . . . . . . : Enabled

LB thernet adapter Intswa:

Connection-specific DNS Suffix
Description .

Physical Address.

DHCP Enabled. S No

Autoconfiguration Enabled . .t Yes

Link-local IPv6 Address . . . . . : fe89::0d88:200f:446C:b440%13(Preferred)
1Pv4 Address. R 192.168.1.1(Preferred)

Subnet Mask . 255.255.255.6

Default Gateway .

Intel(R) PRO/1066 MT Desktop Adapter #2
: 68-60-27-16-8C-86

DHCPYV6 TATD . . 168296487
DHCPYV6 Client DUID. 06-01-00-01-30-66-31-66-68-60-27-1A-86-9D
DNS Servers . 5 ged

127.0.6.1
NetBIOS over Tcpip. . . . . . . . : Enabled

Ethernet adapter External:

Connection-specific DNS Suffix

Description . Intel(R) PRO/1066 MT Desktop Adapter #3
Physical Address. © .. ... : 08-06-27-4B-BF-AA
DHCP Enabled. . . . S ... N0

Autoconfiguration Enabled . Yes

Link-local IPv6 Address . . . : fe80::9aca:a640:58bd: 6b12%15 (Preferred)
1Pv4 Address. . . . . . . .. ..: 20.0.0.1(Preferred)

Subnet Mask . 255.255.255.252

Default Gateway .
DHCPYV6 TATD . .
DHCPYV6 Client DUID.
DNS Servers .

: 185073703
00-01-00-01-30-66-31-06-08-00-27-1A-80-9D

192.168.1.1
NetBIOS over Tcpip. . . . . . . . : Enabled

Jc: \Users\Administrators,
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nmand Prompt

iC: \Users\Administrator>ping 192.168.1.10

Pinging 192.168.1.16 with 32 bytes of data:
Reply from 192.168.1.16: bytes=32 time<ims
Reply from 192.168.1.16: bytes=32 time<ims
Reply from 192.168.1.16: bytes=32 time<ims
Reply from 192.168.1.16: bytes-32 time=ims

ping statistics for 192.168.1.16:
Packets: Sent = 4, Received = 4, Lost = © (8% loss),
approxinate round trip times in milli-seconds:
Minimum = @ms, Maximum = ims, Average = 6ms

Jc: \Users\Administrators,
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C:\Users\Administrator>ping 192.168.2.1

Pinging 192.168.2.1 with 32 bytes of data:
Reply from 192.168.2.1: bytes=32 time<ims TTL=64
Reply from 192.168.2.1: bytes=32 time<ims
Reply from 192.168.2.1: bytes=32 time<ims
[Reply from 192.168.2.1: bytes-32 time<ims TTL-64

ping statistics for 192.168.2.
Packets: Sent = 4, Received = 4, Lost = @ (8% loss),
pproximate round trip times in milli-seconds:
Mininum = ems, Maximum = Oms, Average = oms

Jc: \Users\Administrator>
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