Jake Bevan	Managing Health, Safety and Welfare in Construction	Assignment 2
Managing Health and Safety in a project
	Activity to be Assessed

	Construction of the Block & Block Walls

	Persons undertaking or affected by the activity

	

	
	■
	Employees
	■
	Contractor
	
	Public
	
	Service User
	

	

	
	
	Other …………………………………………………………………………………………….

	Identified Hazards and Associated Risks
	Likelihood
	Severity
	Risk Level

	1
	Skin hazards on site.
	5
	4
	20

	2
	Any sharp edges.
	5
	3
	15

	3
	Heavy loads and or with poor posture
	3
	3
	9

	4
	Exposed to Wet Mortar (contains calcium oxide) 
	4
	3
	12

	Existing Control Measures / Additional Control Measures Required

	1
	Using work methods that increases the distance between the worker and the substance such as longer handled tools.

	2
	Use PPE. This includes gloves, gauntlets and armbands. All PPE must be suitable for the circumstances, considering the different type of employees who will use it.

	3
	Instruct to lift these loads with the correct posture, only handle loads less than your body weight these methods are used to prevent back injuries and any other functions.

	4
	People using said wet mortar to be instructed to wear gloves, and long sleeves if possible, this is to avoid skin burns.

	Reassessment of Activity Hazards

	Name - Jake Bevan
Position - Site Manager
	Site Name – SA1 Domestic Building

	Date of Completion – June 18th

	Reviews
	Key
	

	Review Date: May 7th
	Likelihood
	Severity
	Severity of Injury
	5
	5Y
	10R
	15
	20
	25

	Reviewed by Jake Bevan
	1   very     unlikely
2   unlikely
3   likely
4   very likely
5   certainty
	1   nuisance
2   minor
3   medical treatment
4   major
5   fatal
	
	4
	4
	8
	12
	16
	20

	Review Date: May 14th
	
	
	
	3
	3
	6G
	9
	12
	15

	Reviewed by Jake Bevan
	
	
	
	2
	2
	4
	6Y
	8
	10Y

	Review Date: May 21st
	
	
	
	1
	1
	2
	3
	4
	5G

	Reviewed by Jake Bevan
	
	
	
	0
	1
	2
	3
	4
	5

	Review Date: May 28th
	
	
	
	Likelihood of Injury

	Reviewed by Jake Bevan
	
	
	
	Low Risk
	
	Medium Risk
	
	High Risk


As part 3 of the assignment I will produce risk assessments for activities related to the single, two storey detached domestic building.








	Activity to be Assessed

	Construction of the Carpentry Roof Trusses

	Persons undertaking or affected by the activity

	

	
	■
	Employees
	■
	Contractor
	
	Public
	
	Service User
	

	

	
	
	Other …………………………………………………………………………………………….

	Identified Hazards and Associated Risks
	Likelihood
	Severity
	Risk Level

	1
	Access
	3
	5
	15

	2
	Any sharp edges.
	5
	3
	15

	3
	Physical injury falling off the roof
	2
	4
	8

	4
	Equipment
	3
	5
	15

	Existing Control Measures / Additional Control Measures Required

	1
	Ensure workers can get safely to and from where they work at height with an accessible ladder always available.

	2
	Use PPE. This includes gloves, gauntlets and armbands. All PPE must be suitable for the circumstances, considering the different type of employees who will use it.

	3
	Provide safety nets and barriers around said roof structure to prevent any falls on site.

	4
	Having frequent toolbox talks on equipment, what makes it function, how to tell when to replace it and how to use it in a safe manner.

	Reassessment of Activity Hazards 

	Name - Jake Bevan
Position - Site Manager
	Site Name – SA1 Domestic Building

	Date of Completion – June 25th

	Reviews
	Key
	

	Review Date: May 8th
	Likelihood
	Severity
	Severity of Injury
	5
	5Y
	10R
	15
	20
	25

	Reviewed by Jake Bevan
	1   very     unlikely
2   unlikely
3   likely
4   very likely
5   certainty
	1   nuisance
2   minor
3   medical treatment
4   major
5   fatal
	
	4
	4
	8
	12
	16
	20

	Review Date: May 15th
	
	
	
	3
	3
	6G
	9
	12
	15

	Reviewed by Jake Bevan
	
	
	
	2
	2
	4
	6Y
	8
	10Y

	Review Date: May 22nd
	
	
	
	1
	1
	2
	3
	4
	5G

	Reviewed by Jake Bevan
	
	
	
	0
	1
	2
	3
	4
	5

	Review Date: May 29th
	
	
	
	Likelihood of Injury

	Reviewed by Jake Bevan
	
	
	
	Low Risk
	
	Medium Risk
	
	High Risk









	Activity to be Assessed

	Construction of the Plinths

	Persons undertaking or affected by the activity

	

	
	■
	Employees
	■
	Contractor
	
	Public
	
	Service User
	

	

	
	
	Other …………………………………………………………………………………………….

	Identified Hazards and Associated Risks
	Likelihood
	Severity
	Risk Level

	1
	Trips, slips and falls
	4
	5
	20

	2
	Site activity and conditions
	4
	4
	16

	3
	Heavy loads and or with poor posture
	3
	3
	9

	4
	Any sharp edges.
	5
	3
	15

	Existing Control Measures / Additional Control Measures Required

	1
	Make sure of clear walkways, appropriate lighting and a clear non slippery floor and if said floor is likely to make someone slip the put a slippery floor sign down in that area.

	2
	Make sure work is carried out on a stable and level enough ground if possible, put signs in place of where other works activities are being carried out.

	3
	Instruct to lift these loads with the correct posture, only handle loads less than your body weight these methods are used to prevent back injuries and any other functions.

	4
	Use PPE. This includes gloves, gauntlets and armbands. All PPE must be suitable for the circumstances, considering the different type of employees who will use it.

	Reassessment of Activity Hazards 

	Name - Jake Bevan
Position - Site Manager
	Site Name – SA1 Domestic Building

	Date of Completion – July 1st

	Reviews
	Key
	

	Review Date: June 8th
	Likelihood
	Severity
	Severity of Injury
	5
	5Y
	10R
	15
	20
	25

	Reviewed by Jake Bevan
	1   very     unlikely
2   unlikely
3   likely
4   very likely
5   certainty
	1   nuisance
2   minor
3   medical treatment
4   major
5   fatal
	
	4
	4
	8
	12
	16
	20

	Review Date: June 15th
	
	
	
	3
	3
	6G
	9
	12
	15

	Reviewed by Jake Bevan
	
	
	
	2
	2
	4
	6Y
	8
	10Y

	Review Date: June 22nd
	
	
	
	1
	1
	2
	3
	4
	5G

	Reviewed by Jake Bevan
	
	
	
	0
	1
	2
	3
	4
	5

	Review Date: June 29th
	
	
	
	Likelihood of Injury

	Reviewed by Jake Bevan
	
	
	
	Low Risk
	
	Medium Risk
	
	High Risk
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Jake Bevan   Managing Health, Safety and  Welfare in Construction   Assignment 2   Managing Health and Safety in a project   As part  3   of the assignment I will produce  risk   assessments   for activities related to the  single, two storey detached domestic building.              

Activity to be Assessed  

Construction of  the  Block   & Block Walls  

Persons undertaking or affected by the activity  

 

 ¦  Employees  ¦  Contractor   Public   Service User   

 

  Other …………………………………………………………………………………………….  

Identified Hazards and Associated Risks  Likelihood  Severity  Risk Level  

1  Skin hazards on site .  5  4  20  

2  Any sharp edges .  5  3  15  

3  Heavy loads and or with poor posture  3  3  9  

4  Exposed to Wet Mortar (co ntains  calcium oxide)    4  3  12  

Existing Control Measures / Additional Control Measures Required  

1  U sing work methods that increases the distance between the worker and the substance such as  longer handled tools .  

2  U se  PPE .  This include s   gloves, gauntlets and   armbands. All PPE must be suitable for the   circumstances,  considering the  different type of   employees who will use it .  

3  Instruct to lift  these loads with the correct posture, only handle loads less than your body  weight these  methods are used to prevent back injuries and any other functions.  

4  People using said wet mortar to be instructed to wear gloves, and long sleeves if possible, this is to avoid  skin burns.  

Reassessment of Activity Hazards  

Name  -   Jake Bevan   Position  -   Site Manager  Site Name  –   SA1 Domestic  Building    Date of Completion   –   June  18th  

Reviews  Key   

Review Date:  May 7th  Likelihood  Severity  Severity of  Injury  5  5Y  10R  15  20  25  

Reviewed  by   Jake Bevan  1   very       unlikely   2    unlikely   3   likely   4   very likely   5   certainty  1   nuisance   2   minor   3   medical  treatment   4   major   5   fatal   4  4  8  12  16  20  

Review  Date: May   14th   3  3  6G  9  12  15  

Reviewed  by   Jake Bevan   2  2  4  6Y  8  10Y  

Review  Date: May   21st   1  1  2  3  4  5G  

Reviewed  by   Jake Bevan   0  1  2  3  4  5  

Review  Date: May   28th    Likelihood of Injury  

Reviewed  by   Jake Bevan    Low Risk   Medium Risk   High Risk  

