We are interested in:
· The cumulative Vd (Σ), and
· The cumulative Hd (Σ)
c
Vd = difference in height between points


Drop / vertical distance Vd
Horizontal distance Hd


For plotting, we need:
· Hd (cumulative) and the Reduced Levels
· Reduce levels = Bench Mark value (100) - drop [for each surveying point ]
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