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	Personnel Involved:

Operatives.
	PPE: All personnel will wear hard hats, safety footwear and high visibility jackets/vest.
	SUPERVISOR IN CHARGE: 
C Keys

	Operation: Concrete placing 

	ACTIVITY AND HAZARDS

(Identify hazards associated with task)
	INITIAL RISK RATING
	CONTROL MEASURES

(Identify measures to eliminate, reduce or control hazard or those that are requested by others)
	RESIDUAL RISK RATING
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	Reversing of concrete lorries.

Use of concrete pump.

Use of excavator and concrete skip.

Entanglement in moving parts of plant.

Collision of mobile plant.
Prolonged exposure to noisy plant.
Working on reinforcement.
Eye injuries due to concrete splashes.
Contact dermatitis 

Concrete burns.

Noise and vibration from plant. 
Environmental pollution.


	(
(
(
(

	(
(
(
(
(
(
(
(

	
	All moving and reversing plant/ vehicles will be under the control of Banks man.
Plant and traffic management schemes should be formalised, regardless of the size of pours.
Concrete should not be poured too quickly

Impervious safety boots and gloves to be worn when working with wet concrete.

Long sleeve shirts and full-length trousers to be worn by all operatives

All concrete splashes to be washed off skin immediately with warm clean water.

All concrete splashes to be washed of off clothing as soon as practicable.

Safety glasses will be worn to protect eyes from concrete splashes.

Pump operator to hold current CPCS or equivalent certificate.

Pump to be in good working order

Concrete skip to be kept clean and in good working condition.
Plant and all lifting equipment to be inspected (chains etc) to have current thorough examination certificate, which must have been carried out with in the past 12 months.

Check to make sure that all plant is in good condition and well maintained.

Plant and traffic management schemes should be formalised, regardless of the size of pours.

Ensure guards are fitted to all parts of machinery where applicable.
No loose clothing to be worn around the operating plant.

High visibility vest to be worn correctly and done up.

Long hair to be tied back to ensure safety of operatives working around plant. 

All moving and reversing plant/ vehicles will be under the control of Banks man.

All moving and reversing plant/ vehicles will be under the control of Banks man.

Plant and traffic management schemes should be formalised, regardless of the size of pours.

Ear protection will be worn when working with or near to noisy plant.
Where operatives have to walk on reinforcement due care must be taken and if practicable scaffold boards or similar used.

Safety glasses will be worn to protect eyes from concrete splashes.
In the case of concrete splashing and entering the eye immediately wash out with eye wash or copious amounts of water and obtain further help if necessary.
All concrete splashes to be washed off skin immediately with warm clean water.
Always wear appropriate gloves and skin covering for the task that you are carrying out.

Apply barrier cream prior to starting to work and also after you have finished the job in hand.

Impervious safety boots and gloves to be worn when working with wet concrete.

Long sleeve shirts and full-length trousers to be worn by all operatives

All concrete splashes to be washed off skin immediately with warm clean water.

All concrete splashes to be washed of off clothing as soon as practicable.

Safety glasses will be worn to protect eyes from concrete splashes.
Replace PPE When necessary. 
Ear protection will be worn when working with or near to noisy plant.

All vibrating tools will be reduced vibration, kept in good condition and fit for purpose.
Concrete mixer to be washed out in designated areas only to avoid pollution to water courses.

The accumulation of concrete spillage should be prevented.
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All persons undertaking activities indicated on this risk assessment form must be made fully aware of its contents
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