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® PT Activity:

1. Configure Host Names on each device (Based on the Labels in the Topology)

2. Assign Encrypted Privileged Password hello to all the Routers

3. Configure console connection: Password is hello123 for all the Routers, Set logging synchronous.
4. Configure Virtual Terminal line: (Permit 2 lines), Password is hello456 for all the Routers, Allow only telnet and local login
5. Disable DNS lookup in all the routers

6. Encrypt all the passwords in all the routers

7. Set motd banner: & unauthorized access prohibited & for all the Routers. Note, use special character & to begin and end the
banner as stated in the red, underlined text.

Part - B Route Configuration

8. Configure all devices with IP address as shown in the Addressing table and network topology. Configure both IPv4 and IPv6
address. For IPv6 address, configure appropriate Link Local address manually

9.0n R1, configure IPv4 and IPV6 static route to R2 and R3 networks

10. On R2, configure 1Pv4 and IPV6 static route to R3 networks

11. On R3, configure 1Pv4 and IPV6 static router to R2 networks.

12. Configure 1Pv4 and IPv6 default static route on R2 and R3 to reach Lot and Lo2 network using next-hop ip address.
13. Set the bandwidth on serial links to 512kbps.

14. Set the clock rate on DCE to be 9600

15. In R1, create a domain with name acca.com, username: userl and encrypted password: password. Set privelge as 10.





