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Addressing Table: IPv4 and IPv6 Address

[Time Elapsea: 02.01:57
O Top O Dock

Device | Tnterface TPvd Address TPv6 Address TPv6 Link Local
R1 Gi0/00.10 [ 192.168.10.124 | 2001:dbS:acad:10:1/64 | £e80::1
Gi0/0020 [ 192.16820.124 | 2001:dbS:acad:20:1/64 | £e80::1
Gi0/0/1 19216830124 | 2001:dbSacad:30:1/64 | fe80=1
5¢0/1/0 10.13.0.130 2001:dbS:cafe:13:1/64 | £e80:1
Se0/1/1 10.12.0.130 2001:dbS:cafe:12:1/64 | £e80::1
R2 Gi0/0/0 19216840124 | 2001:dbSacad:40:1/64 | fe80:2
S0/t 1023.0230 2001:dbS:cafe23:2/64 | £e80:2
5010 10.12.0230 2001:dbS:cafe:12:2/64 | £e80:2
R3 Gi0/0/0 209.165.200.124 | 2001:dbS:cafe:09:1/64 | fe80:3
50120 10.13.0230 2001:dbS:cafe:13:2/64 | £e80:3
S02/1 1023.0.130 2001:dbS:cafe23:1/64 | £e80:3
ISP Gi0/0/0 209165200224 | 2001:dbS:cafe:09-2/64 | fe80:4
Pal NIC DHCP DHCP DHCP
Pa2 NIC DHCP DHCP DHCP
Pa3 NIC DHCP DHCP DHCP
Pbl NIC DHCP DHCP DHCP
Serl NIC 19216840524 | 2001:dbS:acad:40:5/64 | N/A
VLAN Table
Devi VLAN Vian TP Address Default
evice Number Interface Gateway
10 (One) ., 20 0 197.168.102724 | 192.168.10.1
Sal
(Two)
10 (One), 20 20 197168202724 | 192.168.20.1
Sa2
(Two)
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=) Excluded Addresses
o 192.168.10.1 182.168.10.10 Correct
o 192.168.20.1 192.166.20.10 Correct
| 192.168.40.1 192.166.40.10 Correct
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5 PooiTen
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X Subnetmask Incorrect
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o DiSserverP Correct
o Name Correct
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X Attempts. Incorrect
X Duraton Incorrect
X Enabled Incorrect
X period Incorrect
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£ Process D 15
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5 Networks.
X Routed Incorrect
v Routel Correct
v Route2 Correct
v Route3 Correct
o Routes Correct
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£ Ports
£ GigabiEthemet0/0/0.10
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"o/ DHCP client enable Correct 1
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