
R1(config)#exit
R1#
*Aug 19 11:33:37.864: %SYS-5-CONFIG_I: Configured from console by console
R1#en
R1#conf term
Enter configuration commands, one per line.  End with CNTL/Z.
R1(config)#enable secret class
R1(config)#exit
R1#
*Aug 19 11:48:17.337: %SYS-5-CONFIG_I: Configured from console by console
R1#conf term#
            ^
% Invalid input detected at '^' marker.

R1#conf term
Enter configuration commands, one per line.  End with CNTL/Z.
R1(config)#serviceb password-encryption
                  ^
% Invalid input detected at '^' marker.

R1(config)#service password-encryption
R1(config)#excit
              ^
% Invalid input detected at '^' marker.

R1(config)#exit
R1#
*Aug 19 11:50:14.672: %SYS-5-CONFIG_I: Configured from console by console
R1#conf term
Enter configuration commands, one per line.  End with CNTL/Z.
R1(config)#exit
R1#
*Aug 19 11:51:20.848: %SYS-5-CONFIG_I: Configured from console by console
R1#conf term
Enter configuration commands, one per line.  End with CNTL/Z.
R1(config)#password cisco
                    ^
% Invalid input detected at '^' marker.

R1(config)#password-cisco
                   ^
% Invalid input detected at '^' marker.

R1(config)#password cisco
                    ^
% Invalid input detected at '^' marker.

R1(config)#password Cisco
                    ^
% Invalid input detected at '^' marker.

R1(config)#line vty 0 15
R1(config-line)#password cisco
R1(config-line)#log in
                    ^
% Invalid input detected at '^' marker.

R1(config-line)#login
R1(config-line)#exit
R1(config)#service password-encryption
R1(config)#exit
R1#
*Aug 19 12:00:03.172: %SYS-5-CONFIG_I: Configured from console by consoleconf
Configuring from terminal, memory, or network [terminal]?
Enter configuration commands, one per line.  End with CNTL/Z.
R1(config)#banner moto"Unauthorized acces is prohibited"
Enter TEXT message.  End with the character 'm'.
Unauthorized acces is prohibited

exit
R1#exit
m
R1(config)#int G0/0/0
R1(config-if)#ip add
R1(config-if)#ip address 172.16.0.1 255.255.255.0
R1(config-if)#exit
R1(config)#exit
R1#c
*Aug 19 12:06:51.193: %SYS-5-CONFIG_I: Configured from console by consoleonf term
Enter configuration commands, one per line.  End with CNTL/Z.
R1(config)#int G0/0/1
R1(config-if)#ip add
% Incomplete command.

R1(config-if)#ip add
R1(config-if)#ip address 172.16.11.1 255.255.255.0
R1(config-if)#exit
R1(config)#exit
R1#
*Aug 19 12:11:30.095: %SYS-5-CONFIG_I: Configured from console by console
R1#show run
Building configuration...


Current configuration : 3585 bytes
!
! Last configuration change at 12:11:30 UTC Mon Aug 19 2019
!
version 16.9
service timestamps debug datetime msec
service timestamps log datetime msec
service password-encryption
platform qfp utilization monitor load 80
no platform punt-keepalive disable-kernel-core
!
hostname R1
!
boot-start-marker
boot-end-marker
!
!
enable secret 5 $1$dJ2f$URKZGJZAQ/9aRnv5SoI9I.
!
no aaa new-model
!
no ip domain lookup
ip admission watch-list expiry-time 0
!
!
!
!
!
!
!
!
!
!
subscriber templating
multilink bundle-name authenticated
!
!
!
crypto pki trustpoint TP-self-signed-1227001095
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-1227001095
 revocation-check none
 rsakeypair TP-self-signed-1227001095
!
!
crypto pki certificate chain TP-self-signed-1227001095
 certificate self-signed 01
  30820330 30820218 A0030201 02020101 300D0609 2A864886 F70D0101 05050030
  31312F30 2D060355 04031326 494F532D 53656C66 2D536967 6E65642D 43657274
  69666963 6174652D 31323237 30303130 3935301E 170D3139 30383139 31313036
  32305A17 0D333030 31303130 30303030 305A3031 312F302D 06035504 03132649
  4F532D53 656C662D 5369676E 65642D43 65727469 66696361 74652D31 32323730
  30313039 35308201 22300D06 092A8648 86F70D01 01010500 0382010F 00308201
  0A028201 0100E13F 41E28DC3 6E79C42A 120AB5AB FB074C04 20030A04 A39FC2D9
  97C62680 5561B973 070F8C54 B3350E79 DB58AB9D 08DEEE1C 76311E33 8CAF7A7A
  94C17316 B376D1B4 C2D603F7 EDA8045B F871C027 223E24F5 851AECF2 AA07F922
  4AD9AD00 9CE179B3 374BF276 65727C0C 90E16252 B23FE634 CFF6F622 2D780D2E
  44FFED7B D7FFC5BC DDED4BC4 5A64DAE1 65FD5DF0 4EB881B9 259DB368 1952052A
  35EC2DB0 19A90AA0 09E67EE6 CC924AA3 514F3A67 05425409 BD0365B3 1A16BCD2
  528576A6 4FB004F6 A6CEB7B4 EA92E213 2D36EE29 54E81BD0 56EABD14 6F35F5A0
  5D6EE5CE F1B0887F 5285DB58 3A4B0D87 913AB0EC 4B7E4834 03F53B92 721131E3
  CA037077 E82B0203 010001A3 53305130 0F060355 1D130101 FF040530 030101FF
  301F0603 551D2304 18301680 1418BCC6 B436D988 C2EB51AE A92ADB93 4F907704
  79301D06 03551D0E 04160414 18BCC6B4 36D988C2 EB51AEA9 2ADB934F 90770479
  300D0609 2A864886 F70D0101 05050003 82010100 5F8ABD28 22CF544E 57F16D05
  25D83362 AAF47DC0 3B9EBFF1 449F9A7D F5C1B955 289FE24B 88B1A1FD A32D694A
  81D0D6C7 8CF76426 3DDFECFB 921E0B8B 92D632A3 F8ABA556 843F5EA3 DDAEE5FD
  50DBCCB6 3D788DDC 5A3FEE52 DC69281B 842F9265 57A73C6B FD8ED87D 787CAA0E
  ACBE27B2 73B681AA E091BB3D E784636E ED342AF3 DEEE7683 283499BB 716CE6F9
  2B66724D D6ECD8EB 662FB4E7 33E96AA0 B1B29343 C2978C2D 530652D3 F3C618B6
  0EAB7095 36323DB9 BA6C8648 A199F2A0 E7F49613 0D578431 E1D64A97 E9B5D553
  662D76C0 EAB393C9 3D4515C4 6626EBEA 81A00C33 081F5713 6E07FF9A 6DF1D98A
  63CBDB27 5DA609AA 0474F009 5C80F311 ABA68FFF
        quit
!
license udi pid ISR4221/K9 sn FGL224190DV
no license smart enable
diagnostic bootup level minimal
!
spanning-tree extend system-id
!
!
!
!
redundancy
 mode none
!
!
!
!
!
!
!
!
interface GigabitEthernet0/0/0
 ip address 172.16.0.1 255.255.255.0
 shutdown
 negotiation auto
!
interface GigabitEthernet0/0/1
 ip address 172.16.11.1 255.255.255.0
 shutdown
 negotiation auto
!
interface Serial0/1/0
 no ip address
 shutdown
!
interface Serial0/1/1
 no ip address
 shutdown
!
ip forward-protocol nd
ip http server
ip http authentication local
ip http secure-server
!
!
!
!
!
!
control-plane
!
banner motd ^Coto"Unauthorized acces is prohibited"
Unauthorized acces is prohibited

exit
R1#exit
^C
!
line con 0
 transport input none
 stopbits 1
line vty 0 4
 password 7 14141B180F0B
 login
line vty 5 15
 password 7 14141B180F0B
 login
!
!
!
!
!
!
end

R1#conf term
Enter configuration commands, one per line.  End with CNTL/Z.
R1(config)#no shut down
                   ^
% Invalid input detected at '^' marker.

R1(config)#no shutdown
% Incomplete command.

R1(config)#no sh
% Incomplete command.

R1(config)#interface vlan1
                      ^
% Invalid input detected at '^' marker.

R1(config)#interface vlan
                      ^
% Invalid input detected at '^' marker.

R1(config)#interface fast ethernet 0/0
                      ^
% Invalid input detected at '^' marker.

R1(config)#show run
             ^
% Invalid input detected at '^' marker.

R1(config)#exit
R1#
*Aug 19 12:18:08.068: %SYS-5-CONFIG_I: Configured from console by consoleno shutdown
      ^
% Invalid input detected at '^' marker.

R1#no shutdown
      ^
% Invalid input detected at '^' marker.

R1#en
R1#conf term
Enter configuration commands, one per line.  End with CNTL/Z.
R1(config)#show run
             ^
% Invalid input detected at '^' marker.

R1(config)#exit
R1#show
*Aug 19 12:18:50.195: %SYS-5-CONFIG_I: Configured from console by consolerun
Building configuration...


Current configuration : 3585 bytes
!
! Last configuration change at 12:18:50 UTC Mon Aug 19 2019
!
version 16.9
service timestamps debug datetime msec
service timestamps log datetime msec
service password-encryption
platform qfp utilization monitor load 80
no platform punt-keepalive disable-kernel-core
!
hostname R1
!
boot-start-marker
boot-end-marker
!
!
enable secret 5 $1$dJ2f$URKZGJZAQ/9aRnv5SoI9I.
!
no aaa new-model
!
no ip domain lookup
 --More—
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% Unknown command or computer name, or unable to find computer address
S1>
S1>
S1>conf term
      ^
% Invalid input detected at '^' marker.

S1>configure term
      ^
% Invalid input detected at '^' marker.

S1>conf term
      ^
% Invalid input detected at '^' marker.

S1>conf
Translating "conf"...domain server (255.255.255.255)
% Unknown command or computer name, or unable to find computer address
S1>
S1>
S1>conf ter
      ^
% Invalid input detected at '^' marker.

S1>en
S1#conf term
Enter configuration commands, one per line.  End with CNTL/Z.
S1(config)#no ip domain-lookup
S1(config)#

































S1 con0 is now available





Press RETURN to get started.









*Mar  1 00:59:52.790: %SYS-5-CONFIG_I: Configured from console by console
S1>conf term
      ^
% Invalid input detected at '^' marker.

S1>conf term
      ^
% Invalid input detected at '^' marker.

S1>en
S1#conf term
Enter configuration commands, one per line.  End with CNTL/Z.
S1(config)#no ip domain-lookup
S1(config)#exit
S1#
*Mar  1 01:37:32.412: %SYS-5-CONFIG_I: Configured from console by console
S1#conf term
Enter configuration commands, one per line.  End with CNTL/Z.
S1(config)#banner motd
% Incomplete command.

S1(config)#banner motd"message-of-the-day"
S1(config)#exit
S1#
*Mar  1 01:39:06.440: %SYS-5-CONFIG_I: Configured from console by console
S1#conf term
Enter configuration commands, one per line.  End with CNTL/Z.
S1(config)#interface vlan1
S1(config-if)#ip address 172.16.11.10 255.255.255.0
S1(config-if)#no shutdown
S1(config-if)#exit
S1(config)#exit
S1#
*Mar  1 01:42:45.375: %SYS-5-CONFIG_I: Configured from console by consoleinterface
Translating "interface"
% Unknown command or computer name, or unable to find computer address
S1#
S1#conf term
Enter configuration commands, one per line.  End with CNTL/Z.
S1(config)#conf default gateway
               ^
% Invalid input detected at '^' marker.

S1(config)#default gateway
                    ^
% Invalid input detected at '^' marker.

S1(config)#interface ip
                     ^
% Invalid input detected at '^' marker.

S1(config)#interface
% Incomplete command.

S1(config)#interface VLAN!
                         ^
% Invalid input detected at '^' marker.

S1(config)#interface VLAN1
S1(config-if)#default gateway 172.16.11.1
                      ^
% Invalid input detected at '^' marker.

S1(config-if)#default
% Incomplete command.

S1(config-if)#default 172.16.11.1
                      ^
% Invalid input detected at '^' marker.

S1(config-if)#exit
S1(config)#interface fast ethernet 0/0
                      ^
% Invalid input detected at '^' marker.

S1(config)#line vty0 15
                   ^
% Invalid input detected at '^' marker.

S1(config)#line vty 0 15
S1(config-line)#exit
S1(config)#exit
S1#
*Mar  1 01:48:10.928: %SYS-5-CONFIG_I: Configured from console by consoleshow run
Building configuration...

Current configuration : 1379 bytes
!
! Last configuration change at 01:48:10 UTC Mon Mar 1 1993
!
version 15.2
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname S1
!
boot-start-marker
boot-end-marker
!
!
no aaa new-model
system mtu routing 1500
!
!
!
!

S1#show run
Building configuration...

Current configuration : 1379 bytes
!
! Last configuration change at 01:48:10 UTC Mon Mar 1 1993
!
version 15.2
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname S1
!
boot-start-marker
boot-end-marker
!
!
no aaa new-model
system mtu routing 1500
!
!
!
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Connection-specific DNS Suffix
Description .

Physical Address.

DHCP Enabled. G
Autoconfiguration Enabled .
Link-local TPv6 Address .
1Pv4 Address.

Subnet Mask .

Default Gateway .

DHCPY6 TATD . i

DHCPY6 Client DUID.

DNS Servers .

NetBIOS over Tcpip.
cthernet adapter Ethernet 2:

Connection-specific DNS Suffix
Description .

Physical Address.

DHCP Enabled. G
Autoconfiguration Enabled .
Link-local IPv6 Address .
Autoconfiguration IPv4 Address.
Subnet Mask .

Default Gateway .

DHCPY6 TATD . i

DHCPY6 Client DUID.

DNS Servers .

NetBIOS over Tcpip.

C:\Users\Admin>

VirtualBox Host-Only Ethernet Adapter
©A-00-27-00-00-6C

: No

Yes

Fe80: :5¢42:55b3:dase: F69d%12(Preferred)
: 192.168.56.1(Preferred)

255.255.255.6

: 554303527
00-01-00-01-23-57-53-C6-0C-0D-92-BF-BB-BD
FecB:0:0:FFFF::1%1
FecB:0:0:FFFF::2%1
Fecd:0;
: Enabled

Npcap Loopback Adapter
02-00-4C-4F-4F-50

: Yes

Yes

Fego: :884F:34dC: FFF1:269%13 (Preferred)
: 169.254.166.217 (Preferred)

255.255.0.0
: 402784332
00-01-00-01-23-57-53-C6-0C-0D-92-BF-BB-BD
FecB:0:0:FFFF::1%1
FecB:0:0:FFFF::2%1
Fecd:0;

: Enabled
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Users\Admin>ip conf
ip’ is not recognized as an internal or external command,

operable program or batch file.

C:\Users\Adninping

Usage: ping [-t] [

-a] [-n count] [-1 size] [-f] [-i TTL] [-v TOS]

[-r count] [-s count] [[-J host-list] | [-k host-list]]
[-w timeout] [-R] [-5 srcaddr] [-c compartment] [-p]

[-41 0

-a
-n count
-1 size
=
B
-v Tos

-r count
-5 count

-j host-list
-k host-list
-w timeout
R

-5 srcaddr
-c compartment
-p
-4
-6

-6] target_name

Ping the specified host until stopped.

To see statistics and continue - type Control-Break;

To stop - type Control-C.

Resolve addresses to hostnames.

Number of echo requests to send.

Send buffer size.

Set Don't Fragment flag in packet (IPv4-only).

Time To Live.

Type Of Service (IPva-only. This setting has been deprecated
and has no effect on the type of service field in the IP
Header) .

Record route for count hops (IPv4-only).

Timestamp for count hops (IPv4-only).

Loose source route along host-1ist (IPva-only).

Strict source route along host-list (IPva-only).

Timeout in milliseconds to wait for each reply.

Use routing header to test reverse route also (IPv6-only).
Per RFC 5605 the use of this routing header has been
deprecated. Some systems may drop echo requests if

this header is used.

Source address to use.

Routing compartment identifier.

Ping a Hyper-V Network Virtualization provider address.
Force using IPva.

Force using IPV6.

:\Users\Adnin>ipconfig/all




image3.jpeg
Ping a Hyper-V Network Virtualization provider address.
Force using IPva.
Force using IPV6.

\Users\Admin>ipconfig/all

tindous IP Configuration

Host Name . LN264-NETLAB
Primary Dns Suffix’
Node Type . Hybrid

Ip Routing Enabled.
WINS Proxy Enabled.

hernet adapter Ethernet:

Media State .
Connection-specific DNS Suffix’
Description .

Physical Address.

DHCP Enabled.
Autoconfiguration Enabled .

: Media disconnected
campus. local

Intel(R) Ethernet Connection (2) I219-LM
C-9D-92-BF-B9-88

No

: Yes

hernet adapter Npcap Loopback Adapter

Connection-specific DNS Suffix
Description .

Physical Address.

DHCP Enabled.
Autoconfiguration Enabled .
Link-local IPv6 Address .
1Pv4 Address.

Subnet Mask .

Default Gateway .

DHCPV6 TATD .

DHCPV6 Client DUID.

DNS Servers .

Npcap Loopback Adapter
62-60-4C-4F-4F-56

::192F:2CF8:4bb3:94de%10(Preferred)
192.168.1.16(Preferred)

255.255.255.6

192.168.6.1

260893196
0-61-60-61-23-56-48-37-0C-9D-92-BF -89-88

NetBIOS over Tcpip.

hernet adapter Ethernet 2:
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Host Name .
Primary Dns Suffix
Node Type . . .

Ip Routing Enabled.
WINS Proxy Enabled.

Ethernet adapter Ethernet:

Media State .
Connection-specific DNS Suffix’
Description .

Physical Address.

DHCP Enabled. .
Autoconfiguration Enabled .

LN264-NETLAB

Media disconnected
campus . local

: Intel(R) Ethernet Connection (2) 1219-LM

C-9D-92-BF-B9-88
No

: Yes

Ethernet adapter Npcap Loopback Adapter:

Connection-specific DNS Suffix
Description .

Physical Address.

DHCP Enabled. .
Autoconfiguration Enabled .
Link-local IPv6 Address .
1Pv4 Address.

Subnet Mask .

Default Gateway .

DHCPV6 TATD . .

DHCPV6 Client DUID.

DNS Servers .

NetBIOS over Tcpip.
Ethernet adapter Ethernet 2:

Connection-specific DNS Suffix
Description .

Physical Address.

DHCP Enabled. .
Autoconfiguration Enabled .
Link-local IPv6 Address .

Autoconfiguration IPv4 Address.

Npcap Loopback Adapter

: ©2-00-4C-4F-4F-50

No
Yes

: feB6::192f:2Cf8:4bb3:94de%10(Preferred)

192.168.1.16(Preferred)
255.255.255.6

: 192.168.0.1

469893196
90-01-00-61-23-56-43-37-0C-0D-92-BF-89-88

Npcap Loopback Adapter

: ©2-00-4C-4F-4F-50

Yes
ves

: feB6::61e6:5db0: eb35:3603%16(Preferred)

160.254.54.147 (Preferred)

Activate Windc
Go to Settings to ac




image5.jpeg
EAGoMS 18 CONTIgUration

Host Name . : LN265-NETLAB
Primary Dns Suffix’

Node Type . . . Hybrid

Ip Routing Enabled. No

WINS Proxy Enabled. No

thernet adapter Ethernet:

Media State .
Connection-specific DNS Suffix’
Description .

Physical Address.

DHCP Enabled.
Autoconfiguration Enabled .

Media disconnected
campus . local

Intel(R) Ethernet Connection (2) 1219-M
8C-9D-92-BF-B8-BD

No

Yes

thernet adapter Npcap Loopback Adapter

Connection-specific DNS Suffix
Description .
Physical Address.

Npcap Loopback Adapter
02-00-4C-4F-4F-50

DHCP Enabled. . No
Autoconfiguration Enabled . ves
Link-local IPv6 Address . Fego: :a08:9384:3ab6: F7C6%14(Preferred)

1Pv4 Address.
Subnet Mask .
Default Gateway .

192.168.1.16(Preferred)
255.255.255.6

DHCPV6 IAID . . 486670412
DHCPV6 Client DUID. 00-61-00-01-23-57-53-C6-0C-0D-92-BF-BB-BD.
DNS Servers . Feco.

feco
feco
NetBIOS over Tcpip. . . . . . . . : Enabled

thernet adapter VirtualBox Host-Only Network:

Connection-specific DNS Suffix
Description .
Physical Address.

VirtualBox Host-Only Ethernet Adapter
0A-00-27-00-00-6C

DHCP Enabled. . No
Autoconfiguration Enabled . ves
Y iak 15051 16 Addieks . £e80: :5c42:55b3 : das





