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	MANAGING HEALTH AND SAFTEY WELFARE AND RISK IN CONSTRUCTION
	THOMAS BRETT





2. Method Statement for Excavations and Groundworks
	Project/Contract
	A single two storey detached domestic building with loft room on a green field site

	Principal Contractor
	Major Property Developer

	Site Address
	Green Field Site 

	Project Start Date 
	06/05/2019

	Expected Duration
	10 weeks

	Projected completion Date
	10/07/2019



The following document has been produced to provide a safe system of work and must be adhered to at all times. Any deviation from the following method statement and this should be raised with the manager or safety representative for the action to be authorised. 
Main Hazards
1. Injury from Slip trips and falls
2. Injury from Manual Handling
3. Falling from Height (Excavations)
4. Injury from machines and vehicle movement
5. Injury from strikes to underground utilities
6. Injury to public due to unsecured work areas
Preventative Measures taken
1. You must ensure the area of works is safe for yourself and other contractors
2. You must be trained and competent to carry out the task
3. You must not work alone
4. You must not over exert yourself by lifting beyond your capabilities
5. Only permitted people are to enter the site, visitors and other members must be signed in to the site and accompanied by a competent person. 
6. All persons on site must have appropriate PPE including visitors. 
Mandatory PPE on site
1. Hard Hats
2. Hi Visibility Clothing
3. Safety Glasses
4. Safety Boots
5. Gloves
6. Eye Protection
7. Dust Masks where appropriate
Welfare
The Principal Contractor will be responsible for adequate welfare. This is to include washing facilities, toilets, drying and refreshment facilities. 
First Aid
It is the responsibility of the employer to provide adequate first aid on site. There will be trained first aid on site with first aid equipment readily available. This will be confirmed in the onsite induction. 
Scope of Works
To clear site and excavate ready for footings to be constructed. All excavation work will be carried out in accordance in the detailed specifications. If there are specifications incomplete or not provided then this will be referred back to the Principal Contractor for more information. 

Site Access and Egress
It is the responsibility of the Principal Contractor to provide safe access and egress to the site, staff will ensure the access and egress is maintained for themselves and other contractors in the area they are working by maintaining high levels of housekeeping of the works area. 
Manual Handling
All staff to attend a toolbox talk on Manual Handling and sign attendance document before any works to be undertaken on site. The toolbox talk will highlight the potential dangers of manual handling and staff will not lift beyond their capabilities. Where possible mechanical lifting will be used. It is the responsibility of the manager of the site to identify and control potentially dangerous manual handling situations as they occur on site day to day. 
Vehicle Control
Vehicle control on site is the responsibility of the Principal Contractor. Vehicle movements on site will be controlled in such a manner to not cause unnecessary risks to workers or visitors to the site. All staff will follow the rules and guidelines while driving on site. 
Excavations and Trenches
No unauthorised vehicles or machines will be allowed near any excavations or trenches to minimise any risks of collapse, all trenches/excavations will have barriers erected around the perimeters. Dependant on the ground conditions and depths of excavation then decision to be made by site manager if trench supports are required. 
Working at Height
All staff to receive a toolbox talk on Working at Height and be made aware of the dangers and consequences of falling from height. All tasks with risk at working at height will be properly planned, organised and supervised by trained and competent staff. The site manager will have risk assessments in place prior to works and will put in place the correct contingencies to reduce or eliminate risks to health and safety. 
Plant/Machinery and Tools
1. 5t Excavator
2. Cat and Genny (Calibrated)
3. Spray Paint (marking excavations and utilities)
4. Barriers/Heras Fencing
5. Shovel and other required hand tools
6. 2” Submersible Pump in case of flooding
Excavator
· Only competent operators to use plant. Pre-use checks to be undertaken prior to operating any plant.
· Only certificated excavators of sufficient capability are to be used for lifting activities. 
· All personnel to be positioned in a position of safety during lifting activities. No personnel to be stood in close proximity or under suspended loads 
· Banks-man to control all access to site during excavation
· Excavation Banks-man shall be used to assist the excavator operator during the excavation process. Excavation Banks-man to maintain a safe distance from the machine and within the line of sight, having regard to the Plant Exclusion Zone. Banks-man to be aware of swing radius of arm and counter balance of machines
· If anything unusually is seen by banks-man work to stop until proven safe
· Only personnel involved in work to be around excavation.
· Before Banks-man approaches the machine, the machine operator shall lower arm/bucket and switch off machine, before giving authorisation to approach machine.
Method of Works Procedure
1. Attend site office and complete site induction and toolbox talks as per Principal Contractor requirements.
2. Put on Personal Protective Equipment
3. Take tools and plant to work area. 
4. Set up work area and exclusions zones. 
5. Mark area for excavations if not already done so, following Principal Contractor plans. If there are no plans or areas marked for excavations then refer back to sire manager for drawings. 
6. There should be no other utilities due to the location of the site but a Cat and Genny sweep to be undertaken before any excavation work. 
7. When Excavations are marked and site has been investigated for other utilities then excavations can begin. 
8. All pre checks to excavator must be completed. 
9. Work can begin only when there is a banksman present. 
10. Excavation work to follow safe systems of work. Strip excavations to a depth of 1m.
11. Spoil to be placed in a safe place adequately away from edge of excavations and within barrier safe zone. 
12. Ground structure to be continually assessed and if there are any concerns in the stability then this is to be raised to the site manager and trench supports to be considered.  
13. Work area housekeeping to be maintained to a good standard throughout works. 
14. No tools or machinery to be left unattended.
15. All tools and equipment to be removed from site at end of each day. 
16. Area to be left clean and tidy at the end of each day.
17. Report to Site office and sign out at end of each day. (Nwfacilities.com, 2019)

3. Method Statements for Substructure and Wall    
	Project/Contract
	A single two storey detached domestic building with loft room on a green field site

	Principal Contractor
	Major Property Developer

	Site Address
	Green Field Site 

	Project Start Date 
	06/05/2019

	Expected Duration
	10 weeks

	Projected completion Date
	10/07/2019



The following document has been produced to provide a safe system of work and must be adhered to at all times. Any deviation from the following method statement and this should be raised with the manager or safety representative for the action to be authorised. 
Main Hazards
1. Injury from Slip trips and falls
2. Injury from Manual Handling
3. Falling from Height (Excavations and scaffolding)
4. Injury from machines and vehicle movement
5. Injury to public due to unsecured work areas
6. Severe burns contact dermatitis from exposure to dust and wet concrete
Preventative Measures taken
1. You must ensure the area of works is safe for yourself and other contractors
2. You must be trained and competent to carry out the task
3. You must not work alone
4. You must not over exert yourself by lifting beyond your capabilities
5. Only permitted people are to enter the site, visitors and other members must be signed in to the site and accompanied by a competent person. 
6. All persons on site must have appropriate PPE including visitors. 
Mandatory PPE on site
1. Hard Hats
2. Hi Visibility Clothing
3. Safety Glasses
4. Safety Boots
5. Gloves
6. Eye Protection
7. Dust Masks

Welfare
The Principal Contractor will be responsible for adequate welfare. This is to include washing facilities, toilets, drying and refreshment facilities. 
First Aid
It is the responsibility of the employer to provide adequate first aid on site. There will be trained first aid on site with first aid equipment readily available. This will be confirmed in the onsite induction. 
Scope of Works
Pouring of concrete to construct foundations as per Principal Contractor’s dimensions. Construct sub structure and walls up to the eaves.
Site Access and Egress
It is the responsibility of the Principal Contractor to provide safe access and egress to the site, staff will ensure the access and egress is maintained for themselves and other contractors in the area they are working by maintaining high levels of housekeeping of the works area. 
Manual Handling
All staff to attend a toolbox talk on Manual Handling and sign attendance document before any works to be undertaken on site. The toolbox talk will highlight the potential dangers of manual handling and staff will not lift beyond their capabilities. Where possible mechanical lifting will be used. It is the responsibility of the manager of the site to identify and control potentially dangerous manual handling situations as they occur on site day to day. 
Vehicle Control
Vehicle control on site is the responsibility of the Principal Contractor. Vehicle movements on site will be controlled in such a manner to not cause unnecessary risks to workers or visitors to the site. All staff will follow the rules and guidelines while driving on site. 
Excavations and Trenches
No unauthorised vehicles or machines will be allowed near any excavations or trenches to minimise any risks of collapse, all trenches/excavations will have barriers erected around the perimeters. Dependant on the ground conditions and depths of excavation then decision to be made by site manager if trench supports are required. 
Working at Height
All staff to receive a toolbox talk on Working at Height and be made aware of the dangers and consequences of falling from height. All tasks with risk at working at height will be properly planned, organised and supervised by trained and competent staff. The site manager will have risk assessments in place prior to works and will put in place the correct contingencies to reduce or eliminate risks to health and safety. 

Scaffolding
Scaffold will be provided by an approved contractor. The hand rail will be extended to a minimum of 1m above the working area. The site manager will confirm a handover certificate is received from the appointed contractor prior to access being granted to the scaffolding. Access to scaffolding will be via ladders and they will be removed at the end of shift to stop unauthorised access. 
Lifting Operations
Lifting operations in relation to the movement of heavy materials will be completed in accordance to the Lifting Operations and Lifting Equipment Regulations 1998 (LOLER). Lifting on site will be planned by the Principal Contractor. The works will be undertaken by competent persons and will be fit for purpose. 
Plant/Machinery and Tools
1. Mobile Mixer Unit
2. Level
3. Trowel
4. Shovel
5. Wheelbarrow
6. Mobile crane for lifting of Heavy Materials
Method of Works Procedure
1. Attend site office and complete site induction and toolbox talks as per Principal Contractor requirements.
2. Put on Personal Protective Equipment.
3. Take tools and plant to work area. 
4. Set up work area and exclusions zones. 
5. Pre Equipment checks to be undertaken.
6. Pouring of concrete via ready mix loaded lorry. 
7. Spread concrete and check level.
8. Position blocks near work area using a crane/lifting equipment.
9. Collect mortar from mobile mixing units.
10. Carry out substructure blockwork as per Principal Contractor Drawings – Cavity Wall.
11. Damp proof membrane, cavity wall ties, cavity trays and insulation etc to be installed as per drawings.
12. Builds walls then arrange scaffold.
13. Set out doorways and windows as per drawings.
14. All blockwork to be level and plumb.
15. As the height of the blockwork increases the scaffold will need to be increased.
16. Floors will need to be installed before blockwork being taken up to first floor/second floor.
17. Work area housekeeping to be maintained to a good standard throughout works. 
18. No tools or machinery to be left unattended.
19. All tools and equipment to be removed from site at end of each day. 
20. Area to be left clean and tidy at the end of each day.
21. Report to Site office and sign out at end of each day. (Nwfacilities.com, 2019)




4. Method Statements for Roof Structure    
	Project/Contract
	A single two storey detached domestic building with loft room on a green field site

	Principal Contractor
	Major Property Developer

	Site Address
	Green Field Site 

	Project Start Date 
	06/05/2019

	Expected Duration
	10 weeks

	Projected completion Date
	10/07/2019



The following document has been produced to provide a safe system of work and must be adhered to at all times. Any deviation from the following method statement and this should be raised with the manager or safety representative for the action to be authorised. 
Main Hazards
1. Injury from Slip trips and falls
2. Injury from Manual Handling
3. Falling from Height (Excavations and scaffolding)
4. Injury from machines and vehicle movement
5. Injury to public due to unsecured work areas
Preventative Measures taken
1. You must ensure the area of works is safe for yourself and other contractors
2. You must be trained and competent to carry out the task
3. You must not work alone
4. You must not over exert yourself by lifting beyond your capabilities
5. Only permitted people are to enter the site, visitors and other members must be signed in to the site and accompanied by a competent person. 
6. All persons on site must have appropriate PPE including visitors. 
Mandatory PPE on site
1. Hard Hats
2. Hi Visibility Clothing
3. Safety Glasses
4. Safety Boots
5. Gloves
6. Eye Protection
7. Dust Masks (where applicable)
Welfare
The Principal Contractor will be responsible for adequate welfare. This is to include washing facilities, toilets, drying and refreshment facilities. 


First Aid
It is the responsibility of the employer to provide adequate first aid on site. There will be trained first aid on site with first aid equipment readily available. This will be confirmed in the onsite induction. 
Scope of Works
Construction and weathering of the roof. 
Site Access and Egress
It is the responsibility of the Principal Contractor to provide safe access and egress to the site, staff will ensure the access and egress is maintained for themselves and other contractors in the area they are working by maintaining high levels of housekeeping of the works area. 
Manual Handling
All staff to attend a toolbox talk on Manual Handling and sign attendance document before any works to be undertaken on site. The toolbox talk will highlight the potential dangers of manual handling and staff will not lift beyond their capabilities. Where possible mechanical lifting will be used. It is the responsibility of the manager of the site to identify and control potentially dangerous manual handling situations as they occur on site day to day. 
Vehicle Control
Vehicle control on site is the responsibility of the Principal Contractor. Vehicle movements on site will be controlled in such a manner to not cause unnecessary risks to workers or visitors to the site. All staff will follow the rules and guidelines while driving on site. 
Excavations and Trenches
No unauthorised vehicles or machines will be allowed near any excavations or trenches to minimise any risks of collapse, all trenches/excavations will have barriers erected around the perimeters. Dependant on the ground conditions and depths of excavation then decision to be made by site manager if trench supports are required. 
Working at Height
All staff to receive a toolbox talk on Working at Height and be made aware of the dangers and consequences of falling from height. All tasks with risk at working at height will be properly planned, organised and supervised by trained and competent staff. The site manager will have risk assessments in place prior to works and will put in place the correct contingencies to reduce or eliminate risks to health and safety. 
Scaffolding
Scaffold will be provided by an approved contractor. The hand rail will be extended to a minimum of 1m above the working area. The site manager will confirm a handover certificate is received from the appointed contractor prior to access being granted to the scaffolding. Access to scaffolding will be via ladders and they will be removed at the end of shift to stop unauthorised access. 
Lifting Operations
Lifting operations in relation to the movement of heavy materials will be completed in accordance to the Lifting Operations and Lifting Equipment Regulations 1998 (LOLER). Lifting on site will be planned by the Principal Contractor. The works will be undertaken by competent persons and will be fit for purpose. 
Plant/Machinery and Tools
1. Mobile crane for lifting of Roof Trusses
2. Hiab 
3. Nail Gun
4. Roofing Hammer and other associated hand tools. 
Method of Works Procedure
1. Attend site office and complete site induction and toolbox talks as per Principal Contractor requirements.
2. Put on Personal Protective Equipment.
3. Take tools and plant to work area. 
4. Set up work area and exclusions zones. 
5. Pre Equipment checks to be undertaken.
6. Scaffold will be erected around the perimeter by the competent persons.
7. Fall protection measures to be installed. (crash deck)
8. Trusses will be delivered by lorry and safely delivered and stored in a vertical position. This will be assisted by a banksman.
9. The crane will be positioned assisted by a banksman ready for lifting.
10. The crane appointed person will lift each trusses individually as per the lift plan.
11. The first truss will be put into position and secured to the wall plate. 
12. The remaining trusses will be lifted into position and temporarily braced back to the first truss.
13. Bracing will then be fixed to the ceiling ties, trusses and struts.
14. Trusses will then need to be fixed to the gables and walls.
15. Felt will be set up in the work area ready for installation.
16. Felt will then be laid systematically in direction of the roof gradient and suitable side and end flaps to be secured. 
17. Roof battens (2x1) will be lifted to the roof by the crane and the operatives will install battens at suitable spacing ready for tiling.
18. Roof Slates will then be transported to the working area and fixed to the roof battens.
19. Ridge tiles will be cemented into place.
20. Work area housekeeping to be maintained to a good standard throughout works. 
21. No tools or machinery to be left unattended.
22. All tools and equipment to be removed from site at end of each day. 
23. Area to be left clean and tidy at the end of each day. Any surplus materials to be removed and disposed of correctly. 
24. Report to Site office and sign out at end of each day. (Alc-prd-media-01.azureedge.net, 2019)



5.Risk Assessment for Excavations/Groundworks
Control Matrix
	Likelihood of Event Occuring
	Severity of Consequences

	
	Very Low Severity
	Low Severity
	Medium Severity
	High Severity
	Very High Severity

	Very High
	
	
	
	
	

	High
	
	
	
	
	

	Medium
	
	
	
	
	

	Low
	
	
	
	
	

	Very Low
	
	
	
	
	



	Risk Categories
	Low Risk
	Medium Risk
	High Risk
	Very High Risk

	
	
	
	
	



(www.researchgate.net, 2019)


	Hazard
Personnel
Effected
	Risk Before Controls
	Control Measures
	Risk After Controls
	Responsible Person

	Manual Handling
	Employees
Subcontractors
	High
	Operatives to be competent and trained in manual handling techniques.
Use mechanical lifting techniques where possible.
	Low
	Operatives


	People and Plant Interface - Vehicles
	Employees
Subcontractors
Visitors
MOPs

	Very High

	Minimise reversing on sites where possible
When reversing, use of a competent and trained banksman shall be used. Banksman to wear high visibility clothing and be visible to driver at all times. If driver loses site of Banksman, then driver must stop.
Banksman to control unauthorised access during reversing activities.
Driver to use driving aids and mirrors when reversing. 

	Low
	Vehicle Driver
Operatives

	Underground Utilities
	Employees
Subcontractors
MOPs

	Very High
	Up to date colour utility drawings to be available on site. Operatives to review surrounding area for signs of underground utilities. CAT & Genny to be used in all modes. All traced utilities to be marked up. CAT & Genny to be used as excavation progresses (minimum of 300mm). Safe digging techniques to be used. Treat all utilities as Live. 
	Low
	Operatives





	Use of Plant/Equipment
	Employees
Subcontractors
Visitors
Members of Public
	Very High


	Only Competent and trained persons to use plant/equipment. Pre-use checks to be undertaken before use. All defect plant/equipment to be quarantined.
	Low
	Operatives


	Dust
	Employees
Subcontractors
Visitors
Members of Public 
	High


	Approved Respiratory equipment to be used when risk of dust particles being on site. 
Minimal use of brushes and other tasks that may cause dust particles to become airborne. 
	Low
	Operatives

	Unsecured work areas (Pedestrians)
	Employees
Subcontractors
Visitors
Members of Public 
	Very High


	All work areas and excavations to be secured using approved NRSWA barriers to prevent unauthorised access. Footpath/road plates to installed as per manufacturer’s instructions. 
	Low
	Operatives

	Slips, Trips and Falls (STF)
	Employees
Subcontractors
Visitors
Members of Public 
	High



	High standard of housekeeping to be maintained.
Unauthorised access to work area to be prevented.
Good Lighting will be provided to keep areas well lit. 
	Low
	Operatives


	Hand Arm Vibrations
	Employees
Subcontractors
	Medium



	Low vibratory equipment to be provided. Equipment along with all attachments to be Fit for Purpose. Operatives to be aware of the vibration levels. Gloves to be worn. Task is to be rotated between working party. HAVs exposure to be recorded on SSRA.
	Low
	Operatives


	Noise Induced Hearing Loss
	Employees
Subcontractors
	Medium



	Plant/Equipment to be Fit for Purpose. Operatives to be aware of the noise levels. Ear protection to be worn. Task is to be rotated between working party. Plant/Equipment to be switched off when not in use
	Low
	Operatives





6.Risk Assessment for Construction of Ground Floor

	Hazard
Personnel
Effected
	Risk Before Controls
	Control Measures
	Risk After Controls
	Responsible Person

	Manual Handling
	Employees
Subcontractors
	High
	Operatives to be competent and trained in manual handling techniques.
Use mechanical lifting techniques where possible.
	Low
	Operatives


	Plant – Mixer (if required)
	Employees
Subcontractors

	Very High

	Only operatives trained and deemed competent to use the plant for mixing concrete. 
All appropriate PPE to be work by operatives. 
No additional operatives - not required to be in works area of plant allowed. 
	Low
	Operatives

	Concrete Burns from contact with concrete
	Employees
Subcontractors


	Very High
	Only operatives trained and competent to be in vicinity when concrete being poured.
Correct PPE to be worn.  
Safeguarding zone and signage to be used when pouring complete.
First Aid kits and correct protocol to be followed if operative comes into contact with concrete. 
Anyone not involved with this task to not be in vicinity of works. 
Coshh Assessments to be made available to operatives. 
	Low
	Operatives


	Concrete contact with eyes
	Employees
Subcontractors

	Very High
	Only operatives trained and competent to be in vicinity when concrete being poured.
Correct PPE to be worn.  
Safeguarding zone and signage to be used when pouring complete.
First Aid kits and correct protocol to be followed if operative comes into contact with concrete. 
Anyone not involved with this task to not be in vicinity of works. 
Coshh Assessments to be made available to operatives.
	Low 
	Operatives

	Plant – Vehicles (Concrete mixer lorry)
	Employees
Subcontractors
Visitors
Members of Public
	Very High
	Minimise reversing on sites where possible
When reversing, use of a competent and trained banksman shall be used. Banksman to wear high visibility clothing and be visible to driver at all times. If driver loses site of Banksman, then driver must stop.
Banksman to control unauthorised access during reversing activities.
Driver to use driving aids and mirrors when reversing.
Anyone not involved in task to be removed from area of works.  

	Low
	Operatives
Vehicle/Plant driver

	Slips, Trips and Falls (STF)
	Employees
Subcontractors

	High
	High standard of housekeeping to be maintained.
Unauthorised access to work area to be prevented.
Good Lighting will be provided to keep areas well lit.
	Low
	Operatives



7.Risk Assessment for Roof Construction
	Hazard
Personnel
Effected
	Risk Before Controls
	Control Measures
	Risk After Controls
	Responsible Person

	Manual Handling
	Employees
Subcontractors
	High
	Operatives to be competent and trained in manual handling techniques.
Use mechanical lifting techniques where possible.
	Low
	Operatives


	Slips trips and Falls
	Employees
Subcontractors

	High

	High standard of housekeeping to be maintained.
Unauthorised access to work area to be prevented.
Good Lighting will be provided to keep areas well lit.
	Low
	Operatives

	Working at Height
	Employees
Subcontractors


	Very High
	Only Operatives adequately trained and deemed competent to use Equipment (scaffolding, etc) shall use it. 
Suitable fall arrest equipment to always be used. 
Safe systems of work to be followed at all times. 
	Low
	Operatives


	Tools/Equipment falling from height
	Employees
Subcontractors
Visitors

	Very High
	Barrier off working area.
Suitable PPE to be worn by all operatives (last form of defence)
No operatives to work below un-necessarily. All operatives to be made aware of work on site. 
Tool-box talk beforehand. 
	Low 
	Operatives

	Scaffolding
	Employees
Subcontractors
Visitors
Members of Public
	Very High
	Weekly check and daily inspection to be carried out by competent person. Ensure Scaffolding tags are in place and in date.

	Low
	Operatives
Vehicle/Plant driver

	Slips, Trips and Falls (STF)
	Employees
Subcontractors

	High
	High standard of housekeeping to be maintained.
Unauthorised access to work area to be prevented.
Good Lighting will be provided to keep areas well lit.
	Low
	Operatives










8. Health & Safety Legislation
The primary piece of legislation which can relate to the project and in fact the primary piece of legislation which covers occupational health and safety in Great Britain is The Health and Safety at Work Act 1974. This produces a whole host of duties on Employers. The employer must protect the welfare, health and safety of all their employees and others on the premises of the employer. “It shall be the duty of every employer to ensure, as far as is reasonably practicable, the health, safety and welfare at work of all his employees.” (Legislation.gov.uk, 2019)
It is down to the employer to have adequate policies and procedures in place to make tasks for the employees as safe as is reasonably practicable. It is then the duty of the employee to follow these policies and procedures. This can relate to everything to do with the business/works. It can cover plant, machinery and their use, information and training for the employees to make sure they are equipped with the tools for the job and arrangements for ensuring safety and absence of risks to health with the use, handling, storage and transport of articles and substances. 
The Health and Safety at Work Act 1974 is the primary piece of legislation all employers follow but there are legislations which refer to the construction industry specifically and also legislation which relates to even more specific tasks. 
Legislation which relates to this project is the Construction (Design and Management) Regulations (CDM Regs) 2015. This legislation was created to govern the way construction projects of all sizes and types are planned. “CDM aims to improve health and safety in the industry by helping you to: sensibly plan the work so the risks involved are managed from start to finish” (Hse.gov.uk, 2019).
The property developer is a “Commercial client” and under CDM they are the duty holder for overseeing the project. “Organisations or individuals for whom a construction project is carried out that is done as part of a business.” (Hse.gov.uk, 2019) The main duties of the commercial client is to make suitable arrangements to manage the project, they are to make sure that appropriate duty holders are appointed to undertake works. They must make sure the relevant information is provided to additional duty holders, sufficient welfare is in place and that the principal designer or principal contractor carry out their duties.
This project is a notifiable project under CDM Regs, “A project is notifiable if the construction work on a construction site is scheduled to (a) last longer than 30 working days and have more than 20 workers working simultaneously at any point in the project or (b) exceed 500 person days.” (Legislation.gov.uk, 2019) then there must be a Principal Contractor or Principal Designer appointed. A notifiable project means that the project needs to be notified to the Health and Safety Executive as soon as is practicable before the construction begins. This must be done in writing.
There are several other legislations which will come under this construction project. 
Manual Handling Operations Regulations 1992 is the regulations defined as “any transporting or supporting of a load (including the lifting, putting down, pushing, pulling, carrying or moving thereof) by hand or bodily force". (Hse.gov.uk, 2019). These regulations set out the clear measures of dealing with risks from manual handling. These are: 
· first : avoid hazardous manual handling operations so far as is reasonably practicable; 
· second : assess any hazardous manual handling operations that cannot be avoided; and 
· third: reduce the risk of injury so far as is reasonably practicable. (Hse.gov.uk, 2019)
Incorrect manual handling is one of the most common causes for injury at work. These musculoskeletal injuries account for over a third of all work place injuries hence the importance of the regulation. 
Another piece of legislation relating to this project would be the Working at Height Regulations 2005. The working at height regulations don’t have a minimum height for it to be classed as working at height, any activity that means a worker is at risk of falling a distance and causing personal injury is classed as working at height. This may be falling from scaffolding or falling from ground level into an excavation. The working at height regulations is the guidance for the control measures that should be in place for these type of activities. “Every employer shall ensure that work at height is properly planned, appropriately supervised; and carried out in a manner which is so far as is reasonably practicable safe.” (Legislation.gov.uk, 2019)
Another that would be relevant on the site would be the Provision and Use of Work Equipment Regulations 1998 (PUWER).  These regulations place responsibility to businesses and organisations who have employees that use work equipment, whether it is owned by them or not. “Work equipment is any machinery, appliance, apparatus, tool or installation for use at work (whether exclusively or not). This includes equipment which employees provide for their own use at work. The scope of work equipment is therefore extremely wide. The use of work equipment is also very widely interpreted and '...means any activity involving work equipment and includes starting, stopping, programming, setting, transporting, repairing, modifying, maintaining, servicing and cleaning.” (Hse.gov.uk, 2019)
PUWER requires that equipment for work be suitable for the job being undertaken, it should be properly maintained, safe for use and in safe condition, people only adequately trained and deemed competent is to use the equipment and that all equipment be used in accordance with the health and safety guidelines that are in place. It is worth noting that some equipment has more specific regulations which should be adhered to in addition to the PUWER Regs. 
Another regulation which is relevant to the construction site is the Personal Protective Equipment at Work Regulations 1992. “Every employer shall ensure that suitable personal protective equipment is provided to his employees who may be exposed to a risk to their health or safety while at work except where and to the extent that such risk has been adequately controlled by other means which are equally or more effective.” (Legislation.gov.uk, 2019) Personal protective equipment is known as the last form of defence when it comes to Health and Safety.
The list of Health and Safety Legislation can go on and on in relation to construction. 
Control of Substances Hazardous to Health Regulations 2002 – this relates to the control of substances and the use of these, Employers need to reduce exposure or remove exposure to substances that can be hazardous to somebodies health. 
In relation to this project the Major property developer would be the Duty holder for the project and thus the duty holder and accountable for legislation. If the property developer was to hire a contractor who then oversees the project on their behalf then they would become the duty holder in this case. 
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