
Username: cisco
Password:
S1>en
Password:
S1#sh run
Building configuration...

Current configuration : 3654 bytes
!
! Last configuration change at 16:58:57 UTC Thu Aug 22 2024
!
version 15.2
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
service password-encryption
!
hostname S1
!
boot-start-marker
boot-end-marker
!
enable password 7 030752180500701E1D
!
username cisco password 7 01100F175804575D72
no aaa new-model
switch 1 provision c1000-24t-4g-l
system mtu routing 1500
!
!
!
shutdown vlan 26
!
!
!
!
!
!
!
!
spanning-tree mode rapid-pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
!
!
!
interface Port-channel1
!
interface GigabitEthernet1/0/1
 switchport access vlan 25
 switchport trunk native vlan 26
 switchport mode trunk
 shutdown
 channel-group 1 mode auto
!
interface GigabitEthernet1/0/2
 switchport access vlan 25
 switchport trunk native vlan 26
 switchport mode trunk
 shutdown
 channel-group 1 mode auto
!
interface GigabitEthernet1/0/3
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/4
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/5
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/6
 switchport access vlan 22
 switchport mode access
 switchport port-security mac-address sticky
!
interface GigabitEthernet1/0/7
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/8
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/9
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/10
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/11
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/12
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/13
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/14
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/15
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/16
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/17
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/18
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/19
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/20
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/21
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/22
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/23
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/24
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/25
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/26
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/27
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/28
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface Vlan1
 no ip address
 shutdown
!
ip http server
ip http secure-server
!
!
!
!
line con 0
 password 7 070C285F4D06485744
line vty 0
 login
 transport input ssh
line vty 1 4
 login
 transport input none
line vty 5 15
 login
 transport input none
!
end

S1#sh ip int br
Interface              IP-Address      OK? Method Status                Protocol
Vlan1                  unassigned      YES unset  administratively down down
GigabitEthernet1/0/1   unassigned      YES unset  administratively down down
GigabitEthernet1/0/2   unassigned      YES unset  administratively down down
GigabitEthernet1/0/3   unassigned      YES unset  administratively down down
GigabitEthernet1/0/4   unassigned      YES unset  administratively down down
GigabitEthernet1/0/5   unassigned      YES unset  administratively down down
GigabitEthernet1/0/6   unassigned      YES unset  up                    up
GigabitEthernet1/0/7   unassigned      YES unset  administratively down down
GigabitEthernet1/0/8   unassigned      YES unset  administratively down down
GigabitEthernet1/0/9   unassigned      YES unset  administratively down down
GigabitEthernet1/0/10  unassigned      YES unset  administratively down down
GigabitEthernet1/0/11  unassigned      YES unset  administratively down down
GigabitEthernet1/0/12  unassigned      YES unset  administratively down down
GigabitEthernet1/0/13  unassigned      YES unset  administratively down down
GigabitEthernet1/0/14  unassigned      YES unset  administratively down down
GigabitEthernet1/0/15  unassigned      YES unset  administratively down down
GigabitEthernet1/0/16  unassigned      YES unset  administratively down down
GigabitEthernet1/0/17  unassigned      YES unset  administratively down down
GigabitEthernet1/0/18  unassigned      YES unset  administratively down down
GigabitEthernet1/0/19  unassigned      YES unset  administratively down down
GigabitEthernet1/0/20  unassigned      YES unset  administratively down down
GigabitEthernet1/0/21  unassigned      YES unset  administratively down down
GigabitEthernet1/0/22  unassigned      YES unset  administratively down down
GigabitEthernet1/0/23  unassigned      YES unset  administratively down down
GigabitEthernet1/0/24  unassigned      YES unset  administratively down down
GigabitEthernet1/0/25  unassigned      YES unset  administratively down down
GigabitEthernet1/0/26  unassigned      YES unset  administratively down down
GigabitEthernet1/0/27  unassigned      YES unset  administratively down down
GigabitEthernet1/0/28  unassigned      YES unset  administratively down down
Port-channel1          unassigned      YES unset  down                  down
S1#sh vlan br

VLAN Name                             Status    Ports
---- -------------------------------- --------- -------------------------------
1    default                          active
7    vlan 7                           active
8    vlan 8                           active
10   vlan 10                          active
11   vlan 11                          active
22   Student                          active    Gi1/0/6
23   Teacher                          active
24   Management                       active
25   Library                          active    Gi1/0/1, Gi1/0/2, Gi1/0/3
                                                Gi1/0/4, Gi1/0/5, Gi1/0/7
                                                Gi1/0/8, Gi1/0/9, Gi1/0/10
                                                Gi1/0/11, Gi1/0/12, Gi1/0/13
                                                Gi1/0/14, Gi1/0/15, Gi1/0/16
                                                Gi1/0/17, Gi1/0/18, Gi1/0/19
                                                Gi1/0/20, Gi1/0/21, Gi1/0/22
                                                Gi1/0/23, Gi1/0/24, Gi1/0/25
                                                Gi1/0/26, Gi1/0/27, Gi1/0/28
26   Native                           act/lshut
1002 fddi-default                     act/unsup
1003 token-ring-default               act/unsup

VLAN Name                             Status    Ports
---- -------------------------------- --------- -------------------------------
1004 fddinet-default                  act/unsup
1005 trnet-default                    act/unsup
S1#
S2>en
Password:
S2#show run
Building configuration...

Current configuration : 3545 bytes
!
! Last configuration change at 15:53:36 UTC Thu Aug 22 2024
!
version 15.2
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
service password-encryption
!
hostname S2
!
boot-start-marker
boot-end-marker
!
enable password 7 14141B180F0B7B7977
!
username cisco password 7 060506324F41584B56
no aaa new-model
switch 1 provision c1000-24t-4g-l
system mtu routing 1500
!
!
!
!
!
!
!
!
!
!
spanning-tree mode rapid-pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
!
!
!
interface GigabitEthernet1/0/1
 switchport access vlan 25
 switchport trunk native vlan 26
 switchport mode trunk
 shutdown
!
interface GigabitEthernet1/0/2
 switchport access vlan 25
 switchport trunk native vlan 26
 switchport mode trunk
 shutdown
!
interface GigabitEthernet1/0/3
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/4
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/5
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/6
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/7
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/8
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/9
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/10
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/11
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/12
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/13
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/14
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/15
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/16
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/17
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/18
 switchport access vlan 23
 switchport mode access
 switchport port-security mac-address sticky
!
interface GigabitEthernet1/0/19
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/20
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/21
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/22
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/23
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/24
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/25
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/26
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/27
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/28
 switchport access vlan 25
 switchport mode access
 shutdown
!
interface Vlan1
 no ip address
!
ip http server
ip http secure-server
!
!
!
!
line con 0
 password 7 094F471A1A0A464058
line vty 0
 login
 transport input ssh
line vty 1 4
 login
 transport input none
line vty 5 15
 login
 transport input none
!
end

S2#sh ip int br
Interface              IP-Address      OK? Method Status                Protocol
Vlan1                  unassigned      YES unset  up                    down
GigabitEthernet1/0/1   unassigned      YES unset  administratively down down
GigabitEthernet1/0/2   unassigned      YES unset  administratively down down
GigabitEthernet1/0/3   unassigned      YES unset  administratively down down
GigabitEthernet1/0/4   unassigned      YES unset  administratively down down
GigabitEthernet1/0/5   unassigned      YES unset  administratively down down
GigabitEthernet1/0/6   unassigned      YES unset  administratively down down
GigabitEthernet1/0/7   unassigned      YES unset  administratively down down
GigabitEthernet1/0/8   unassigned      YES unset  administratively down down
GigabitEthernet1/0/9   unassigned      YES unset  administratively down down
GigabitEthernet1/0/10  unassigned      YES unset  administratively down down
GigabitEthernet1/0/11  unassigned      YES unset  administratively down down
GigabitEthernet1/0/12  unassigned      YES unset  administratively down down
GigabitEthernet1/0/13  unassigned      YES unset  administratively down down
GigabitEthernet1/0/14  unassigned      YES unset  administratively down down
GigabitEthernet1/0/15  unassigned      YES unset  administratively down down
GigabitEthernet1/0/16  unassigned      YES unset  administratively down down
GigabitEthernet1/0/17  unassigned      YES unset  administratively down down
GigabitEthernet1/0/18  unassigned      YES unset  up                    up
GigabitEthernet1/0/19  unassigned      YES unset  administratively down down
GigabitEthernet1/0/20  unassigned      YES unset  administratively down down
GigabitEthernet1/0/21  unassigned      YES unset  administratively down down
GigabitEthernet1/0/22  unassigned      YES unset  administratively down down
GigabitEthernet1/0/23  unassigned      YES unset  administratively down down
GigabitEthernet1/0/24  unassigned      YES unset  administratively down down
GigabitEthernet1/0/25  unassigned      YES unset  administratively down down
GigabitEthernet1/0/26  unassigned      YES unset  administratively down down
GigabitEthernet1/0/27  unassigned      YES unset  administratively down down
GigabitEthernet1/0/28  unassigned      YES unset  administratively down down
S2#sh vlan br

VLAN Name                             Status    Ports
---- -------------------------------- --------- -------------------------------
1    default                          active
7    vlan 7                           active
8    vlan 8                           active
10   vlan 10                          active
11   vlan 11                          active
20   CarPark                          active
22   Student                          active
23   Teacher                          active    Gi1/0/18
24   Management                       active
25   Library                          active    Gi1/0/1, Gi1/0/2, Gi1/0/3
                                                Gi1/0/4, Gi1/0/5, Gi1/0/6
                                                Gi1/0/7, Gi1/0/8, Gi1/0/9
                                                Gi1/0/10, Gi1/0/11, Gi1/0/12
                                                Gi1/0/13, Gi1/0/14, Gi1/0/15
                                                Gi1/0/16, Gi1/0/17, Gi1/0/19
                                                Gi1/0/20, Gi1/0/21, Gi1/0/22
                                                Gi1/0/23, Gi1/0/24, Gi1/0/25
                                                Gi1/0/26, Gi1/0/27, Gi1/0/28
26   Native                           active
1002 fddi-default                     act/unsup

VLAN Name                             Status    Ports
---- -------------------------------- --------- -------------------------------
1003 token-ring-default               act/unsup
1004 fddinet-default                  act/unsup
1005 trnet-default                    act/unsup
S2#
R1>en
Password:
R1#sh run
Building configuration...

Current configuration : 6247 bytes
!
! Last configuration change at 15:24:24 UTC Wed Aug 21 2024
!
version 17.9
service timestamps debug datetime msec
service timestamps log datetime msec
service password-encryption
! Call-home is enabled by Smart-Licensing.
service call-home
platform qfp utilization monitor load 80
platform punt-keepalive disable-kernel-core
!
hostname R1
!
boot-start-marker
boot-end-marker
!
!
no aaa new-model
!
!
!
!
!
!
!
!
!
!
login on-success log
!
!
!
!
!
!
!
subscriber templating
vtp version 1
multilink bundle-name authenticated
!
!
!
crypto pki trustpoint TP-self-signed-2192705810
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-2192705810
 revocation-check none
 rsakeypair TP-self-signed-2192705810
!
crypto pki trustpoint SLA-TrustPoint
 enrollment pkcs12
 revocation-check crl
!
!
crypto pki certificate chain TP-self-signed-2192705810
 certificate self-signed 01
  30820330 30820218 A0030201 02020101 300D0609 2A864886 F70D0101 05050030
  31312F30 2D060355 04031326 494F532D 53656C66 2D536967 6E65642D 43657274
  69666963 6174652D 32313932 37303538 3130301E 170D3234 30383231 31343131
  32395A17 0D333430 38323131 34313132 395A3031 312F302D 06035504 03132649
  4F532D53 656C662D 5369676E 65642D43 65727469 66696361 74652D32 31393237
  30353831 30308201 22300D06 092A8648 86F70D01 01010500 0382010F 00308201
  0A028201 0100CB85 0DCF1BBA 0923537C 9824CB5F A005F110 C1F80D72 4B6919FE
  211D47BE 6E504582 AF33B264 31A56C7A B9297D79 BAE4BCF1 9FD1E932 6516EF92
  A2F9CB0A 17723596 3178EDDA F4052877 3C17E748 907E114E 6E6B3E01 1A72FDE3
  DBF5B1AF 0605CD1F 8137287B 0A82872F C48840DD AB33A16C 8B0FBADB 824E2BEB
  A7E1E99D 73B9E800 A9C3E5AC 23273570 7B947E12 D2430466 1FBB54DF ED980063
  3FF5FAEC D653670D D826EE3C F14FCD78 C82661EA 48D08374 78A77C30 ECA35335
  B88072D5 BD89D61B 4B9A8B5A D94B9E43 EE9E8E56 BDA78E06 011A198D 667590ED
  B470B17F 64A74C31 2C77E120 BA77F36B D119704C B47166B6 09F53CC1 BE37F3E1
  2999DB79 D9CD0203 010001A3 53305130 0F060355 1D130101 FF040530 030101FF
  301F0603 551D2304 18301680 140A8F6B B61837CA 5359DDD9 D699637F 619080BE
  FB301D06 03551D0E 04160414 0A8F6BB6 1837CA53 59DDD9D6 99637F61 9080BEFB
  300D0609 2A864886 F70D0101 05050003 82010100 9B72E9C9 C1114B22 AD168F84
  5144F704 92AA285C AF4CEF79 E5B32A09 67403123 4C83CFCF D6CB992D 430CD5B6
  61B50C61 0F4FCE6F 1295DF96 23450D39 7F3BF6C7 3D79E250 F5B53A3E 2C244C62
  3E3205BF F2E664D4 644FCB2F 62F826A0 C0CCA588 2F6D8332 3CB0470F 72A1CB15
  BE284FDC 4C8DF345 94ED7557 0D92E6F4 8C016DE2 E9B64D00 6FEDE035 C71A2F06
  4877B123 3DD5405A 7EA3719B 49A16BA5 BE1511E8 53563454 CC97ED63 9D666EA1
  3041E81E F576E276 472163E2 088C6D8D 5E9F291D CE414559 1679A954 DE6FEFFF
  4C9F9F79 8AA0168B 946DE52C 2C3D4794 6C5911CC CCE3E1BA 107A851A 6C9CB4E2
  2B6BF105 D1B8F802 A4166CFA 2EA88E2C 7E7B2427
        quit
crypto pki certificate chain SLA-TrustPoint
 certificate ca 01
  30820321 30820209 A0030201 02020101 300D0609 2A864886 F70D0101 0B050030
  32310E30 0C060355 040A1305 43697363 6F312030 1E060355 04031317 43697363
  6F204C69 63656E73 696E6720 526F6F74 20434130 1E170D31 33303533 30313934
  3834375A 170D3338 30353330 31393438 34375A30 32310E30 0C060355 040A1305
  43697363 6F312030 1E060355 04031317 43697363 6F204C69 63656E73 696E6720
  526F6F74 20434130 82012230 0D06092A 864886F7 0D010101 05000382 010F0030
  82010A02 82010100 A6BCBD96 131E05F7 145EA72C 2CD686E6 17222EA1 F1EFF64D
  CBB4C798 212AA147 C655D8D7 9471380D 8711441E 1AAF071A 9CAE6388 8A38E520
  1C394D78 462EF239 C659F715 B98C0A59 5BBB5CBD 0CFEBEA3 700A8BF7 D8F256EE
  4AA4E80D DB6FD1C9 60B1FD18 FFC69C96 6FA68957 A2617DE7 104FDC5F EA2956AC
  7390A3EB 2B5436AD C847A2C5 DAB553EB 69A9A535 58E9F3E3 C0BD23CF 58BD7188
  68E69491 20F320E7 948E71D7 AE3BCC84 F10684C7 4BC8E00F 539BA42B 42C68BB7
  C7479096 B4CB2D62 EA2F505D C7B062A4 6811D95B E8250FC4 5D5D5FB8 8F27D191
  C55F0D76 61F9A4CD 3D992327 A8BB03BD 4E6D7069 7CBADF8B DF5F4368 95135E44
  DFC7C6CF 04DD7FD1 02030100 01A34230 40300E06 03551D0F 0101FF04 04030201
  06300F06 03551D13 0101FF04 05300301 01FF301D 0603551D 0E041604 1449DC85
  4B3D31E5 1B3E6A17 606AF333 3D3B4C73 E8300D06 092A8648 86F70D01 010B0500
  03820101 00507F24 D3932A66 86025D9F E838AE5C 6D4DF6B0 49631C78 240DA905
  604EDCDE FF4FED2B 77FC460E CD636FDB DD44681E 3A5673AB 9093D3B1 6C9E3D8B
  D98987BF E40CBD9E 1AECA0C2 2189BB5C 8FA85686 CD98B646 5575B146 8DFC66A8
  467A3DF4 4D565700 6ADF0F0D CF835015 3C04FF7C 21E878AC 11BA9CD2 55A9232C
  7CA7B7E6 C1AF74F6 152E99B7 B1FCF9BB E973DE7F 5BDDEB86 C71E3B49 1765308B
  5FB0DA06 B92AFE7F 494E8A9E 07B85737 F3A58BE1 1A48A229 C37C1E69 39F08678
  80DDCD16 D6BACECA EEBC7CF9 8428787B 35202CDC 60E4616A B623CDBD 230E3AFB
  418616A9 4093E049 4D10AB75 27E86F73 932E35B5 8862FDAE 0275156F 719BB2F0
  D697DF7F 28
        quit
!
!
license udi pid C8200L-1N-4T sn FCZ2818R0RR
memory free low-watermark processor 62972
!
diagnostic bootup level minimal
!
spanning-tree extend system-id
!
enable password 7 045802150C2E1D1C5A
!
username cisco password 7 030752180500701E1D
!
redundancy
 mode none
!
!
!
!
!
!
!
!
interface GigabitEthernet0/0/0
 no ip address
 shutdown
 negotiation auto
!
interface GigabitEthernet0/0/1
 ip address 192.168.10.1 255.255.255.0
 shutdown
 negotiation auto
 vlan-range dot1q 22 26
 !
 vlan-id dot1q 1
 !
!
interface GigabitEthernet0/0/1.22
 shutdown
!
interface GigabitEthernet0/0/1.23
!
interface GigabitEthernet0/0/2
 no ip address
 shutdown
 negotiation auto
!
interface GigabitEthernet0/0/3
 no ip address
 shutdown
 negotiation auto
!
interface Serial0/1/0
!
interface Serial0/1/1
!
ip http server
ip http authentication local
ip http secure-server
ip forward-protocol nd
!
!
!
!
!
!
control-plane
!
!
line con 0
 password 7 094F471A1A0A464058
 stopbits 1
line aux 0
line vty 0
 location line
 login
 transport input ssh
line vty 1 4
 login
 transport input ssh
line vty 5 14
 login
 transport input ssh
!
call-home
 ! If contact email address in call-home is configured as sch-smart-licensing@cisco.com
 ! the email address configured in Cisco Smart License Portal will be used as contact email address to send SCH notifications.
 contact-email-addr sch-smart-licensing@cisco.com
 profile "CiscoTAC-1"
  active
  destination transport-method http
!
!
!
!
!
!
end

R1#sh ip int br
Any interface listed with OK? value "NO" does not have a valid configuration

Interface              IP-Address      OK? Method Status                Protocol
GigabitEthernet0/0/0   unassigned      YES unset  administratively down down
GigabitEthernet0/0/1   192.168.10.1    YES manual administratively down down
Gi0/0/1.22             unassigned      YES unset  administratively down down
Gi0/0/1.23             unassigned      YES unset  administratively down down
GigabitEthernet0/0/2   unassigned      YES unset  administratively down down
GigabitEthernet0/0/3   unassigned      YES unset  administratively down down
Serial0/1/0            unassigned      NO  unset  down                  down
Serial0/1/1            unassigned      NO  unset  down                  down
R1#
