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Lab - Accessing Network Devices with SSH

Lab - Accessing Network Devices with SSH 
Topology
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Addressing Table
	Device
	Interface
	IP Address
	Subnet Mask
	Default Gateway

	R1
	G0/1
	192.168.1.1
	255.255.255.0
	N/A

	S1
	VLAN 1
	192.168.1.11
	255.255.255.0
	192.168.1.1

	PC-A
	NIC
	192.168.1.3
	255.255.255.0
	192.168.1.1


Objectives
Part 1: Configure Basic Device Settings
Part 2: Configure Basic Security Measures on the Router and Switch
Part 3: Configure the Router for SSH Access
Part 4: Configure the Switch for SSH Access
Part 5: SSH from the CLI on the Switch
Background / Scenario
In the past, Telnet was the most common network protocol used to remotely configure network devices. Telnet does not encrypt the information between the client and server. This allows a network sniffer to intercept passwords and configuration information.
Secure Shell (SSH) is a network protocol that establishes a secure terminal emulation connection to a router or other networking device. SSH encrypts all information that passes over the network link and provides authentication of the remote computer. SSH is rapidly replacing Telnet as the remote login tool of choice for network professionals. SSH is most often used to log in to a remote device and execute commands; however, it can also transfer files using the associated Secure FTP (SFTP) or Secure Copy (SCP) protocols.
The network devices that are communicating must be configured to support SSH in order for SSH to function. In this lab, you will enable the SSH server on a router and then connect to that router using a PC with an SSH client installed. On a local network, the connection is normally made using Ethernet and IP.
Note: The routers used with CCNA hands-on labs are Cisco 1941 Integrated Services Routers (ISRs) with Cisco IOS Release 15.2(4)M3 (universalk9 image). The switches used are Cisco Catalyst 2960s with Cisco IOS Release 15.0(2) (lanbasek9 image). Other routers, switches, and Cisco IOS versions can be used. Depending on the model and Cisco IOS version, the commands available and the output produced might vary from what is shown in the labs. Refer to the Router Interface Summary Table at the end of this lab for the correct interface identifiers.
Note: Make sure that the routers and switches have been erased and have no startup configurations. If you are unsure, contact your instructor.
Required Resources
1 Router (Cisco 1941 with Cisco IOS Release 15.2(4)M3 universal image or comparable)
1 Switch (Cisco 2960 with Cisco IOS Release 15.0(2) lanbasek9 image or comparable)
1 PC (Windows 7 or 8 with terminal emulation program, such as Tera Term, and Wireshark installed)
Console cables to configure the Cisco IOS devices via the console ports
Ethernet cables as shown in the topology
Configure Basic Device Settings
In Part 1, you will set up the network topology and configure basic settings, such as the interface IP addresses, device access, and passwords on the router.
Cable the network as shown in the topology.
Step 1: Initialize and reload the router and switch.
Step 2: Configure the router.
a. Console into the router and enable privileged EXEC mode.
b. Enter configuration mode.
c. Disable DNS lookup to prevent the router from attempting to translate incorrectly entered commands as though they were host names.
d. Assign class as the privileged EXEC encrypted password.
e. Assign cisco as the console password and enable login.
f. Assign cisco as the VTY password and enable login.
g. Encrypt the plaintext passwords.
h. Create a banner that will warn anyone accessing the device that unauthorized access is prohibited.
i. Configure and activate the G0/1 interface on the router using the information contained in the Addressing Table.
j. Save the running configuration to the startup configuration file.
Configure PC-A.
Configure PC-A with an IP address and subnet mask.
Configure a default gateway for PC-A.
Verify network connectivity.
Ping R1 from PC-A. If the ping fails, troubleshoot the connection.



1. Configure Basic Security Measures on the Router
b. Encrypt the clear text passwords.
R1(config)# service password-encryption
b. Strengthen passwords.
An administrator should ensure that passwords meet the standard guidelines for strong passwords. These guidelines could include combining letters, numbers and special characters in the password and setting a minimum length.
Note: Best practice guidelines require the use of strong passwords, such as those shown here, in a production environment. However, the other labs in this course use the cisco and class passwords for ease in performing the labs.
2. Change the privileged EXEC encrypted password to meet guidelines.
R1(config)# enable secret Enablep@55
2. Require that a minimum of 10 characters be used for all passwords.
R1(config)# security passwords min-length 10
b. Secure the console and VTY lines.
3. You can set the router to log out of a connection that has been idle for a specified time. If a network administrator was logged into a networking device and was suddenly called away, this command automatically logs the user out after the specified time. The following commands cause the line to log out after five minutes of inactivity.
R1(config)# line console 0
R1(config-line)# exec-timeout 5 0
R1(config-line)# line vty 0 4
R1(config-line)# exec-timeout 5 0
R1(config-line)# exit
R1(config)#
3. The following command impedes brute force login attempts. The router blocks login attempts for 30 seconds if someone fails two attempts within 120 seconds. This timer is set especially low for the purpose of this lab.
R1(config)# login block-for 30 attempts 2 within 120
What does the 2 within 120 mean in the above command?
The 2 represents how many attempts you have within 120 seconds.
What does the block-for 30 mean in the above command?
30 means that you are locked out from entering a password for 30 seconds due to the password being incorrectly entered.
b. Verify that all unused ports are disabled.
Router ports are disabled by default, but it is always prudent to verify that all unused ports are in an administratively down state. This can be quickly checked by issuing the show ip interface brief command. Any unused ports that are not in an administratively down state should be disabled using the shutdown command in interface configuration mode.


R1# show ip interface brief
Interface                  IP-Address      OK? Method Status                Protocol
Embedded-Service-Engine0/0 unassigned      YES NVRAM  administratively down down    
GigabitEthernet0/0         unassigned      YES NVRAM  administratively down down    
GigabitEthernet0/1         192.168.1.1     YES manual up                    up      
Serial0/0/0                unassigned      YES NVRAM  administratively down down    
Serial0/0/1                unassigned      YES NVRAM  administratively down down    

Configure the Router for SSH Access
Using Telnet to connect to a network device is a security risk because all information is transmitted in a clear text format. SSH encrypts the session data and provides device authentication, which is why SSH is recommended for remote connections. In Part 2, you will configure the router to accept SSH connections over the VTY lines.
Configure device authentication.
The device name and domain are used as part of the crypto key when it is generated. Therefore, these names must be entered prior to issuing the crypto key command.
Configure the domain for the device.
R1(config)# ip domain-name ccna-lab.com
Configure the encryption key method.
R1(config)# crypto key generate rsa modulus 1024
The name for the keys will be: R1.ccna-lab.com

% The key modulus size is 1024 bits
% Generating 1024 bit RSA keys, keys will be non-exportable...
[OK] (elapsed time was 1 seconds) 

R1(config)#
*Jan 28 21:09:29.867: %SSH-5-ENABLED: SSH 1.99 has been enabled
Configure a local database username.
R1(config)# username admin privilege 15 secret adminpass
Note: A privilege level of 15 gives the user administrator rights. Note: password is adminpass1
Enable SSH on the VTY lines.
Enable Telnet and SSH on the inbound VTY lines using the transport input command.
R1(config)# line vty 0 4
R1(config-line)# transport input ssh
Change the login method to use the local database for user verification.
R1(config-line)# login local
R1(config-line)# end
R1#
Save the running configuration to the startup configuration file.
R1# copy running-config startup-config
Destination filename [startup-config]?
Building configuration...
[OK]
R1#
Establish an SSH connection to the router.
Start Tera Term from PC-A.
Use Tera Term to telnet to R1.
Does R1 accept the Telnet connection? Explain.
R1 does not accept the connection, this because telnet connection on R1 is closed, this doesn’t really affect us due to the fact that telnet isn’t as secure as using an ssh connection.
Use Tera Term, establish an SSH session to R1. Use the username admin and password adminpass. You should be able to establish an SSH session with R1.
Does R1 accept the SSH connection? 
Yes R1 accepts SSH connection with admin privileges.
Intentionally mistype the user and password information to see if login access is blocked after two attempts.
What happened after you failed to login the second time?
R1 closes the SSH session with PCA.


From your console session on the router, issue the show login command to view the login status. In the example below, the show login command was issued within the 30 second login blocking period and shows that the router is in Quiet-Mode. The router will not accept any login attempts for 14 more seconds.
R1# show login
     A default login delay of 1 second is applied.
     No Quiet-Mode access list has been configured.

     Router enabled to watch for login Attacks.
     If more than 2 login failures occur in 120 seconds or less,
     logins will be disabled for 30 seconds.

     Router presently in Quiet-Mode.
     Will remain in Quiet-Mode for 14 seconds.
     Denying logins from all sources.
R1#
After the 30 seconds has expired, SSH to R1 again and login using the SSHadmin username and Admin1p@55 for the password.
After you successfully logged in, what was displayed? It displayed the command line interface for R1 after logging in.

 
Enter privileged EXEC mode and use Enablep@55 for the password.
If you mistype this password, are you disconnected from your SSH session after two failed attempts within 120 seconds? Explain.
It is impossible to use privilege executive mode as we are using the admin which already has level 15 security and by passes all blocks.
Issue the show running-config command at the privileged EXEC prompt to view the security settings you have applied.
Configure the Switch for SSH Access
In Part 3, you will configure the switch in the topology to accept SSH connections. After the switch has been configured, establish an SSH session using Tera Term.
Configure the basic settings on the switch.
Console into the switch and enable privileged EXEC mode.
Enter configuration mode.
Disable DNS lookup to prevent the router from attempting to translate incorrectly entered commands as though they were host names.
Assign class as the privileged EXEC encrypted password.
Assign cisco as the console password and enable login.
Assign cisco as the VTY password and enable login.
Encrypt the plain text passwords.
Create a banner that will warn anyone accessing the device that unauthorized access is prohibited.
Configure and activate the VLAN 1 interface on the switch according to the Addressing Table.
Save the running configuration to the startup configuration file.
Configure the switch for SSH connectivity.
Use the same commands that you used to configure SSH on the router in Part 2 to configure SSH for the switch.
Configure the device name as listed in the Addressing Table.
Configure the domain for the device.
S1(config)# ip domain-name ccna-lab.com
Configure the encryption key method.
S1(config)# crypto key generate rsa modulus 1024
Configure a local database username.
S1(config)# username admin privilege 15 secret adminpass
Enable Telnet and SSH on the VTY lines. Note: Password is adminpass1
S1(config)# line vty 0 15
S1(config-line)# transport input telnet ssh
Change the login method to use the local database for user verification.
S1(config-line)# login local
S1(config-line)# end
Establish an SSH connection to the switch.
Start Tera Term from PC-A, and then SSH to the SVI interface on S1.
Are you able to establish an SSH session with the switch?
Yes I am able to establish an SSH session with the switch and able to use the switches CLI with PCA
SSH From the CLI on the Switch
The SSH client is built into the Cisco IOS and can be run from the CLI. In Part 4, you will SSH to the router from the CLI on the switch.
View the parameters available for the Cisco IOS SSH client.
Use the question mark (?) to display the parameter options available with the ssh command.
S1# ssh ?
  -c    Select encryption algorithm
  -l    Log in using this user name
  -m    Select HMAC algorithm
  -o    Specify options
  -p    Connect to this port
  -v    Specify SSH Protocol Version
  -vrf  Specify vrf name
  WORD  IP address or hostname of a remote system
SSH to R1 from S1.
You must use the –l admin option when you SSH to R1. This allows you to log in as user admin. When prompted, enter adminpass for the password.
S1# ssh -l admin 192.168.1.1
Password: 
***********************************************
  Warning: Unauthorized Access is Prohibited!
***********************************************

R1#
You can return to S1 without closing the SSH session to R1 by pressing Ctrl+Shift+6. Release the Ctrl+Shift+6 keys and press x. The switch privileged EXEC prompt displays.
R1#
S1#
To return to the SSH session on R1, press Enter on a blank CLI line. You may need to press Enter a second time to see the router CLI prompt.
S1#
[Resuming connection 1 to 192.168.1.1 ... ]

R1#
To end the SSH session on R1, type exit at the router prompt.
R1# exit

[Connection to 192.168.1.1 closed by foreign host]
S1#

What versions of SSH are supported from the CLI?
The CLI supports SSH versions 1 and 2
How would you provide multiple users, each with their own username, access to a network device?
You would put each user’s username and password into a database.

Reflection (max 800 words): 
Write a research report comparing various Encryption standards, e.g AES, SHA, DES, RSA.  


Jack Rout
1802047
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Encryption standards
Introduction:
This report will be talking about Encryption standards such as Advanced Encryption Standards (AES), Secure Hash Algorithms (SHA), Data Encryption Standard (DES) and Rivest-Shamir-Adleman (RSA).

Advanced Encryption Standards:
AES is a military grade encryption that was designed for the sole purpose of protecting classified information. AES was created since they used DES before AES, they realized that DES was becoming weak to users attempting to brute forced their way in. AES was also designed to be easy to implement into software and hardware, this also offers a good defense against anyone who tries to bypass this encryption.

AES has a group of 3 in bit block groups that hold a crypto key though the key sizes are unlimited the blocks that the keys are in are not unlimited and are 128,192,256 bits in size. AES replaced DES by being able to encrypt each block that the key is held in. AES algorithm makes it so that there is only 1 key to encrypt data and decrypt it. It is predicted that AES will last for 20 to 30 years before it is going to need to be replaced. AES is also available to everyone worldwide; it doesn’t cost anything in order to use it and is easy to implement into hardware and software. [1] [2]
Secure Hash Algorithms:
SHA is a function designed to keep data secure, it does this by transforming data into hash values, this is good for companies since they would be using a database to keep hold of usernames and passwords and since the hash values encrypt the passwords into a completely different value. 
With the password being changed to a different value in the database this makes it easier for the server to keep track of specific data belonging to that user and their hash value. It is also easier to tell if a file with a hash value has been tampered with for example a word file could easily be tampered with and it would be hard to notice the difference. 

SHA makes it difficult for those who hack into secure databases since there will be nothing that you can gain from it visually since the hash function has completely changed the password into a different value and the password will only be know to the person that created the password to begin with. [3]

Data Encryption Standards:
DES was a military grade encryption until it became obsolete compared to its successor AES, this was mostly because the biggest weakness that DES has is the fact that someone could brute force their way into secure files. 
The way DES works is by using the same private key to encrypt and decrypt files for example if I were to send a file to a friend and it is encrypted both myself and the friend will have to know the private key in order to access the file, or as mentioned earlier these files can be brute forces. [4]
Rivest-Shamir-Adleman:
RSA is an encryption used to send secret coded messages between 2 people or more, for this to work every person receiving this encoded message will have to have the key in order to access the message that was sent.

 RSA works by 2 people setting up a private key so that they can access for example a file, they would then send out a different key to another person that person will then use this key to encrypt the data that they want to send. Once the data is sent it then can only be opened by the people with a private key. [5]
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