S2(config-if-range)#exit
S2(config)#int
*Aug 21 16:29:18.605: %LINK-5-CHANGED: Interface GigabitEthernet1/0/3, changed s                                                                                                                                                             tate to administratively down
*Aug 21 16:29:18.607: %LINK-5-CHANGED: Interface GigabitEthernet1/0/4, changed s                                                                                                                                                             tate to administratively down
*Aug 21 16:29:18.608: %LINK-5-CHANGED: Interface GigabitEthernet1/0/5, changed s                                                                                                                                                             tate to administratively down ran
% Incomplete command.

S2(config)#
S2(config)#
S2(config)#int range g1/0/7-28
S2(config-if-range)#shutdown
S2(config-if-range)#exi
S2(config)#exit
S2#
*Aug 21 16:29:57.825: %LINK-5-CHANGED: Interface GigabitEthernet1/0/7, changed s                                                                                                                                                             tate to administratively down
*Aug 21 16:29:57.827: %LINK-5-CHANGED: Interface GigabitEthernet1/0/8, changed s                                                                                                                                                             tate to administratively down
*Aug 21 16:29:57.829: %LINK-5-CHANGED: Interface GigabitEthernet1/0/9, changed s                                                                                                                                                             tate to administratively down
*Aug 21 16:29:57.830: %LINK-5-CHANGED: Interface GigabitEthernet1/0/10, changed                                                                                                                                                              state to administratively down
*Aug 21 16:29:57.832: %LINK-5-CHANGED: Interface GigabitEthernet
S2#1/0/11, changed state to administratively down
*Aug 21 16:29:57.833: %LINK-5-CHANGED: Interface GigabitEthernet1/0/12, changed                                                                                                                                                              state to administratively down
*Aug 21 16:29:57.835: %LINK-5-CHANGED: Interface GigabitEthernet1/0/13, changed                                                                                                                                                              state to administratively down
*Aug 21 16:29:57.837: %LINK-5-CHANGED: Interface GigabitEthernet1/0/14, changed                                                                                                                                                              state to administratively down
*Aug 21 16:29:57.838: %LINK-5-CHANGED: Interface GigabitEthernet1/0/15, changed                                                                                                                                                              state to administratively down
*Aug 21 16:29:57.840: %LINK-5-CHANGED: Interface GigabitEthernet1/0/16, changed                                                                                                                                                              state to administratively down
*Aug 21 16:29:57.841: %LINK-5-CHANGED: Interface GigabitEthernet1/0/17, changed                                                                                                                                                              state to administratively down
*Aug 21 16:29:57.843: %LINK-5-CHANGED: Interface GigabitEthernet1/0/18, changed                                                                                                                                                              state to administratively down
*Aug 21 16:29:57.905: %LINK-5-CHANGED: Interface GigabitEthernet1/0/19, changed                                                                                                                                                              state to administratively down
*Aug 21 16:29:57.907: %LINK-5-CHANGED: Interface GigabitEthernet1/0/20, changed                                                                                                                                                              state to administratively down
*Aug 21 16:29:57.908: %LINK-5-CHANGED: Interface GigabitEthernet1/0/21, changed                                                                                                                                                              state to administratively down
*Aug 21 16:29:57.910: %LINK-5-CHANGED: Interface GigabitEthernet1/0/22, changed                                                                                                                                                              state to administratively down
*Aug 21 16:29:57.911: %LINK-5-CHANGED: Interface GigabitEthernet1/0/23, changed                                                                                                                                                              state to administratively down
*Aug 21 16:29:57.913: %LINK-5-CHANGED: Interface GigabitEthernet1/0/24, changed                                                                                                                                                              state to administratively down
*Aug 21 16:29:57.915: %LINK-5-CHANGED: Interface GigabitEthernet1/0/25, changed                                                                                                                                                              state to administratively down
*Aug 21 16:29:57.916: %LINK-5-CHANGED: Interface GigabitEthernet1/0/26, changed                                                                                                                                                              state to administratively down
*Aug 21 16:29:57.917: %LINK-5-CHANGED: Interface GigabitEthernet1/0/27, changed                                                                                                                                                              state to administratively down
*Aug 21 16:29:57.919: %LINK-5-CHANGED: Interface GigabitEthernet1/0/28, changed                                                                                                                                                              state to administratively down
*Aug 21 16:29:58.577: %SYS-5-CONFIG_I: Configured from console by console
*Aug 21 16:29:58.843: %LINEPROTO-5-UPDOWN: Line protocol on Interface GigabitEth                                                                                                                                                             ernet1/0/18, changed state to down
S2#
S2#
S2#
S2#
S2#
S2#
S1#
S1#
S1#
S1#
S1#en
S1#config t
Enter configuration commands, one per line.  End with CNTL/Z.
S1(config)#int range g1/0/3-5
S1(config-if-range)#shutdown
S1(config-if-range)#exit
S1(config)#
S1(config)#exit
S1#sh i
*Aug 21 16:31:49.834: %SYS-5-CONFIG_I: Configured from console by consolep
% Incomplete command.

S1#
S1#
S1#sh ip int brief
Interface              IP-Address      OK? Method Status                Protocol
Vlan1                  unassigned      YES unset  up                    up
Vlan24                 192.168.110.2   YES manual up                    down
GigabitEthernet1/0/1   unassigned      YES unset  up                    up
GigabitEthernet1/0/2   unassigned      YES unset  up                    up
GigabitEthernet1/0/3   unassigned      YES unset  administratively down down
GigabitEthernet1/0/4   unassigned      YES unset  administratively down down
GigabitEthernet1/0/5   unassigned      YES unset  administratively down down
GigabitEthernet1/0/6   unassigned      YES unset  down                  down
GigabitEthernet1/0/7   unassigned      YES unset  administratively down down
GigabitEthernet1/0/8   unassigned      YES unset  administratively down down
GigabitEthernet1/0/9   unassigned      YES unset  administratively down down
GigabitEthernet1/0/10  unassigned      YES unset  administratively down down
GigabitEthernet1/0/11  unassigned      YES unset  administratively down down
GigabitEthernet1/0/12  unassigned      YES unset  administratively down down
GigabitEthernet1/0/13  unassigned      YES unset  administratively down down
GigabitEthernet1/0/14  unassigned      YES unset  administratively down down
GigabitEthernet1/0/15  unassigned      YES unset  administratively down down
GigabitEthernet1/0/16  unassigned      YES unset  administratively down down
GigabitEthernet1/0/17  unassigned      YES unset  administratively down down
GigabitEthernet1/0/18  unassigned      YES unset  administratively down down
GigabitEthernet1/0/19  unassigned      YES unset  administratively down down
GigabitEthernet1/0/20  unassigned      YES unset  administratively down down
GigabitEthernet1/0/21  unassigned      YES unset  administratively down down
GigabitEthernet1/0/22  unassigned      YES unset  administratively down down
GigabitEthernet1/0/23  unassigned      YES unset  administratively down down
GigabitEthernet1/0/24  unassigned      YES unset  administratively down down
GigabitEthernet1/0/25  unassigned      YES unset  administratively down down
GigabitEthernet1/0/26  unassigned      YES unset  administratively down down
GigabitEthernet1/0/27  unassigned      YES unset  administratively down down
GigabitEthernet1/0/28  unassigned      YES unset  administratively down down
Port-channel1          unassigned      YES unset  up                    up
S1# config t
Enter configuration commands, one per line.  End with CNTL/Z.
S1(config)#int range 1/0/7-28
                     ^
% Invalid input detected at '^' marker.

S1(config)#int range g1/0/7-28
S1(config-if-range)#shutdown
S1(config-if-range)#exi
S1(config)#exi
S1#
*Aug 21 16:32:36.024: %SYS-5-CONFIG_I: Configured from console by console
S1#
S1#
S1#
S1#
S1#
S1#
S1#
S1#

User Access Verification

Password:
Password:
R1>en
Password:
R1#copy run start
Destination filename [startup-config]?
Building configuration...
[OK]
R1#
R1#
*Aug 21 16:31:26.461: %SYS-6-PRIVCFG_ENCRYPT_SUCCESS: Successfully encrypted pri                                                                                                                                                             vate config file
S1#
S1#copy run start
Destination filename [startup-config]?
Building configuration...
[OK]
S1#
S1#
S2#
S2#copy run start
Destination filename [startup-config]?
Building configuration...
[OK]
S2#
S2#
R1#sh run
Building configuration...

Current configuration : 6502 bytes
!
! Last configuration change at 15:18:38 UTC Wed Aug 21 2024
!
version 17.9
service timestamps debug datetime msec
service timestamps log datetime msec
service password-encryption
! Call-home is enabled by Smart-Licensing.
service call-home
platform qfp utilization monitor load 80
platform punt-keepalive disable-kernel-core
!
hostname R1
!
boot-start-marker
boot-end-marker
!
!
no aaa new-model
!
!
!
!
!
!
!
ip domain name swre-lab.com
!
!
!
login on-success log
!
!
!
!
!
!
!
subscriber templating
vtp version 1
multilink bundle-name authenticated
!
!
!
crypto pki trustpoint TP-self-signed-3889378622
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-3889378622
 revocation-check none
 rsakeypair TP-self-signed-3889378622
!
crypto pki trustpoint SLA-TrustPoint
 enrollment pkcs12
 revocation-check crl
!
!
crypto pki certificate chain TP-self-signed-3889378622
 certificate self-signed 01
  30820330 30820218 A0030201 02020101 300D0609 2A864886 F70D0101 05050030
  31312F30 2D060355 04031326 494F532D 53656C66 2D536967 6E65642D 43657274
  69666963 6174652D 33383839 33373836 3232301E 170D3234 30383231 31333135
  32315A17 0D333430 38323131 33313532 315A3031 312F302D 06035504 03132649
  4F532D53 656C662D 5369676E 65642D43 65727469 66696361 74652D33 38383933
  37383632 32308201 22300D06 092A8648 86F70D01 01010500 0382010F 00308201
  0A028201 0100ACE1 876E0E2B 1ECDB5D8 19AC0920 E8C0AD6A F5E17BBE 4C015D2F
  3B7F5A2D 79A4248F 2653343F 604BDC77 DBF73FE1 68C6A088 09163237 07B8AA39
  29B7C21B 48F1B04C 06F6FA5D 6A5EECB6 5A2E5E43 9B7E3864 7C08D6C4 530867C6
  D872B680 7EC0A537 BC145B03 23C0930A A055B81B 15868C62 9C51EE06 F3184D54
  0B03676B C36E1FFB 4838EE30 FB6A2A65 8DC8DE25 5D657CB4 96D2BBA0 A01C785D
  8F88A431 768A56B8 1390FC9E 782B3218 431A409B A75894E3 9CC71E6F 23394DC7
  56279F8A 53DDDCE4 08D5109D A4995358 20872980 52ADE105 4312F45C 78447E02
  0E69D161 0DE21A7B F64DF7C6 7EFED911 A5741446 DDA8A0E7 D33BD19C 30EC7E96
  E259485C 5C950203 010001A3 53305130 0F060355 1D130101 FF040530 030101FF
  301F0603 551D2304 18301680 148E2851 B654347C 66ADFD91 C5E1115B DE3BA4C6
  87301D06 03551D0E 04160414 8E2851B6 54347C66 ADFD91C5 E1115BDE 3BA4C687
  300D0609 2A864886 F70D0101 05050003 82010100 411BDB3F EA6D3431 E204C3B7
  E4D64F10 29F2DE0A 5105AC0C 4EB1A8CE 155D6ACC B0AE84F7 0FA67028 58E51D77
  491FD56F AD612316 9D889266 D935C926 F1547A46 663E357B 26330B01 3FB05B33
  BC82C5BB 341E8A39 EAABC233 612CC04A 7BE638AE 0C2C1658 1682351D 7CDFFB07
  FEBB9893 04EE518A C3639264 BEDD9624 ED790409 115A80A6 FF89D26B 3868B22E
  1FA4F8A7 83441C86 B395BEF5 29475AB9 ED968576 2554A62A F6866708 85A721FC
  5CB19FCD 9754F8F3 5C09E7D3 A0AC9DFE 567B9D27 5DD951B1 B6A5FBB5 B7BE2359
  331B2E66 7A46DFA8 6B417A3E 54D5EAAB D2EFCD61 BC462007 057B7FF3 B7A74A3F
  342EE402 7CB247C2 50442475 4FA82B4A 7EB2CD51
        quit
crypto pki certificate chain SLA-TrustPoint
 certificate ca 01
  30820321 30820209 A0030201 02020101 300D0609 2A864886 F70D0101 0B050030
  32310E30 0C060355 040A1305 43697363 6F312030 1E060355 04031317 43697363
  6F204C69 63656E73 696E6720 526F6F74 20434130 1E170D31 33303533 30313934
  3834375A 170D3338 30353330 31393438 34375A30 32310E30 0C060355 040A1305
  43697363 6F312030 1E060355 04031317 43697363 6F204C69 63656E73 696E6720
  526F6F74 20434130 82012230 0D06092A 864886F7 0D010101 05000382 010F0030
  82010A02 82010100 A6BCBD96 131E05F7 145EA72C 2CD686E6 17222EA1 F1EFF64D
  CBB4C798 212AA147 C655D8D7 9471380D 8711441E 1AAF071A 9CAE6388 8A38E520
  1C394D78 462EF239 C659F715 B98C0A59 5BBB5CBD 0CFEBEA3 700A8BF7 D8F256EE
  4AA4E80D DB6FD1C9 60B1FD18 FFC69C96 6FA68957 A2617DE7 104FDC5F EA2956AC
  7390A3EB 2B5436AD C847A2C5 DAB553EB 69A9A535 58E9F3E3 C0BD23CF 58BD7188
  68E69491 20F320E7 948E71D7 AE3BCC84 F10684C7 4BC8E00F 539BA42B 42C68BB7
  C7479096 B4CB2D62 EA2F505D C7B062A4 6811D95B E8250FC4 5D5D5FB8 8F27D191
  C55F0D76 61F9A4CD 3D992327 A8BB03BD 4E6D7069 7CBADF8B DF5F4368 95135E44
  DFC7C6CF 04DD7FD1 02030100 01A34230 40300E06 03551D0F 0101FF04 04030201
  06300F06 03551D13 0101FF04 05300301 01FF301D 0603551D 0E041604 1449DC85
  4B3D31E5 1B3E6A17 606AF333 3D3B4C73 E8300D06 092A8648 86F70D01 010B0500
  03820101 00507F24 D3932A66 86025D9F E838AE5C 6D4DF6B0 49631C78 240DA905
  604EDCDE FF4FED2B 77FC460E CD636FDB DD44681E 3A5673AB 9093D3B1 6C9E3D8B
  D98987BF E40CBD9E 1AECA0C2 2189BB5C 8FA85686 CD98B646 5575B146 8DFC66A8
  467A3DF4 4D565700 6ADF0F0D CF835015 3C04FF7C 21E878AC 11BA9CD2 55A9232C
  7CA7B7E6 C1AF74F6 152E99B7 B1FCF9BB E973DE7F 5BDDEB86 C71E3B49 1765308B
  5FB0DA06 B92AFE7F 494E8A9E 07B85737 F3A58BE1 1A48A229 C37C1E69 39F08678
  80DDCD16 D6BACECA EEBC7CF9 8428787B 35202CDC 60E4616A B623CDBD 230E3AFB
  418616A9 4093E049 4D10AB75 27E86F73 932E35B5 8862FDAE 0275156F 719BB2F0
  D697DF7F 28
        quit
!
!
license udi pid C8200L-1N-4T sn FCZ2818R0M2
memory free low-watermark processor 62972
!
diagnostic bootup level minimal
!
spanning-tree extend system-id
!
enable password 7 02050D4808095E731F
!
username cisco privilege 15 password 7 030752180500701E1D
!
redundancy
 mode none
!
!
!
!
!
!
!
!
interface Loopback0
 ip address 209.165.101.1 255.255.255.224
!
interface GigabitEthernet0/0/0
 no ip address
 shutdown
 negotiation auto
!
interface GigabitEthernet0/0/1
 no ip address
 negotiation auto
!
interface GigabitEthernet0/0/1.22
 encapsulation dot1Q 22
 ip address 192.168.90.1 255.255.255.0
!
interface GigabitEthernet0/0/1.23
 encapsulation dot1Q 23
 ip address 192.168.100.1 255.255.255.0
!
interface GigabitEthernet0/0/1.24
 encapsulation dot1Q 24
 ip address 192.168.110.1 255.255.255.0
!
interface GigabitEthernet0/0/2
 no ip address
 shutdown
 negotiation auto
!
interface GigabitEthernet0/0/3
 no ip address
 shutdown
 negotiation auto
!
interface Serial0/1/0
 no ip address
 shutdown
!
interface Serial0/1/1
 no ip address
 shutdown
!
ip http server
ip http authentication local
ip http secure-server
ip forward-protocol nd
!
!
!
!
!
!
control-plane
!
!
line con 0
 password 7 121A0C0411045D5679
 login
 stopbits 1
line aux 0
line vty 0 4
 login local
 transport input ssh
line vty 5 15
 login local
 transport input ssh
!
call-home
 ! If contact email address in call-home is configured as sch-smart-licensing@ci                                                                                                                                                             sco.com
 ! the email address configured in Cisco Smart License Portal will be used as co                                                                                                                                                             ntact email address to send SCH notifications.
 contact-email-addr sch-smart-licensing@cisco.com
 profile "CiscoTAC-1"
  active
  destination transport-method http
!
!
!
!
!
!
end

R1#sh ip int brief
Interface              IP-Address      OK? Method Status                Protocol
GigabitEthernet0/0/0   unassigned      YES unset  administratively down down
GigabitEthernet0/0/1   unassigned      YES unset  down                  down
Gi0/0/1.22             192.168.90.1    YES manual down                  down
Gi0/0/1.23             192.168.100.1   YES manual down                  down
Gi0/0/1.24             192.168.110.1   YES manual down                  down
GigabitEthernet0/0/2   unassigned      YES unset  administratively down down
GigabitEthernet0/0/3   unassigned      YES unset  administratively down down
Serial0/1/0            unassigned      YES unset  administratively down down
Serial0/1/1            unassigned      YES unset  administratively down down
Loopback0              209.165.101.1   YES manual up                    up
R1#
S1#sh run
Building configuration...

Current configuration : 2437 bytes
!
! Last configuration change at 16:32:36 UTC Wed Aug 21 2024
!
version 15.2
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
service password-encryption
!
hostname S1
!
boot-start-marker
boot-end-marker
!
enable password 7 05080F1C22431F5B4A
!
username cisco privilege 15 password 7 02050D4808095E731F
no aaa new-model
switch 1 provision c1000-24t-4g-l
system mtu routing 1500
!
!
no ip domain-lookup
ip domain-name swre-lab.com
!
shutdown vlan 25
!
!
!
!
!
!
!
!
spanning-tree mode rapid-pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
!
!
!
interface Port-channel1
!
interface GigabitEthernet1/0/1
 channel-group 1 mode active
!
interface GigabitEthernet1/0/2
 channel-group 1 mode active
!
interface GigabitEthernet1/0/3
 shutdown
!
interface GigabitEthernet1/0/4
 shutdown
!
interface GigabitEthernet1/0/5
 switchport trunk native vlan 26
 switchport mode trunk
 shutdown
!
interface GigabitEthernet1/0/6
 switchport access vlan 22
 switchport mode access
 switchport port-security maximum 3
 switchport port-security violation restrict
 switchport port-security
!
interface GigabitEthernet1/0/7
 shutdown
!
interface GigabitEthernet1/0/8
 shutdown
!
interface GigabitEthernet1/0/9
 shutdown
!
interface GigabitEthernet1/0/10
 shutdown
!
interface GigabitEthernet1/0/11
 shutdown
!
interface GigabitEthernet1/0/12
 shutdown
!
interface GigabitEthernet1/0/13
 shutdown
!
interface GigabitEthernet1/0/14
 shutdown
!
interface GigabitEthernet1/0/15
 shutdown
!
interface GigabitEthernet1/0/16
 shutdown
!
interface GigabitEthernet1/0/17
 shutdown
!
interface GigabitEthernet1/0/18
 shutdown
!
interface GigabitEthernet1/0/19
 shutdown
!
interface GigabitEthernet1/0/20
 shutdown
!
interface GigabitEthernet1/0/21
 shutdown
!
interface GigabitEthernet1/0/22
 shutdown
!
interface GigabitEthernet1/0/23
 shutdown
!
interface GigabitEthernet1/0/24
 shutdown
!
interface GigabitEthernet1/0/25
 shutdown
!
interface GigabitEthernet1/0/26
 shutdown
!
interface GigabitEthernet1/0/27
 shutdown
!
interface GigabitEthernet1/0/28
 shutdown
!
interface Vlan1
 no ip address
!
interface Vlan24
 ip address 192.168.110.2 255.255.255.0
!
ip default-gateway 192.168.110.1
ip http server
ip http secure-server
!
!
!
!
line con 0
 password 7 0822455D0A16544541
 login
line vty 0 4
 login local
 transport input ssh
line vty 5 15
 login local
 transport input none
!
end

S1#sh ip int brief
Interface              IP-Address      OK? Method Status                Protocol
Vlan1                  unassigned      YES unset  up                    up
Vlan24                 192.168.110.2   YES manual up                    down
GigabitEthernet1/0/1   unassigned      YES unset  up                    up
GigabitEthernet1/0/2   unassigned      YES unset  up                    up
GigabitEthernet1/0/3   unassigned      YES unset  administratively down down
GigabitEthernet1/0/4   unassigned      YES unset  administratively down down
GigabitEthernet1/0/5   unassigned      YES unset  administratively down down
GigabitEthernet1/0/6   unassigned      YES unset  down                  down
GigabitEthernet1/0/7   unassigned      YES unset  administratively down down
GigabitEthernet1/0/8   unassigned      YES unset  administratively down down
GigabitEthernet1/0/9   unassigned      YES unset  administratively down down
GigabitEthernet1/0/10  unassigned      YES unset  administratively down down
GigabitEthernet1/0/11  unassigned      YES unset  administratively down down
GigabitEthernet1/0/12  unassigned      YES unset  administratively down down
GigabitEthernet1/0/13  unassigned      YES unset  administratively down down
GigabitEthernet1/0/14  unassigned      YES unset  administratively down down
GigabitEthernet1/0/15  unassigned      YES unset  administratively down down
GigabitEthernet1/0/16  unassigned      YES unset  administratively down down
GigabitEthernet1/0/17  unassigned      YES unset  administratively down down
GigabitEthernet1/0/18  unassigned      YES unset  administratively down down
GigabitEthernet1/0/19  unassigned      YES unset  administratively down down
GigabitEthernet1/0/20  unassigned      YES unset  administratively down down
GigabitEthernet1/0/21  unassigned      YES unset  administratively down down
GigabitEthernet1/0/22  unassigned      YES unset  administratively down down
GigabitEthernet1/0/23  unassigned      YES unset  administratively down down
GigabitEthernet1/0/24  unassigned      YES unset  administratively down down
GigabitEthernet1/0/25  unassigned      YES unset  administratively down down
GigabitEthernet1/0/26  unassigned      YES unset  administratively down down
GigabitEthernet1/0/27  unassigned      YES unset  administratively down down
GigabitEthernet1/0/28  unassigned      YES unset  administratively down down
Port-channel1          unassigned      YES unset  up                    up
S1#sh vlan brief

VLAN Name                             Status    Ports
---- -------------------------------- --------- -------------------------------
1    default                          active    Gi1/0/3, Gi1/0/4, Gi1/0/5
                                                Gi1/0/7, Gi1/0/8, Gi1/0/9
                                                Gi1/0/10, Gi1/0/11, Gi1/0/12
                                                Gi1/0/13, Gi1/0/14, Gi1/0/15
                                                Gi1/0/16, Gi1/0/17, Gi1/0/18
                                                Gi1/0/19, Gi1/0/20, Gi1/0/21
                                                Gi1/0/22, Gi1/0/23, Gi1/0/24
                                                Gi1/0/25, Gi1/0/26, Gi1/0/27
                                                Gi1/0/28, Po1
7    London                           active
8    Swansea                          active
10   Birmingham                       active
22   Student                          active    Gi1/0/6
23   Teacher                          active
24   Management                       active
25   Library                          act/lshut
26   Native                           active
1002 fddi-default                     act/unsup
1003 token-ring-default               act/unsup
1004 fddinet-default                  act/unsup

VLAN Name                             Status    Ports
---- -------------------------------- --------- -------------------------------
1005 trnet-default                    act/unsup
S1#sh run
Building configuration...

Current configuration : 2428 bytes
!
! Last configuration change at 16:29:58 UTC Wed Aug 21 2024
!
version 15.2
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
service password-encryption
!
hostname S2
!
boot-start-marker
boot-end-marker
!
enable password 7 01100F175804575D72
!
username cisco privilege 15 password 7 01100F175804575D72
no aaa new-model
switch 1 provision c1000-24t-4g-l
system mtu routing 1500
!
!
no ip domain-lookup
ip domain-name swre-lab.com
!
!
!
!
!
!
!
!
spanning-tree mode rapid-pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
!
!
!
interface Port-channel1
!
interface GigabitEthernet1/0/1
 channel-group 1 mode active
!
interface GigabitEthernet1/0/2
 channel-group 1 mode active
!
interface GigabitEthernet1/0/3
 shutdown
!
interface GigabitEthernet1/0/4
 shutdown
!
interface GigabitEthernet1/0/5
 switchport trunk native vlan 26
 switchport mode trunk
 shutdown
!
interface GigabitEthernet1/0/6
!
interface GigabitEthernet1/0/7
 shutdown
!
interface GigabitEthernet1/0/8
 shutdown
!
interface GigabitEthernet1/0/9
 shutdown
!
interface GigabitEthernet1/0/10
 shutdown
!
interface GigabitEthernet1/0/11
 shutdown
!
interface GigabitEthernet1/0/12
 shutdown
!
interface GigabitEthernet1/0/13
 shutdown
!
interface GigabitEthernet1/0/14
 shutdown
!
interface GigabitEthernet1/0/15
 shutdown
!
interface GigabitEthernet1/0/16
 shutdown
!
interface GigabitEthernet1/0/17
 shutdown
!
interface GigabitEthernet1/0/18
 switchport access vlan 23
 switchport mode access
 switchport port-security maximum 3
 switchport port-security violation restrict
 switchport port-security
 shutdown
!
interface GigabitEthernet1/0/19
 shutdown
!
interface GigabitEthernet1/0/20
 shutdown
!
interface GigabitEthernet1/0/21
 shutdown
!
interface GigabitEthernet1/0/22
 shutdown
!
interface GigabitEthernet1/0/23
 shutdown
!
interface GigabitEthernet1/0/24
 shutdown
!
interface GigabitEthernet1/0/25
 shutdown
!
interface GigabitEthernet1/0/26
 shutdown
!
interface GigabitEthernet1/0/27
 shutdown
!
interface GigabitEthernet1/0/28
 shutdown
!
interface Vlan1
 no ip address
 shutdown
!
interface Vlan24
 ip address 192.168.110.3 255.255.255.0
!
ip default-gateway 192.168.110.1
ip http server
ip http secure-server
!
!
!
!
line con 0
 password 7 094F471A1A0A464058
 login
line vty 0 4
 login local
 transport input ssh
line vty 5 15
 login local
 transport input none
!
end

S2#sh ip int brief
Interface              IP-Address      OK? Method Status                Protocol
Vlan1                  unassigned      YES unset  administratively down down
Vlan24                 192.168.110.3   YES manual up                    down
GigabitEthernet1/0/1   unassigned      YES unset  up                    up
GigabitEthernet1/0/2   unassigned      YES unset  up                    up
GigabitEthernet1/0/3   unassigned      YES unset  administratively down down
GigabitEthernet1/0/4   unassigned      YES unset  administratively down down
GigabitEthernet1/0/5   unassigned      YES unset  administratively down down
GigabitEthernet1/0/6   unassigned      YES unset  down                  down
GigabitEthernet1/0/7   unassigned      YES unset  administratively down down
GigabitEthernet1/0/8   unassigned      YES unset  administratively down down
GigabitEthernet1/0/9   unassigned      YES unset  administratively down down
GigabitEthernet1/0/10  unassigned      YES unset  administratively down down
GigabitEthernet1/0/11  unassigned      YES unset  administratively down down
GigabitEthernet1/0/12  unassigned      YES unset  administratively down down
GigabitEthernet1/0/13  unassigned      YES unset  administratively down down
GigabitEthernet1/0/14  unassigned      YES unset  administratively down down
GigabitEthernet1/0/15  unassigned      YES unset  administratively down down
GigabitEthernet1/0/16  unassigned      YES unset  administratively down down
GigabitEthernet1/0/17  unassigned      YES unset  administratively down down
GigabitEthernet1/0/18  unassigned      YES unset  administratively down down
GigabitEthernet1/0/19  unassigned      YES unset  administratively down down
GigabitEthernet1/0/20  unassigned      YES unset  administratively down down
GigabitEthernet1/0/21  unassigned      YES unset  administratively down down
GigabitEthernet1/0/22  unassigned      YES unset  administratively down down
GigabitEthernet1/0/23  unassigned      YES unset  administratively down down
GigabitEthernet1/0/24  unassigned      YES unset  administratively down down
GigabitEthernet1/0/25  unassigned      YES unset  administratively down down
GigabitEthernet1/0/26  unassigned      YES unset  administratively down down
GigabitEthernet1/0/27  unassigned      YES unset  administratively down down
GigabitEthernet1/0/28  unassigned      YES unset  administratively down down
Port-channel1          unassigned      YES unset  up                    up
S2# sh vlan brief

VLAN Name                             Status    Ports
---- -------------------------------- --------- -------------------------------
1    default                          active    Gi1/0/3, Gi1/0/4, Gi1/0/5
                                                Gi1/0/6, Gi1/0/7, Gi1/0/8
                                                Gi1/0/9, Gi1/0/10, Gi1/0/11
                                                Gi1/0/12, Gi1/0/13, Gi1/0/14
                                                Gi1/0/15, Gi1/0/16, Gi1/0/17
                                                Gi1/0/19, Gi1/0/20, Gi1/0/21
                                                Gi1/0/22, Gi1/0/23, Gi1/0/24
                                                Gi1/0/25, Gi1/0/26, Gi1/0/27
                                                Gi1/0/28, Po1
7    London                           active
8    Swansea                          active
9    Management                       active
10   Birmingham                       active
22   Student                          active
23   Teacher                          active    Gi1/0/18
24   Management                       active
25   Library                          active
26   Native                           active
1002 fddi-default                     act/unsup
1003 token-ring-default               act/unsup

VLAN Name                             Status    Ports
---- -------------------------------- --------- -------------------------------
1004 fddinet-default                  act/unsup
1005 trnet-default                    act/unsup
S2#$l1          unassigned      YES unset  down                  down
               ^
% Invalid input detected at '^' marker.

S2#S1#show vl
    ^
% Invalid input detected at '^' marker.

S2#S1#show vlan br
    ^
% Invalid input detected at '^' marker.

S2#S1#show vlan brief
    ^
% Invalid input detected at '^' marker.

S2#
S2#VLAN Name                             Status    Ports
    ^
% Invalid input detected at '^' marker.

S2#$-------------------------- --------- -------------------------------
---- -------------------------------- --------- -------------------------------
^
% Invalid input detected at '^' marker.

S2#$t                          active    Gi1/0/25, Gi1/0/26, Gi1/0/27
   ^
% Invalid input detected at '^' marker.

S2#                                                Gi1/0/28
% Unknown command or computer name, or unable to find computer address
S2#7    London                           active    Gi1/0/6
   ^
% Invalid input detected at '^' marker.

S2#8    Swansea                          active
   ^
% Invalid input detected at '^' marker.

S2#9    Management                       active
   ^
% Invalid input detected at '^' marker.

S2#10   Birmingham                       active    Gi1/0/1, Gi1/0/2, Gi1/0/3
   ^
% Invalid input detected at '^' marker.

S2#                                                Gi1/0/4, Gi1/0/5, Gi1/0/7
                                                   ^
% Invalid input detected at '^' marker.

S2#                                                Gi1/0/8, Gi1/0/9, Gi1/0/10
                                                   ^
% Invalid input detected at '^' marker.

S2#$                                     Gi1/0/11, Gi1/0/12, Gi1/0/13
                                                   ^
% Invalid input detected at '^' marker.

S2#$                                     Gi1/0/14, Gi1/0/15, Gi1/0/16
                                                   ^
% Invalid input detected at '^' marker.

S2#$                                     Gi1/0/17, Gi1/0/18, Gi1/0/19
                                                   ^
% Invalid input detected at '^' marker.

S2#$                                     Gi1/0/20, Gi1/0/21, Gi1/0/22
                                                   ^
% Invalid input detected at '^' marker.

S2#                                                Gi1/0/23, Gi1/0/24
                                                   ^
% Invalid input detected at '^' marker.

S2#11   Native                           active
   ^
% Invalid input detected at '^' marker.

S2#1002 fddi-default                     act/unsup
   ^
% Invalid input detected at '^' marker.

S2#1003 token-ring-default               act/unsup
   ^
% Invalid input detected at '^' marker.

S2#1004 fddinet-default                  act/unsup
   ^
% Invalid input detected at '^' marker.

S2#1005 trnet-default                    act/unsup
   ^
% Invalid input detected at '^' marker.

S2#S1#
% Unknown command or computer name, or unable to find computer address
S2#R1#
% Unknown command or computer name, or unable to find computer address
S2#R1#
% Unknown command or computer name, or unable to find computer address
S2#R1#
% Unknown command or computer name, or unable to find computer address
S2#R1#
% Unknown command or computer name, or unable to find computer address
S2#R1#
% Unknown command or computer name, or unable to find computer address
S2#
S2#R1#show r
    ^
% Invalid input detected at '^' marker.

S2#R1#show ru
    ^
% Invalid input detected at '^' marker.

S2#R1#show run
    ^
% Invalid input detected at '^' marker.

S2#R1#show running-config
    ^
% Invalid input detected at '^' marker.

S2#Building configuration...
     ^
% Invalid input detected at '^' marker.

S2#
S2#Current configuration : 6756 bytes
    ^
% Invalid input detected at '^' marker.

S2#!
S2#! Last configuration change at 11:37:55 UTC Wed Aug 21 2024
S2#!
S2#version 17.9
      ^
% Invalid input detected at '^' marker.

S2#service timestamps debug datetime msec
     ^
% Invalid input detected at '^' marker.

S2#service timestamps log datetime msec
     ^
% Invalid input detected at '^' marker.

S2#service password-encryption
     ^
% Invalid input detected at '^' marker.

S2#! Call-home is enabled by Smart-Licensing.
S2#service call-home
     ^
% Invalid input detected at '^' marker.

S2#platform qfp utilization monitor load 80
    ^
% Invalid input detected at '^' marker.

S2#platform punt-keepalive disable-kernel-core
    ^
% Invalid input detected at '^' marker.

S2#!
S2#hostname R1
    ^
% Invalid input detected at '^' marker.

S2#!
S2#boot-start-marker
Translating "boot-start-marker"
% Unknown command or computer name, or unable to find computer address
S2#boot-end-marker
Translating "boot-end-marker"
% Unknown command or computer name, or unable to find computer address
S2#!
S2#!
S2#no aaa new-model
      ^
% Invalid input detected at '^' marker.

S2#!
S2#!
S2#!
S2#!
S2#!
S2#!
S2#!
S2#no ip domain lookup
          ^
% Invalid input detected at '^' marker.

S2#ip domain name swre-lab.com
       ^
% Invalid input detected at '^' marker.

S2#ip dhcp excluded-address 192.168.20.1 192.168.20.244
           ^
% Invalid input detected at '^' marker.

S2#!
S2#ip dhcp pool vlan2
           ^
% Invalid input detected at '^' marker.

S2# network 192.168.20.0 255.255.255.0
     ^
% Invalid input detected at '^' marker.

S2# default-router 192.168.20.1
      ^
% Invalid input detected at '^' marker.

S2# dns-server 8.8.8.8
     ^
% Invalid input detected at '^' marker.

S2#!
S2#!
S2#!
S2#login on-success log
         ^
% Invalid input detected at '^' marker.

S2#!
S2#!
S2#!
S2#!
S2#!
S2#!
S2#!
S2#subscriber templating
    ^
% Invalid input detected at '^' marker.

S2#vtp version 1
       ^
% Invalid input detected at '^' marker.

S2#multilink bundle-name authenticated
    ^
% Invalid input detected at '^' marker.

S2#!
S2#!
S2#!
S2#crypto pki trustpoint TP-self-signed-1574925342
              ^
% Invalid input detected at '^' marker.

S2# enrollment selfsigned
      ^
% Invalid input detected at '^' marker.

S2# subject-name cn=IOS-Self-Signed-Certificate-1574925342
     ^
% Invalid input detected at '^' marker.

S2# revocation-check none
      ^
% Invalid input detected at '^' marker.

S2# rsakeypair TP-self-signed-1574925342
      ^
% Invalid input detected at '^' marker.

S2#!
S2#crypto pki trustpoint SLA-TrustPoint
              ^
% Invalid input detected at '^' marker.

S2# enrollment pkcs12
      ^
% Invalid input detected at '^' marker.

S2# revocation-check crl
      ^
% Invalid input detected at '^' marker.

S2#!
S2#!
S2#crypto pki certificate chain TP-self-signed-1574925342
               ^
% Invalid input detected at '^' marker.

S2# certificate self-signed 01
     ^
% Invalid input detected at '^' marker.

S2#  30820330 30820218 A0030201 02020101 300D0609 2A864886 F70D0101 05050030
     ^
% Invalid input detected at '^' marker.

S2#  31312F30 2D060355 04031326 494F532D 53656C66 2D536967 6E65642D 43657274
     ^
% Invalid input detected at '^' marker.

S2#  69666963 6174652D 31353734 39323533 3432301E 170D3234 30383231 30383236
     ^
% Invalid input detected at '^' marker.

S2#  33335A17 0D333430 38323130 38323633 335A3031 312F302D 06035504 03132649
     ^
% Invalid input detected at '^' marker.

S2#  4F532D53 656C662D 5369676E 65642D43 65727469 66696361 74652D31 35373439
     ^
% Invalid input detected at '^' marker.

S2#  32353334 32308201 22300D06 092A8648 86F70D01 01010500 0382010F 00308201
     ^
% Invalid input detected at '^' marker.

S2#  0A028201 0100A687 02E78A91 82F59D4A B0A329A2 BAC72422 C079841F 7EEB1C2C
     ^
% Invalid input detected at '^' marker.

S2#  1CBF6E9A B65D62B2 C23CF41F 0AE8CF67 56A53050 34A5E4AA 5DA040BA 5518214D
     ^
% Invalid input detected at '^' marker.

S2#  3F8F6B4F 99B25553 22A928F3 D8EE802D 25CA329A 1FF09657 58E79890 3F5B96D0
     ^
% Invalid input detected at '^' marker.

S2#  89B6042E CCE38B1F 5252EA07 B1B0FE0D 1EBE34DD CE0D6DD6 EFBBD3F1 EEA38620
     ^
% Invalid input detected at '^' marker.

S2#  3C2A8FB0 6C3AF456 C05308A9 383A25F4 91B08A7F C1CC2080 93BCB47C 47BD1D18
     ^
% Invalid input detected at '^' marker.

S2#  78B3396C 707F393B 8E1D5E77 21DD8AE1 72B093F4 2DAD431A 59A128FB 80D0A984
     ^
% Invalid input detected at '^' marker.

S2#  EBCF3E29 18422629 2362E72B F0C199FB 0C5ED2E7 8BD9F0C8 97BC6098 2A95E65E
      ^
% Invalid input detected at '^' marker.

S2#  8537EA6C E7A4506E BAFD4A2F C97F00B5 B140EEE0 87CF45DF 19BD273A EC659083
     ^
% Invalid input detected at '^' marker.

S2#  E13B38C2 754B0203 010001A3 53305130 0F060355 1D130101 FF040530 030101FF
      ^
% Invalid input detected at '^' marker.

S2#  301F0603 551D2304 18301680 1459BB55 BE8A9AAA 885E289C B25A19F3 D10D25DC
     ^
% Invalid input detected at '^' marker.

S2#  01301D06 03551D0E 04160414 59BB55BE 8A9AAA88 5E289CB2 5A19F3D1 0D25DC01
     ^
% Invalid input detected at '^' marker.

S2#  300D0609 2A864886 F70D0101 05050003 82010100 100FD6EA BE02B4FE 29B89F73
     ^
% Invalid input detected at '^' marker.

S2#  712BA30D E768B7D1 9B548705 18DA081D 8D674394 2A960C4F 91D91837 1B7816F5
     ^
% Invalid input detected at '^' marker.

S2#  B8247640 B507D7FF 89FC72FB 4C96B9A6 64281DA2 5D8956DD 42BF7F67 2563810B
      ^
% Invalid input detected at '^' marker.

S2#  0B96E5FA 86DBEA29 BBF76E77 CEA565DC 7EBF51FA 94C22A9A 1550BC11 5F68A9B0
     ^
% Invalid input detected at '^' marker.

S2#  53921D45 9DF66E01 DE90D6E8 14370856 D496DA63 A6DD57E7 2CEF1F87 411AB837
     ^
% Invalid input detected at '^' marker.

S2#  A5F375A6 83186F12 1241370C C0E5480A FC0429E0 80ED50FE 091BE1CC 5D71202E
      ^
% Invalid input detected at '^' marker.

S2#  B71C9B7B 19F9C904 DE848EBB 51802468 63CC2FF1 44555C6E 31C513B1 DE6FCEDF
      ^
% Invalid input detected at '^' marker.

S2#  21643D0F 53C69888 A9788E8E B898E2F2 738F3B67 4BC69155 7387F8B3 B7240C4D
     ^
% Invalid input detected at '^' marker.

S2#  AC775511 6BD7DEF1 FBE522C1 0FF02F98 EB8A5BA8
       ^
% Invalid input detected at '^' marker.

S2#        quit

































S2 con0 is now available





Press RETURN to get started.












User Access Verification

Password:
R1#sh run
Building configuration...

Current configuration : 6502 bytes
!
! Last configuration change at 15:18:38 UTC Wed Aug 21 2024
!
version 17.9
service timestamps debug datetime msec
service timestamps log datetime msec
service password-encryption
! Call-home is enabled by Smart-Licensing.
service call-home
platform qfp utilization monitor load 80
platform punt-keepalive disable-kernel-core
!
hostname R1
!
boot-start-marker
boot-end-marker
!
!
no aaa new-model
!
!
!
!
!
!
!
ip domain name swre-lab.com
!
!
!
login on-success log
!
!
!
!
!
!
!
subscriber templating
vtp version 1
multilink bundle-name authenticated
!
!
!
crypto pki trustpoint TP-self-signed-3889378622
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-3889378622
 revocation-check none
 rsakeypair TP-self-signed-3889378622
!
crypto pki trustpoint SLA-TrustPoint
 enrollment pkcs12
 revocation-check crl
!
!
crypto pki certificate chain TP-self-signed-3889378622
 certificate self-signed 01
  30820330 30820218 A0030201 02020101 300D0609 2A864886 F70D0101 05050030
  31312F30 2D060355 04031326 494F532D 53656C66 2D536967 6E65642D 43657274
  69666963 6174652D 33383839 33373836 3232301E 170D3234 30383231 31333135
  32315A17 0D333430 38323131 33313532 315A3031 312F302D 06035504 03132649
  4F532D53 656C662D 5369676E 65642D43 65727469 66696361 74652D33 38383933
  37383632 32308201 22300D06 092A8648 86F70D01 01010500 0382010F 00308201
  0A028201 0100ACE1 876E0E2B 1ECDB5D8 19AC0920 E8C0AD6A F5E17BBE 4C015D2F
  3B7F5A2D 79A4248F 2653343F 604BDC77 DBF73FE1 68C6A088 09163237 07B8AA39
  29B7C21B 48F1B04C 06F6FA5D 6A5EECB6 5A2E5E43 9B7E3864 7C08D6C4 530867C6
  D872B680 7EC0A537 BC145B03 23C0930A A055B81B 15868C62 9C51EE06 F3184D54
  0B03676B C36E1FFB 4838EE30 FB6A2A65 8DC8DE25 5D657CB4 96D2BBA0 A01C785D
  8F88A431 768A56B8 1390FC9E 782B3218 431A409B A75894E3 9CC71E6F 23394DC7
  56279F8A 53DDDCE4 08D5109D A4995358 20872980 52ADE105 4312F45C 78447E02
  0E69D161 0DE21A7B F64DF7C6 7EFED911 A5741446 DDA8A0E7 D33BD19C 30EC7E96
  E259485C 5C950203 010001A3 53305130 0F060355 1D130101 FF040530 030101FF
  301F0603 551D2304 18301680 148E2851 B654347C 66ADFD91 C5E1115B DE3BA4C6
  87301D06 03551D0E 04160414 8E2851B6 54347C66 ADFD91C5 E1115BDE 3BA4C687
  300D0609 2A864886 F70D0101 05050003 82010100 411BDB3F EA6D3431 E204C3B7
  E4D64F10 29F2DE0A 5105AC0C 4EB1A8CE 155D6ACC B0AE84F7 0FA67028 58E51D77
  491FD56F AD612316 9D889266 D935C926 F1547A46 663E357B 26330B01 3FB05B33
  BC82C5BB 341E8A39 EAABC233 612CC04A 7BE638AE 0C2C1658 1682351D 7CDFFB07
  FEBB9893 04EE518A C3639264 BEDD9624 ED790409 115A80A6 FF89D26B 3868B22E
  1FA4F8A7 83441C86 B395BEF5 29475AB9 ED968576 2554A62A F6866708 85A721FC
  5CB19FCD 9754F8F3 5C09E7D3 A0AC9DFE 567B9D27 5DD951B1 B6A5FBB5 B7BE2359
  331B2E66 7A46DFA8 6B417A3E 54D5EAAB D2EFCD61 BC462007 057B7FF3 B7A74A3F
  342EE402 7CB247C2 50442475 4FA82B4A 7EB2CD51
        quit
crypto pki certificate chain SLA-TrustPoint
 certificate ca 01
  30820321 30820209 A0030201 02020101 300D0609 2A864886 F70D0101 0B050030
  32310E30 0C060355 040A1305 43697363 6F312030 1E060355 04031317 43697363
  6F204C69 63656E73 696E6720 526F6F74 20434130 1E170D31 33303533 30313934
  3834375A 170D3338 30353330 31393438 34375A30 32310E30 0C060355 040A1305
  43697363 6F312030 1E060355 04031317 43697363 6F204C69 63656E73 696E6720
  526F6F74 20434130 82012230 0D06092A 864886F7 0D010101 05000382 010F0030
  82010A02 82010100 A6BCBD96 131E05F7 145EA72C 2CD686E6 17222EA1 F1EFF64D
  CBB4C798 212AA147 C655D8D7 9471380D 8711441E 1AAF071A 9CAE6388 8A38E520
  1C394D78 462EF239 C659F715 B98C0A59 5BBB5CBD 0CFEBEA3 700A8BF7 D8F256EE
  4AA4E80D DB6FD1C9 60B1FD18 FFC69C96 6FA68957 A2617DE7 104FDC5F EA2956AC
  7390A3EB 2B5436AD C847A2C5 DAB553EB 69A9A535 58E9F3E3 C0BD23CF 58BD7188
  68E69491 20F320E7 948E71D7 AE3BCC84 F10684C7 4BC8E00F 539BA42B 42C68BB7
  C7479096 B4CB2D62 EA2F505D C7B062A4 6811D95B E8250FC4 5D5D5FB8 8F27D191
  C55F0D76 61F9A4CD 3D992327 A8BB03BD 4E6D7069 7CBADF8B DF5F4368 95135E44
  DFC7C6CF 04DD7FD1 02030100 01A34230 40300E06 03551D0F 0101FF04 04030201
  06300F06 03551D13 0101FF04 05300301 01FF301D 0603551D 0E041604 1449DC85
  4B3D31E5 1B3E6A17 606AF333 3D3B4C73 E8300D06 092A8648 86F70D01 010B0500
  03820101 00507F24 D3932A66 86025D9F E838AE5C 6D4DF6B0 49631C78 240DA905
  604EDCDE FF4FED2B 77FC460E CD636FDB DD44681E 3A5673AB 9093D3B1 6C9E3D8B
  D98987BF E40CBD9E 1AECA0C2 2189BB5C 8FA85686 CD98B646 5575B146 8DFC66A8
  467A3DF4 4D565700 6ADF0F0D CF835015 3C04FF7C 21E878AC 11BA9CD2 55A9232C
  7CA7B7E6 C1AF74F6 152E99B7 B1FCF9BB E973DE7F 5BDDEB86 C71E3B49 1765308B
  5FB0DA06 B92AFE7F 494E8A9E 07B85737 F3A58BE1 1A48A229 C37C1E69 39F08678
  80DDCD16 D6BACECA EEBC7CF9 8428787B 35202CDC 60E4616A B623CDBD 230E3AFB
  418616A9 4093E049 4D10AB75 27E86F73 932E35B5 8862FDAE 0275156F 719BB2F0
  D697DF7F 28
        quit
!
!
license udi pid C8200L-1N-4T sn FCZ2818R0M2
memory free low-watermark processor 62972
!
diagnostic bootup level minimal
!
spanning-tree extend system-id
!
enable password 7 02050D4808095E731F
!
username cisco privilege 15 password 7 030752180500701E1D
!
redundancy
 mode none
!
!
!
!
!
!
!
!
interface Loopback0
 ip address 209.165.101.1 255.255.255.224
!
interface GigabitEthernet0/0/0
 no ip address
 shutdown
 negotiation auto
!
interface GigabitEthernet0/0/1
 no ip address
 negotiation auto
!
interface GigabitEthernet0/0/1.22
 encapsulation dot1Q 22
 ip address 192.168.90.1 255.255.255.0
!
interface GigabitEthernet0/0/1.23
 encapsulation dot1Q 23
 ip address 192.168.100.1 255.255.255.0
!
interface GigabitEthernet0/0/1.24
 encapsulation dot1Q 24
 ip address 192.168.110.1 255.255.255.0
!
interface GigabitEthernet0/0/2
 no ip address
 shutdown
 negotiation auto
!
interface GigabitEthernet0/0/3
 no ip address
 shutdown
 negotiation auto
!
interface Serial0/1/0
 no ip address
 shutdown
!
interface Serial0/1/1
 no ip address
 shutdown
!
ip http server
ip http authentication local
ip http secure-server
ip forward-protocol nd
!
!
!
!
!
!
control-plane
!
!
line con 0
 password 7 121A0C0411045D5679
 login
 stopbits 1
line aux 0
line vty 0 4
 login local
 transport input ssh
line vty 5 15
 login local
 transport input ssh
!
call-home
 ! If contact email address in call-home is configured as sch-smart-licensing@cisco.com
 ! the email address configured in Cisco Smart License Portal will be used as contact email address to send SCH notifications.
 contact-email-addr sch-smart-licensing@cisco.com
 profile "CiscoTAC-1"
  active
  destination transport-method http
!
!
!
!
!
!
end

R1#sh ip int brief
Interface              IP-Address      OK? Method Status                Protocol
GigabitEthernet0/0/0   unassigned      YES unset  administratively down down
GigabitEthernet0/0/1   unassigned      YES unset  down                  down
Gi0/0/1.22             192.168.90.1    YES manual down                  down
Gi0/0/1.23             192.168.100.1   YES manual down                  down
Gi0/0/1.24             192.168.110.1   YES manual down                  down
GigabitEthernet0/0/2   unassigned      YES unset  administratively down down
GigabitEthernet0/0/3   unassigned      YES unset  administratively down down
Serial0/1/0            unassigned      YES unset  administratively down down
Serial0/1/1            unassigned      YES unset  administratively down down
Loopback0              209.165.101.1   YES manual up                    up
R1#
S1#sh run
Building configuration...

Current configuration : 2437 bytes
!
! Last configuration change at 16:32:36 UTC Wed Aug 21 2024
!
version 15.2
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
service password-encryption
!
hostname S1
!
boot-start-marker
boot-end-marker
!
enable password 7 05080F1C22431F5B4A
!
username cisco privilege 15 password 7 02050D4808095E731F
no aaa new-model
switch 1 provision c1000-24t-4g-l
system mtu routing 1500
!
!
no ip domain-lookup
ip domain-name swre-lab.com
!
shutdown vlan 25
!
!
!
!
!
!
!
!
spanning-tree mode rapid-pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
!
!
!
interface Port-channel1
!
interface GigabitEthernet1/0/1
 channel-group 1 mode active
!
interface GigabitEthernet1/0/2
 channel-group 1 mode active
!
interface GigabitEthernet1/0/3
 shutdown
!
interface GigabitEthernet1/0/4
 shutdown
!
interface GigabitEthernet1/0/5
 switchport trunk native vlan 26
 switchport mode trunk
 shutdown
!
interface GigabitEthernet1/0/6
 switchport access vlan 22
 switchport mode access
 switchport port-security maximum 3
 switchport port-security violation restrict
 switchport port-security
!
interface GigabitEthernet1/0/7
 shutdown
!
interface GigabitEthernet1/0/8
 shutdown
!
interface GigabitEthernet1/0/9
 shutdown
!
interface GigabitEthernet1/0/10
 shutdown
!
interface GigabitEthernet1/0/11
 shutdown
!
interface GigabitEthernet1/0/12
 shutdown
!
interface GigabitEthernet1/0/13
 shutdown
!
interface GigabitEthernet1/0/14
 shutdown
!
interface GigabitEthernet1/0/15
 shutdown
!
interface GigabitEthernet1/0/16
 shutdown
!
interface GigabitEthernet1/0/17
 shutdown
!
interface GigabitEthernet1/0/18
 shutdown
!
interface GigabitEthernet1/0/19
 shutdown
!
interface GigabitEthernet1/0/20
 shutdown
!
interface GigabitEthernet1/0/21
 shutdown
!
interface GigabitEthernet1/0/22
 shutdown
!
interface GigabitEthernet1/0/23
 shutdown
!
interface GigabitEthernet1/0/24
 shutdown
!
interface GigabitEthernet1/0/25
 shutdown
!
interface GigabitEthernet1/0/26
 shutdown
!
interface GigabitEthernet1/0/27
 shutdown
!
interface GigabitEthernet1/0/28
 shutdown
!
interface Vlan1
 no ip address
!
interface Vlan24
 ip address 192.168.110.2 255.255.255.0
!
ip default-gateway 192.168.110.1
ip http server
ip http secure-server
!
!
!
!
line con 0
 password 7 0822455D0A16544541
 login
line vty 0 4
 login local
 transport input ssh
line vty 5 15
 login local
 transport input none
!
end

S1#sh ip int brief
Interface              IP-Address      OK? Method Status                Protocol
Vlan1                  unassigned      YES unset  up                    up
Vlan24                 192.168.110.2   YES manual up                    down
GigabitEthernet1/0/1   unassigned      YES unset  up                    up
GigabitEthernet1/0/2   unassigned      YES unset  up                    up
GigabitEthernet1/0/3   unassigned      YES unset  administratively down down
GigabitEthernet1/0/4   unassigned      YES unset  administratively down down
GigabitEthernet1/0/5   unassigned      YES unset  administratively down down
GigabitEthernet1/0/6   unassigned      YES unset  down                  down
GigabitEthernet1/0/7   unassigned      YES unset  administratively down down
GigabitEthernet1/0/8   unassigned      YES unset  administratively down down
GigabitEthernet1/0/9   unassigned      YES unset  administratively down down
GigabitEthernet1/0/10  unassigned      YES unset  administratively down down
GigabitEthernet1/0/11  unassigned      YES unset  administratively down down
GigabitEthernet1/0/12  unassigned      YES unset  administratively down down
GigabitEthernet1/0/13  unassigned      YES unset  administratively down down
GigabitEthernet1/0/14  unassigned      YES unset  administratively down down
GigabitEthernet1/0/15  unassigned      YES unset  administratively down down
GigabitEthernet1/0/16  unassigned      YES unset  administratively down down
GigabitEthernet1/0/17  unassigned      YES unset  administratively down down
GigabitEthernet1/0/18  unassigned      YES unset  administratively down down
GigabitEthernet1/0/19  unassigned      YES unset  administratively down down
GigabitEthernet1/0/20  unassigned      YES unset  administratively down down
GigabitEthernet1/0/21  unassigned      YES unset  administratively down down
GigabitEthernet1/0/22  unassigned      YES unset  administratively down down
GigabitEthernet1/0/23  unassigned      YES unset  administratively down down
GigabitEthernet1/0/24  unassigned      YES unset  administratively down down
GigabitEthernet1/0/25  unassigned      YES unset  administratively down down
GigabitEthernet1/0/26  unassigned      YES unset  administratively down down
GigabitEthernet1/0/27  unassigned      YES unset  administratively down down
GigabitEthernet1/0/28  unassigned      YES unset  administratively down down
Port-channel1          unassigned      YES unset  up                    up
S1#sh vlan brief

VLAN Name                             Status    Ports
---- -------------------------------- --------- -------------------------------
1    default                          active    Gi1/0/3, Gi1/0/4, Gi1/0/5
                                                Gi1/0/7, Gi1/0/8, Gi1/0/9
                                                Gi1/0/10, Gi1/0/11, Gi1/0/12
                                                Gi1/0/13, Gi1/0/14, Gi1/0/15
                                                Gi1/0/16, Gi1/0/17, Gi1/0/18
                                                Gi1/0/19, Gi1/0/20, Gi1/0/21
                                                Gi1/0/22, Gi1/0/23, Gi1/0/24
                                                Gi1/0/25, Gi1/0/26, Gi1/0/27
                                                Gi1/0/28, Po1
7    London                           active
8    Swansea                          active
10   Birmingham                       active
22   Student                          active    Gi1/0/6
23   Teacher                          active
24   Management                       active
25   Library                          act/lshut
26   Native                           active
1002 fddi-default                     act/unsup
1003 token-ring-default               act/unsup
1004 fddinet-default                  act/unsup

VLAN Name                             Status    Ports
---- -------------------------------- --------- -------------------------------
1005 trnet-default                    act/unsup
S1#
% Bad passwords


































S2 con0 is now available





Press RETURN to get started.
















User Access Verification

Password:
S2>en
Password:
S2#sh run
Building configuration...

Current configuration : 2428 bytes
!
! Last configuration change at 16:29:58 UTC Wed Aug 21 2024
!
version 15.2
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
service password-encryption
!
hostname S2
!
boot-start-marker
boot-end-marker
!
enable password 7 01100F175804575D72
!
username cisco privilege 15 password 7 01100F175804575D72
no aaa new-model
switch 1 provision c1000-24t-4g-l
system mtu routing 1500
!
!
no ip domain-lookup
ip domain-name swre-lab.com
!
!
!
!
!
!
!
!
spanning-tree mode rapid-pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
!
!
!
interface Port-channel1
!
interface GigabitEthernet1/0/1
 channel-group 1 mode active
!
interface GigabitEthernet1/0/2
 channel-group 1 mode active
!
interface GigabitEthernet1/0/3
 shutdown
!
interface GigabitEthernet1/0/4
 shutdown
!
interface GigabitEthernet1/0/5
 switchport trunk native vlan 26
 switchport mode trunk
 shutdown
!
interface GigabitEthernet1/0/6
!
interface GigabitEthernet1/0/7
 shutdown
!
interface GigabitEthernet1/0/8
 shutdown
!
interface GigabitEthernet1/0/9
 shutdown
!
interface GigabitEthernet1/0/10
 shutdown
!
interface GigabitEthernet1/0/11
 shutdown
!
interface GigabitEthernet1/0/12
 shutdown
!
interface GigabitEthernet1/0/13
 shutdown
!
interface GigabitEthernet1/0/14
 shutdown
!
interface GigabitEthernet1/0/15
 shutdown
!
interface GigabitEthernet1/0/16
 shutdown
!
interface GigabitEthernet1/0/17
 shutdown
!
interface GigabitEthernet1/0/18
 switchport access vlan 23
 switchport mode access
 switchport port-security maximum 3
 switchport port-security violation restrict
 switchport port-security
 shutdown
!
interface GigabitEthernet1/0/19
 shutdown
!
interface GigabitEthernet1/0/20
 shutdown
!
interface GigabitEthernet1/0/21
 shutdown
!
interface GigabitEthernet1/0/22
 shutdown
!
interface GigabitEthernet1/0/23
 shutdown
!
interface GigabitEthernet1/0/24
 shutdown
!
interface GigabitEthernet1/0/25
 shutdown
!
interface GigabitEthernet1/0/26
 shutdown
!
interface GigabitEthernet1/0/27
 shutdown
!
interface GigabitEthernet1/0/28
 shutdown
!
interface Vlan1
 no ip address
 shutdown
!
interface Vlan24
 ip address 192.168.110.3 255.255.255.0
!
ip default-gateway 192.168.110.1
ip http server
ip http secure-server
!
!
!
!
line con 0
 password 7 094F471A1A0A464058
 login
line vty 0 4
 login local
 transport input ssh
line vty 5 15
 login local
 transport input none
!
end

S2#sh ip int brief
Interface              IP-Address      OK? Method Status                Protocol
Vlan1                  unassigned      YES unset  administratively down down
Vlan24                 192.168.110.3   YES manual up                    down
GigabitEthernet1/0/1   unassigned      YES unset  up                    up
GigabitEthernet1/0/2   unassigned      YES unset  up                    up
GigabitEthernet1/0/3   unassigned      YES unset  administratively down down
GigabitEthernet1/0/4   unassigned      YES unset  administratively down down
GigabitEthernet1/0/5   unassigned      YES unset  administratively down down
GigabitEthernet1/0/6   unassigned      YES unset  down                  down
GigabitEthernet1/0/7   unassigned      YES unset  administratively down down
GigabitEthernet1/0/8   unassigned      YES unset  administratively down down
GigabitEthernet1/0/9   unassigned      YES unset  administratively down down
GigabitEthernet1/0/10  unassigned      YES unset  administratively down down
GigabitEthernet1/0/11  unassigned      YES unset  administratively down down
GigabitEthernet1/0/12  unassigned      YES unset  administratively down down
GigabitEthernet1/0/13  unassigned      YES unset  administratively down down
GigabitEthernet1/0/14  unassigned      YES unset  administratively down down
GigabitEthernet1/0/15  unassigned      YES unset  administratively down down
GigabitEthernet1/0/16  unassigned      YES unset  administratively down down
GigabitEthernet1/0/17  unassigned      YES unset  administratively down down
GigabitEthernet1/0/18  unassigned      YES unset  administratively down down
GigabitEthernet1/0/19  unassigned      YES unset  administratively down down
GigabitEthernet1/0/20  unassigned      YES unset  administratively down down
GigabitEthernet1/0/21  unassigned      YES unset  administratively down down
GigabitEthernet1/0/22  unassigned      YES unset  administratively down down
GigabitEthernet1/0/23  unassigned      YES unset  administratively down down
GigabitEthernet1/0/24  unassigned      YES unset  administratively down down
GigabitEthernet1/0/25  unassigned      YES unset  administratively down down
GigabitEthernet1/0/26  unassigned      YES unset  administratively down down
GigabitEthernet1/0/27  unassigned      YES unset  administratively down down
GigabitEthernet1/0/28  unassigned      YES unset  administratively down down
Port-channel1          unassigned      YES unset  up                    up
S2# sh vlan brief

VLAN Name                             Status    Ports
---- -------------------------------- --------- -------------------------------
1    default                          active    Gi1/0/3, Gi1/0/4, Gi1/0/5
                                                Gi1/0/6, Gi1/0/7, Gi1/0/8
                                                Gi1/0/9, Gi1/0/10, Gi1/0/11
                                                Gi1/0/12, Gi1/0/13, Gi1/0/14
                                                Gi1/0/15, Gi1/0/16, Gi1/0/17
                                                Gi1/0/19, Gi1/0/20, Gi1/0/21
                                                Gi1/0/22, Gi1/0/23, Gi1/0/24
                                                Gi1/0/25, Gi1/0/26, Gi1/0/27
                                                Gi1/0/28, Po1
7    London                           active
8    Swansea                          active
9    Management                       active
10   Birmingham                       active
22   Student                          active
23   Teacher                          active    Gi1/0/18
24   Management                       active
25   Library                          active
26   Native                           active
1002 fddi-default                     act/unsup
1003 token-ring-default               act/unsup

VLAN Name                             Status    Ports
---- -------------------------------- --------- -------------------------------
1004 fddinet-default                  act/unsup
1005 trnet-default                    act/unsup
S2#
