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Figure 1 Conrod cap removal
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Figure 2 Torx socket and bolt
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Figure 3 Crankshaft removed ready for piston removal
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Figure 4 Measuring the bore of the cylinders
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Figure 5 Sheet used for recording measurements and doing calculations
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Engineceeaiation:
0.7854 xbore cm) xbore cm) xstroke (em) xnumber ofcylners =
07854 x(2:56.) (236, (5. %) xa  actus cc.





