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1.Summary 
This Method Statement outlines proposals for the road construction in the following location: 
· Langdon road
· New proposed road to development 

Where it is identified that there is a need to change the method of work due to unforeseen circumstances for example, then revision, authorisation and issue will follow the same procedure as the original. Any subcontractors will adhere to all current legislation and site guidelines, following any relevant standards to complete this task in the best manor. 

The scope of works for this project are as follows:
· Road Construction Langdon road
· Construction of a new development of retail and apartments in the SA1 
The new development construction will be covered in a separate method statement. 

Site fully secured with solid timber / steel hoarding with temporary works design to suit location 
· 6-meter-wide site gates will be required for plant and materials. 
· 1-meter-wide site pedestrian access gate will be provided where required. 
· Low-level pedestrian barriers will be located on site to segregate plant and materials from pedestrian routes. 
A gate man at all times to ensure the site is secured and deliveries controlled as they enter site. The gates man will also follow all covid guidelines and protocols for the site. 



1. Resources 
Materials 
· Type 1 stone 
· Kerbs 
· Sub-base 
· Tarmac 
· Made Ground 
· Gully Pots 
· Signage 
· Line Markings 
· Steel Pins 
· Timber Boards 
(Further Materials may be used and to be suggested by the site engineer prior to any works commencing).

Plant and Equipment 
· 10t 360o Excavator with various buckets and breaker attachment
· Rubber Duck
· GPS Guided D6 Dozer
· 135 Roller
· 13.5T Vibrating Roller
· 5t Dump Truck
· Car scan for tracing existing services
· Plate Compactor
· Spill kit for the plant
· Various Hand tools
· 100 ton mobile crane for steel erecting and modular units 
· Testing apparatus
· CAT4+ and Genny or equivalent/superior 
· Pipe Laser
· Generator for site set up
· Scaffolding 
· Safety nets for the roof and metal decking
· Rotating laser
· Air test kit
· Concrete pump 
· Pedestrian Barriers
· Disc cutter 
· 50mm pump
· Fuel bowser for the plant 
· Wacker plate
· Mobile road sweeper
· Trench and manhole support system
· Vibrating poker
· Kerb lifter 

All plant and equipment will be tested, tagged and registered prior to being used on site including accompanying lifting gear, e.g. chains, forklift attachment, shackles, etc Copies of Certification will be issued to the Works Manager so that a record is kept in the site office.
· No idling policy to be enforced – vehicles and plant to be switched off and secured when not in use.
· NRMM - Non-road mobile machinery must use ultra-low-sulphur diesel.
· NRMM- non-road mobile machinery - of engine power between 37kW - 560kW must conform to Tier IIIB European emission standard and be pre-notified to Fusion on the NRMM register.
· NRMM register must be provided prior to plant arriving on site.
· Stationary plant will be used with secondary containment measures such as plant nappies to retain any leakage of oil or fuel, which will be emptied at regular intervals to prevent overflow.
· Mobile spill kit to be kept on plant
· Daily plant inspections and pre-use checks will be carried out prior to work commencement and returned to the Works Manager on a weekly basis, these check sheets will be retained in the site files.
· Excavation inspection will also be carried out before each shift.
· Relevant Permit to load or recorded inspection of Temporary works to be carried out.
· Lifting permit will be issued to lift Manhole rings, Pipes and Trench/Manhole Boxes.

Personnel 

· Manager - SMSTS - Minimum
· Supervisor - SSSTS - Minimum
· Excavator Operatives - CPCS
· General Operatives – CSCS

· Full time Site Manager 
· Full time site labourer / gateman / covid officer 
· Building supervisor for internal works only 
· Visiting Contracts Manger 
· Visiting Quantity Surveyor 
· Visiting Design Manager 
· Sub-contractors  
It has been estimated that during the construction programmes busiest period there will be at least 26 operatives including site staff so the accommodation required will be as follows 
· 1 or 2 32x10 Open Plan Office (will need more space due to covid)  
· 1no 32x10 Meeting Room / Office 
· 1no 32x10 Canteen 
· 1no 32x10 Drying Room 
· 1No 3+1 Toilet Block and Tank if no mains drainage available. 
· 2 Steel Storage Containers 

Mandatory PPE for all persons on site
· Hard Hat, 
· High Visibility Vest or Coat (Orange – Full Sleeves)
· High Visibility Trousers (Orange)
· Lace up Boots with midsole and ankle protection- Rigger Boots are not an acceptable form of footwear.
· Cut 5 gloves  
· Light Eye Protection (LEP)

2. Permit Requirements 

· Permit to Dig 
· Permit to work/accessing beneath existing overhead services)
· EAP – Ecological Arboriculture Permit
· Confined Space Permit for classification (NC1, NC2) for generic standard method of safe working
· Lifting Permit
All relevant Permits to work will be issued by Databell Construction prior to works commencing. A copy will be held in Databell Construction Site File. 



3. Emergency Procedure 

· In the event of an emergency the work teams will follow the directions of the Databell Works Manager. Training on the correct emergency procedures will be briefed to operatives at Databell site Induction.
· Ensure no tools or equipment are left unattended. Pedestrian and emergency areas are to be kept clear for safe passage
· There will always be a member of the workforce with 3 Day First Aid at Work certification on site.
· In the event of a site wide emergency the team shall make safe the works area and proceed to the nearest assembly point.

Directions to the nearest hospital will be found in the appendix. 

4. Welfare Arrangements 

· Welfare will be provided in the main compound at SA1 development and will consist of the following.
· Hot and Cold running water
· Fresh Water (Drinking)
· Toilets both male and female
· Canteen
· Drying facilities
· Means to heat food
· Area of worship

This is not an exhaustive list and other facilities may be available.
Note that the following Welfare Requirements will comply with the water Resources technical standard
	[bookmark: _Hlk17193862]Facility
	Measure

	Toilet
	6 and 4 litres dual flush or;
4.5 litres single flush

	Shower
	8 litres/minute

	Hand basin
	5 litres/minute and a self-closing mechanism

	Kitchen taps
	flow rate of 5 litres/minute or less and trigger control is fitted to any pre-rinsing
facilities

	Urinals
	a flow rate of 3 litres/bowl/hour or less, or
hydraulic valves fitted to each urinal, or

	Dishwasher
	1.25 litres/place setting

	Washing machine
	8.17 litres/kilogram

	
	



5. Contact Information 
All relevant site personnel’s contact information will be available in the site office.

6. Interface with members of the public 
Majority of the work off Langdon road is wholly contained within the site boundary fencing and away from local residents and members of the public.
Should you have any interface with a member of the public or any person that you do not recognise be polite and direct them to Databell Construction management team. 
Do not engage with any person or persons you do not recognise or any member of the public.
Be polite at all time when dealing with any member if the public regardless of their attitude to you.
In the case of a security breach, STOP all works and ensure the area is made safe. Do not commence works again until instructed to do so by the Works Manager.

7. Methodology 
All traffic management shall be managed and installed by *** on behalf of Databell Construction. The traffic management provider will erect barriers around each defined works area, ensure both vehicles and pedestrians pass the works safely. At no point shall Databell alter the traffic management in any way; any alterations to TM shall be requested and approved in advance.

General Sequence
All site operatives must have received a Databell Construction site induction prior to starting work. 
Operatives will report to the site compound at the SA1 Site for a Daily Briefing prior to commencing works. As a minimum the daily briefing will include Traffic Management arrangements for the shift, access, egress and segregation measures for plant and pedestrians, daily risks, site operations and safety points.
Access to site will be gained via the existing site compound via A438 at Fabian Way to the site on Langdon road then via the existing haul routes. Deliveries will report to the site compound, receive a driver briefing and be escorted to the delivery point by Databell operatives. All deliveries are to report to the main compound before being escorted to the satellite site locations.
All plant operators will complete a daily inspection of the equipment, this inspection will be recorded daily and will be filed with the Works Manager every Friday.
The Site Registers will be updated every Tuesday morning by the Databell Works Manager.
All mobile plant, and the equipment will not be left unattended with the key in the ignition.
All power tools will be PAT tested on a 3-monthly basis.
· All excavated material to be reused as backfill for constructed carrier drainage. 
· If ground conditions allow all excavations to be stepped back or battered. Temporary Works design to be completed prior works commencement.
· For all excavation support systems Temporary Works design to be completed prior works commencement.
· Assembly and dismantle of support equipment to be done to manufacturers instruction and approved design. Manufacturer’s training to be provided for assembly, maintenance and dismantle of the systems. Temporary Works Co-ordinator/Supervisor to make sure compliance and design followed.
· Inspection of excavations by competent persons at the beginning of each shift and the end of each break to determine ground conditions and to ensure that the excavation remains safe. Excavation inspections to be recorded.
· Excavation edges to be protected with pedestrian barriers and appropriate signage to exclude unnecessary personnel from the area.
· For all Low Risk Confined Spaces (NC1, NC2), Confined Space trained personnel to be only allowed to enter such spaces. Rescue and emergency procedure to be followed in the event of emergency. 
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· Rescue procedure for Confined Space works will be developed at later date prior works commencement.
· Excavator will form 2:1 slope access area at the end of the trench for the access/extraction in case if an emergency and requirement of rescue procedure to be implemented.
· Interface between personnel and site vehicles/plant to be set up around works area by means of pedestrian/crowd barriers and maintained throughout the works. Accessing the work site with piece of machine will be done machine operator and banksman acknowledgement.

Identification of services prior to breaking ground
· Prior commencement of any intrusive works on site a Permit to Dig will be requested with Vision. 
· Vision Utilities specialist will review the locations and complete the initial scanning using CAT4+ and Genny or equivalent/superior scan in all three modes (power, radio and generator) then issue the Permit to Dig.
· All known services to be positively located and marked on ground with exclusion zones for each service.
· The Works Manager will brief the content of the permit to all personnel affected by the works. They will sign to confirm understanding of the conditions within.
· No mechanical means of excavation within exclusion zone unless dispensation and permission from service owner is in place. Always refer and adhere to methodology agreed with service owner.
· If possible, avoid working near over headlines, if that is not feasible communicate with service provider to isolate service during works near it.
· All works near OHL should be done safely, if they cannot be done safely, it should be not be done at all.
· Exclusion zone for working near OHL will be required to avoid arcing:
7m – 400kV-275kV
6m – 132kV
3m – 33kV-11kV (identified on site)
1m – LV
· Size and reach of machinery and plant to be taken to consideration and whether working near, under or just travelling under OHL should be well-thought-out.
· Goal posts (made from nonconductive material) will be installed at crossing points to appropriate design and distance (6m away) from OHL along with fencing to protect overhead services from machine interface and possible damage. It will be restricted to single vehicle width. 
· Warning signs of danger and maximum safe working height will be displayed on the goal posts. Additionally, blue cones will be placed either side of goal post.
· Machines travelling underneath services to have alarms warning the driver that the boom/jib/body is not stowed correctly.
· Machines working underneath or adjacent to OHL but capable of exceeding the maximum height or slew clearances to have electronic/mechanical restrictions on jibs/booms.
· Specific attention musts be paid when working in the hours of darkness especially during the winter season when limited hours of light are available to ensure that overhead services are adequately identified.

Trench Excavation & Pipe Laying
· Engineer to set out and mark drainage position, also control line and level during works 
· Trench excavation will be completed by 360 degree excavator specifically selected for the task/area constraint. 
· Consult Databell Construction to provide Permit to Dig.
· Vision to CAT scan the area to be excavated and verify location of services – mark additional services as required.
· Trenches shall be supported by the use of proprietary trench boxes as ground condition dictate (i.e. battering or stepping not possible). Where trench depths exceed 3.0m deep, additional top boxes shall be used. Trenches shall be dug to a depth of approximately 1.5m prior to the boxes being installed. All further digging shall be undertaken within the trench box, with the box being ‘pushed’ into the excavation at a rate commensurate with the excavation. Trench boxes (and manhole boxes) shall be lifted by means of dedicated lifting chains supplied with the boxes using 360 degree excavator. Lift Plan to be prepared and adhered to at all times. Temporary Works design to be completed prior works commencement.
· Where hard ground is being encountered (i.e. rock, concrete) during excavation process. Excavator equipped with breaker attachment will be used to remove the obstruction.
· Vision Service Locator to scan the area to make sure no services less than a 1m away from the obstruction and is to be scan every 300mm during the excavation.
· When breaker is detached from excavator, it will be placed on plant nappy to make sure ground is protected from any potential hydraulics leaks.
· Noise exclusion zone to be established around breaking out area by physically erecting crowd barriers and to be maintained throughout the duration of works.
· All personnel working or visiting in the vicinity of exclusion zone will wear hearing protection.
· No person shall enter the trench prior to the installation of the trench boxes. 
· Where, by the presence of services and other obstructions, it is not practical to use trench boxes, trench sides shall be supported by the use of traditional sheets and walers. Temporary Works design to be followed and manufacturer’s instructions.
· Trench boxes and trench sheets shall be sized such that they protrude sufficiently to form an edge barrier to the trench.

· Sufficient edge protection should be set up and maintained throughout the duration of works either by means of pedestrian barriers or proprietary system.
· Pipe bedding shall be placed within the trench by use of the excavator. Personnel shall then enter the trench by the use of the secured and tied ladder or proprietary access system and shall spread and level the bedding to receive the pipe. 
· In the event of ground water being encountered in the excavation a temporary sump will be positioned to one side of the excavation to a depth just below the pipe bedding. A suitable sized pump depending on the volume encountered will then be positioned at ground level to one side of the excavation with the suction hose feed into the sump. The pump will sit in a fuel drip tray to avoid any fuel contamination. The ground water will be pumped via a delivery hose into either of the following;
1. Pump the water in the field 
1. Pump the water to the holding pond.
1. Pump the water into a tanker.

Road Construction Process 

· Using the drawings provided by the design team, the engineer is to set out the position of the road using co-ordinates given.
· Profiles are then set out along the road to allow the excavation process to commence.
· All details required for the operatives will be written on the profiles as well as a verbal explanation so there is no confusion. 
· These profiles will be used together with a traveler to guide the excavator during the process of excavating down to formation level as shown in the image below. 
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· Any topsoil along the proposed route of the road will first be stripped using a hydraulic excavator or bulldozer.
· The topsoil will be stored in an appropriately located stockpile and kept for future landscaping needs on site. 
· Once the road, or a section of the road, has been excavated to formation level, the formation ground will first be assessed to ensure that it is in suitable condition.
· When deemed acceptable and all drainage or buried services have been installed, the road construction can begin. 
· At this stage it is the site engineers’ task to set out the kerb line using steel pins.
· Again, using the traveler, type 1 is then used as part of the sub-base, the depth of which is given to the operatives by the site engineer and labelled on the traveler.
· A roller is then used to ensure that the layer of type 1 is flat and to the correct level and then is ready for the next layer.
· Binder course tarmac is now ready to be laid by a separate sub-contractor and again the depth of that layer is given to them before their arrival on site so that the delivery for materials can be made. 
· When the base course is complete the kerb’s are then laid using a rubber duck with the help of operatives so that it complies with the health and safety measures as kerb’s often are heavy and can cause serious injury. 
· When the kerbs are installed, the wearing course can then be laid and like the previous layers the depth of this is pre-determined with the levels constantly being checked by the site engineer.
· The specification of the tarmac is given on the drawing specification given out by the designer.
· Once the road construction is complete this, remedial tasks can then take place, these being 
· Putting the line markings on the road
· Signage

Time, Money and Resource Management

· To maintain an efficient construction process, the number and size of excavators used will be assessed based on the layout and conditions of the site. Additionally, the number of dumpers or dump trucks used will be considered by assessing the time taken for the dumper to make its full journey to the stockpile and back, to keep the excavator working continuously.
· For example, if an excavator takes 5 minutes to excavate and load one dumper, and one dumper takes 10 minutes to return, then 3 dumpers will used, so that the 2nd and 3rd dumper will be loaded in the time taken for the 1st dumper to return.  
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· Existing levels from topographical survey drawings will be compared to proposed road levels, so that cut and fill operations can be carried out as efficiently as possible. 
· The profiles installed by the structural engineer can be used to determine where some excavated material can be used to fill other areas, reducing the volume of imported materials required.  
· Careful consideration will also be taken to ensure that stockpiles are appropriately located, out of the way of any future construction zones and within easy access for tipper lorries to be loaded for removal from site.  


8. Activity Specific Health and Safety requirements 
This is in Addition to the mandatory PPE explained in the site induction, hard hat, hi-vis, steel toe cap boots and gloves. 
· Additional PPE requirements 
· Hearing Protection whist using saw cutter and when using a breaker
· High impact eye protection and FFP3 dusk mask when using saw cutter and within proximity of breaking.
· The following additional training may be required
· CAT4+ and Genny or equivalent/superior scan in all three modes (power, radio and generator)
· Abrasive wheels training to use disc cutter

9. Activity Specific Environmental requirements

The following environmental monitoring is required:

· There will be spill kits made available at strategic points around the site, within the site vehicles and with each excavator.
· All Oil spills must be contained and cleaned up immediately and reported to the Site Manager, The Environmental Manager, and relevant authorities as appropriate. Fusion needs to be notified as soon as reasonably practicable.
· All materials shall be controlled and managed following the Site Waste Management Plan (SWMP). Waste must be adequately segregated and collected in designated skips. Minimise waste where possible. Tool box talks.
· Any used spill kits or contaminated waste will be double bagged and marked with the location, source of contaminant and type of contaminant if known. The contaminated material will be stored in a quarantine area within the site compound until it can be removed by a specialist removal company.
· Skips on site will be colour coded properly and appropriately signed. Skips will be covered from top by either a lid or sheet. It will be placed least 10m away from any watercourse or live drain.
· Daily briefing will identify of any potentially dust-emitting activities on site. A daily visual inspection will be made, and a record will be kept site file of whether there is a risk of dust emissions that day. Where required, dust will be dampened down with means of water where necessary to limit dust.
· Material stockpiles likely to generate dust will be enclosed if possible or kept watered as appropriate.
· Site speed limit will be briefed and asked to adhere to all operatives to limit noise and dust.
· Noise and nuisance will be controlled by making sure any plant emitting noise to be turned off when not in use.
· Spill kit to be kept with diesel bowser and on mobile plant.
· Any excavations left overnight will be covered to stop any wildlife entering the excavation. 
· All materials and wastes shall be controlled and managed in line with the Resource management Plan and SWMP.
· Any timber and wood products will be certified as from a sustainable source (FSC/PEFC) with full chain custody. 
· Fencing to be placed to ensure the protection of retained trees/hedgerows or other ecological features. (Retained trees to be protected in line with BS5738).
· EAP must be in place prior to any works.
· Any excavations left overnight must be covered or with access/egress ramps for any wildlife that may enter 
· Areas of soil around features to be protected from construction activities including retained trees, and archaeology shall be clearly marked out by barrier tape and exclusion signs. To be confirmed with the team where this is required for archaeology.

10. Review and Monitoring 
The method statement will be consistently reviewed and updated so that it is entirely up to date throughout the project duration.


11. Method Statement Briefing Log 
I/We* the undersigned have been given, and fully understood, the briefing of the contents of this method statement.
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12. Appendix – Nearest Hospital 
Singleton Hospital
Telephone Number: 01792 205666
Address: Sketty Lane, Sketty SA2 8QA
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Reference Assets.publishing.service.gov.uk. 2021. [online] Available at: <https://assets.publishing.service.gov.uk/government/uploads/system/uploads/attachment_data/file/935988/20201113_JSP375_Vol3_Chapter_06_Safety_Rule_Book_Confined_Spaces.pdf> [Accessed 21 April 2021].
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