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R1#show config
Using 1605 out of 33554432 bytes
!
! Last configuration change at 15:33:00 UTC Tue Dec 12 2000
!
version 16.9
service timestamps debug datetime msec
service timestamps log datetime msec
service password-encryption
platform qfp utilization monitor load 80
no platform punt-keepalive disable-kernel-core
!
hostname R1
!
boot-start-marker
boot-end-marker
!
!
enable secret 5 $1$v3nw$K6FGOcoDM4Ms23IsQ6Dl51
enable password 7 01100F175804
!
no aaa new-model
!
no ip domain lookup
 --More--
ip admission watch-list expiry-time 0
!
!
!
!
!
!
!
!
!
!
subscriber templating
multilink bundle-name authenticated
!
!
!
crypto pki trustpoint TP-self-signed-1020466531
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-1020466531
 revocation-check none
 rsakeypair TP-self-signed-1020466531
!
!
crypto pki certificate chain TP-self-signed-1020466531
 certificate self-signed 01 nvram:IOS-Self-Sig#6.cer
!
license udi pid ISR4221/K9 sn FGL224190DM
no license smart enable
diagnostic bootup level minimal
!
spanning-tree extend system-id
!
!
!
!
redundancy
 mode none
!
!
!
!
!
!
!
!
interface GigabitEthernet0/0/0
 description pc11
 ip address 172.16.10.1 255.255.255.0
 shutdown
 negotiation auto
!
interface GigabitEthernet0/0/1
 description pc12
 ip address 172.12.11.1 255.255.255.0
 shutdown
 negotiation auto
!
interface Serial0/1/0
!
interface Serial0/1/1
!
ip forward-protocol nd
ip http server
ip http authentication local
ip http secure-server
!
!
!
!
!
!
control-plane
!
banner motd ^CUnautorized access is prohibited^C
!
line con 0
 password 7 0822455D0A16
 login
 transport input none
 stopbits 1
line vty 0 4
 login
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S1#show config
Using 1453 out of 65536 bytes
!
! Last configuration change at 00:49:11 UTC Mon Mar 1 1993
!
version 15.2
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname S1
!
boot-start-marker
boot-end-marker
!
!
no aaa new-model
system mtu routing 1500
!
!
!
!
!
 --More--
!
!
no ip domain-lookup
!
!
!
spanning-tree mode pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
!
!
!
interface FastEthernet0/1
!
interface FastEthernet0/2
!
interface FastEthernet0/3
!
interface FastEthernet0/4
!
interface FastEthernet0/5
!
interface FastEthernet0/6
!
interface FastEthernet0/7
!
interface FastEthernet0/8
!
interface FastEthernet0/9
!
interface FastEthernet0/10
!
interface FastEthernet0/11
!
interface FastEthernet0/12
!
interface FastEthernet0/13
!
interface FastEthernet0/14
!
interface FastEthernet0/15
!
interface FastEthernet0/16
!
interface FastEthernet0/17
!
interface FastEthernet0/18
!
interface FastEthernet0/19
!
interface FastEthernet0/20
!
interface FastEthernet0/21
!
interface FastEthernet0/22
!
interface FastEthernet0/23
!
interface FastEthernet0/24
!
interface GigabitEthernet0/1
!
interface GigabitEthernet0/2
!
interface Vlan1
 ip address 172.16.11.10 255.255.255.0
!
ip default-gateway 172.16.11.1
ip http server
ip http secure-server
!
no vstack
banner motd ^CAuthorized Access Only^C
!
line con 0
 password letmein
 login
line vty 0 4
 login
line vty 5 15
 login
!
end
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R1#show ip int brief
Any interface listed with OK? value "NO" does not have a valid configuration

Interface              IP-Address      OK? Method Status                Protocol
GigabitEthernet0/0/0   172.16.10.1     YES manual administratively down down
GigabitEthernet0/0/1   172.12.11.1     YES manual administratively down down
Serial0/1/0            unassigned      NO  unset  down                  down
Serial0/1/1            unassigned      NO  unset  down                  down
R1#


S1#ÿsÿhow ip iÿnt brkef
Interface              IP-Address      OK? Method Status                Protocol
Vlan1                  172.16.11.10    YES manual up                    up
FastEthernet0/1        unassigned      YES unset  down                  down
FastEthernet0/2        unassigned      YES unset  down                  down
FastEthernet0/3        unassigned      YES unset  down                  down
FastEthernet0/4        unassigned      YES unset  down                  down
FastEthernet0/5        unassigned      YES unset  down                  down
FastEthernet0/6        unassigned      YES unset  down                  down
FastEthernet0/7        unassigned      YES unset  down                  down
FastEthernet0/8        unassigned      YES unset  down                  down
FastEthernet0/9        unassigned      YES unset  down                  down
FastEthernet0/10       unassigned      YES unset  up                    up
FastEthernet0/11       unassigned      YES unset  down                  down
FastEthernet0/12       unassigned      YES unset  down                  down
FastEthernet0/13       unassigned      YES unset  down                  down
FastEthernet0/14       unassigned      YES unset  down                  down
FastEthernet0/15       unassigned      YES unset  down                  down
FastEthernet0/16       unassigned      YES unset  down                  down
FastEthernet0/17       unassigned      YES unset  down                  down
FastEthernet0/18       unassigned      YES unset  down                  down
FastEthernet0/19       unassigned      YES unset  down                  down
FastEthernet0/20       unassigned      YES unset  down                  down
FastEthernet0/21       unassigned      YES unset  down                  down
FastEthernet0/22       unassigned      YES unset  down                  down
FastEthernet0/23       unassigned      YES unset  down                  down
FastEthernet0/24       unassigned      YES unset  down                  down
GigabitEthernet0/1     unassigned      YES unset  down                  down
[bookmark: _GoBack]GigabitEthernet0/2     unassigned      YES unset  down                  down
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