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	Site Specific Activity and Control Measures        

                                     (This section must be completed)


	Method
	Laying of asphalt

	
	Location
	Car Park and Access road

	
	Duration
	2 days

	
	Control
	RA/MS briefing

	Exposure Limits


	5mg/m3 8hr TWA – asphalt, petroleum fumes



	Physical Properties
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	Mixture of aggregates and bitumen.  Supplied at temperatures up to 190°C.

Bitumen is a hydrocarbon derived from the distillation of petroleum crude oil.



	Hazard
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	Skin burns from hot material

Inhalation of fumes in confined spaces

	
	
	

	Work Procedures/PPE
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	Heavy duty, heat resistant gloves - BS EN 374, 388, 511 footwear and overalls

Eye goggles – BS EN166 F

Ensure adequate ventilation during application

Maintain a high standard of personal hygiene.

Restrict public access during application and until set

	First Aid/Fire
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	Skin Contact: cool rapidly in cold water, do not attempt to remove material unless constriction occurs, cover in sterile dressing, seek immediate medical attention. See Bitumen Burns – First Aid Guidance
Ingestion: not considered likely 

Eye Contact: irrigate with plenty of cold water for at least 15 minutes, do not remove material – seek medical attention

Inhalation: remove to fresh air and rest. Seek medical attention if symptoms persist. 

Fire: use dry powder / foam / sand 

	Storage/Disposal
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	Storage: normally supplied in insulated lorries

Disposal: in accordance with legislative and company requirements

	Environmental
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	Spillage: Shovel up for use if possible. Wear PPE as above. Material will set in solid mass/lumps when cooled. May require mechanical breaking up for disposal.

Prevent material entering drains – will cause blockages.
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