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This is an individual practical lab-test, held under examination conditions. You will be assigned 3 Routers, 2 Switches and two PCs; you should configure these devices based on the following specifications. 
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TOPOLOGY DIAGRAM
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	Switch 1 Ports to VLAN

Fa0/2 to 0/7  - VLAN 5
Fa0/8 to 0/14  - VLAN 6
Fa0/15 to 0/20 - VLAN 7
Fa0/21 to 0/24  - VLAN 8
	Switch 2 Ports to VLAN

Fa0/2 to 0/7  - VLAN 5
Fa0/8 to 0/14  - VLAN 6
Fa0/15 to 0/20 - VLAN 7
Fa0/21 to 0/24  - VLAN 8.




















Task 1: IP addressing scheme(5 marks)

	Device
	Interface
	IP Address
	Subnet Mask
	IPv6 Address

	HQ
	Ge0/0
	
	255.255.255.0
	

	
	
	
	
	Link-local:

	
	S0/0/0
	
	255.255.255.252
	

	
	
	
	
	Link-local:

	
	S0/0/1
	
	255.255.255.252
	

	
	
	
	
	Link-local:

	
	Lo1
	
	255.255.255.0
	

	Branch 1
	S0/0/1
	
	255.255.255.252
	

	
	
	
	
	Link-local:

	
	Lo2
	
	255.255.255.0
	

	
	Lo3
	
	255.255.255.0
	

	
	Lo4
	
	255.255.255.0
	

	
	Lo5
	
	255.255.255.0
	

	
	
	
	
	

	
	L06
	
	255.255.255.0
	

	
	
	
	
	Link-local:

	
	Gi0/0
	
	255.255.255.0
	

	
	
	
	255.255.255.0
	

	
	
	
	255.255.255.0
	

	
	
	
	255.255.255.0
	

	
	
	
	255.255.255.0
	

	
	
	
	255.255.255.0
	

	Branch 2
	S0/0/0
	
	255.255.255.0
	

	
	
	
	
	Link-local:

	
	Lo11
	
	255.255.255.0
	

	
	Lo12
	
	255.255.255.0
	

	
	Lo13
	
	255.255.255.0
	

	
	Lo6
	
	255.255.255.0
	

	
	Lo7
	
	255.255.255.0
	

	S1
	VLAN9
	
	255.255.255.0
	

	S2
	VLAN9
	
	255.255.255.0
	

	Internet Server
	
	
	255.255.255.0
	

	
	
	
	
	Link-local:



	

Task 2: Network Connection (5Marks)
	
Using Packet Tracer software create the topology shown above and complete all task below. 


Task 3: Configure the basic configuration (10 Marks)

1. Configure all devices with hostname
2. Disable DNS lookup
3. Configure all devices with interfaces as shown in the topology. 
4. Configure Internet PC with IPv4 and IPv6 address. 
Part 2: 


Task 4: Configure Routers and Switches (65 marks)

1. Configure RIPv2 on all routers and advertise networks shown in the topology. Disable auto summary.
2. Configure IPv6 static route with exit interface on all routers. 
3. On HQ, configure IPV4 and IPv6 default route out Gi0/0 
4. On S1 and S2, configure VLANs
5. Assign the IPv4 address to Management VLAN on S1 and S2. 
6. Assign default gateway on switches
7. On S1, force trunking on Gi0/0 and Fa0/1. Use VLAN1 as the Native VLAN
8. on S2, force trunking on Fa0/1. Use VLAN1 as the Native VLAN. 
9. On S1, assign Fa0/6 to VLAN21 and on S2, assign Fa0/18 to VLAN23.
10. On both switches, shutdown all unused ports.
11. Configure Router-on-Stick inter-VLAN routing.
12. On all Routers, configure all Loopback and Ethernet interfaces as passive.  
13. Configure Branch1 as the DHCP server for VLANs 5 to 8. Reserve first 10 IP addresses for static configurations. 

	VLAN 5
Name: Research
DNS-Server: 1.1.1.1
Domain-Name: SoAC.com
Set the default gateway
	VLAN 6
Name: Technical
DNS-Server: 1.1.1.1
Domain-Name: SoAC.com
Set the default gateway
	VLAN 7
Name: Sales
DNS-Server: 1.1.1.1
Domain-Name: SoAC.com
Set the default gateway
	VLAN 8
Name: HR
DNS-Server: 1.1.1.1
Domain-Name: SoAC.com
Set the default gateway



14. Create a local database with 1 user account: username: webuser, password: soac1234, privilege: 15. 
15. On HQ, configure a static NAT to the Web Server. Use the inside global address 209.165.200.26. Assign the inside and outside interface for static NAT.
16. Configure the dynamic NAT. Allow VLAN 5 and 6 networks on Branch 1to be translated. 
17. Define the pool of usable public IP addresses, 209.165.200.225 to 209.165.200.228.
18. Define the dynamic NAT translation. 


Task 5: Verify connectivity(15 marks)

After configuring each host computer, record the host network settings with the ipconfig /all command. 


	Host PC-A Network Configuration

	Description
	

	Physical Address
	

	IP Address
	192.168.5.11

	Subnet Mask
	255.255.255.0

	Default Gateway
	192.168.6.1






	Host PC-B Network Configuration

	Description
	

	Physical Address
	

	IP Address
	192.168.6.11

	Subnet Mask
	255.255.255.0

	Default Gateway
	192.168.6.1




Verify PC-A can ping PC-B. Is it successful? __________________

Use a Web browser on the Internet PC to access the Web Server (209.165.200.26). Login with Username: webuser and password: soac1234.
Is the Web server accessible? _____________________________


Submission Requirement
The packet tracer file should be saved as“studentname_id” anduploaded on Moodle. In addition to packet tracer file, you mustalso submit 
· the output of show running-configuration command in a text file for all devices configured. 
· [bookmark: _GoBack]This document with task 1 and task 5 completed 

All documentation for your solution should be submitted electronically on Moodle.
It is your responsibility that you submit all the outputs and files correctly.
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‘Name No  IPv4 Address
Research 5  192.168.5.0/24
Technical 6  192.168.6.0/24
Sales 7 192.168.7.0/26
HR 8  192.168.8.0/28
MGMT 9 192.168.9.0/27





