Ion Gabriel Matei_1816251

Switch configuration:


S1 con0 is now available





Press RETURN to get started.














This is my switch
S1>en
S1#show run
Building configuration...

Current configuration : 1446 bytes
!
! Last configuration change at 21:35:40 UTC Thu Mar 11 1993
!
version 15.0
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname S1
!
boot-start-marker
boot-end-marker
!
!
no aaa new-model
system mtu routing 1500
!
!
no ip domain-lookup
!
!
!
!
!
!
!
!
spanning-tree mode pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
!
!
!
interface FastEthernet0/1
!
interface FastEthernet0/2
!
interface FastEthernet0/3
!
interface FastEthernet0/4
!
interface FastEthernet0/5
!
interface FastEthernet0/6
!
interface FastEthernet0/7
!
interface FastEthernet0/8
!
interface FastEthernet0/9
!
interface FastEthernet0/10
!
interface FastEthernet0/11
!
interface FastEthernet0/12
!
interface FastEthernet0/13
!
interface FastEthernet0/14
!
interface FastEthernet0/15
!
interface FastEthernet0/16
!
interface FastEthernet0/17
!
interface FastEthernet0/18
!
interface FastEthernet0/19
!
interface FastEthernet0/20
!
interface FastEthernet0/21
!
interface FastEthernet0/22
!
interface FastEthernet0/23
!
interface FastEthernet0/24
!
interface GigabitEthernet0/1
!
interface GigabitEthernet0/2
!
interface Vlan1
 ip address 172.16.11.10 255.255.255.0
!
ip default-gateway 172.16.11.1
ip http server
ip http secure-server
!
banner motd ^CThis is my switch^C
!
line con 0
line vty 0 4
 password cisco
 login
line vty 5 15
 password cisco
 login
!
end

S1#sh ip int brief
Interface              IP-Address      OK? Method Status                Protocol
Vlan1                  172.16.11.10    YES manual up                    up
FastEthernet0/1        unassigned      YES unset  down                  down
FastEthernet0/2        unassigned      YES unset  down                  down
FastEthernet0/3        unassigned      YES unset  down                  down
FastEthernet0/4        unassigned      YES unset  down                  down
FastEthernet0/5        unassigned      YES unset  up                    up
FastEthernet0/6        unassigned      YES unset  up                    up
FastEthernet0/7        unassigned      YES unset  down                  down
FastEthernet0/8        unassigned      YES unset  down                  down
FastEthernet0/9        unassigned      YES unset  up                    up
FastEthernet0/10       unassigned      YES unset  up                    up
FastEthernet0/11       unassigned      YES unset  down                  down
FastEthernet0/12       unassigned      YES unset  up                    up
FastEthernet0/13       unassigned      YES unset  down                  down
FastEthernet0/14       unassigned      YES unset  down                  down
FastEthernet0/15       unassigned      YES unset  down                  down
FastEthernet0/16       unassigned      YES unset  down                  down
FastEthernet0/17       unassigned      YES unset  down                  down
FastEthernet0/18       unassigned      YES unset  down                  down
FastEthernet0/19       unassigned      YES unset  down                  down
FastEthernet0/20       unassigned      YES unset  down                  down
FastEthernet0/21       unassigned      YES unset  down                  down
FastEthernet0/22       unassigned      YES unset  down                  down
FastEthernet0/23       unassigned      YES unset  down                  down
FastEthernet0/24       unassigned      YES unset  down                  down
GigabitEthernet0/1     unassigned      YES unset  down                  down
GigabitEthernet0/2     unassigned      YES unset  down                  down
S1#
S1#
S1#

Router configuration:

R1#sh run
Building configuration...

Current configuration : 286299 bytes
!
! Last configuration change at 13:28:39 UTC Mon Aug 19 2019
!
version 15.4
service timestamps debug datetime msec
service timestamps log datetime msec
service password-encryption
!
hostname R1
!
boot-start-marker
boot-end-marker
!
!
enable secret 5 $1$FHBQ$BurP.Q0xksXFLQnJVWhBR/
!
no aaa new-model
!
!
!
!
 --More—
!
no ip domain lookup
ip cef
no ipv6 cef
multilink bundle-name authenticated
!
!
cts logging verbose
!
!
crypto pki certificate pool

nterface Embedded-Service-Engine0/0
 no ip address
 shutdown
!
interface GigabitEthernet0/0
 ip address 172.16.10.1 255.255.255.0
 duplex auto
 speed auto
!
interface GigabitEthernet0/1
 ip address 172.16.11.1 255.255.255.0
 duplex auto
 speed auto
!
interface Serial0/0/0
 no ip address
 shutdown
 clock rate 2000000
!
interface Serial0/0/1
 no ip address
 shutdown
 clock rate 2000000
!
ip forward-protocol nd
!
no ip http server
no ip http secure-server
!
!
!
!
!
control-plane
!
!
banner motd ^C Unauthorized access is prohibited^C
!
line con 0
 exec-timeout 0 0
 password 7 104D000A0618
 login
line aux 0
line 2
 no activation-character
 no exec
 transport preferred none
 transport output pad telnet rlogin lapb-ta mop udptn v120 ssh
 stopbits 1
line vty 0 4
 password 7 1511021F0725
 login
 transport input none
line vty 5 15
 password 7 1511021F0725
 login
 transport input none
!
scheduler allocate 20000 1000
ntp server pnpntpserver.campus.local
!
End
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:\Users\Admin>ping 172.16.10.1

inging 172.16.10.1 with 32 bytes of data:
eply from 172.
eply from 172.
eply from 172.16.10.1: bytes=32 time-ms
eply from 172.16.10.1: bytes=32 time-1ms

ing statistics for 172.16.10.1:
Packets: Sent = 4, Received = 4, Lost = © (8% loss),
pproximate round trip times in milli-second:
Minimum = ims, Maximum = ims, Average = ims

:\Users\Adnin>ping 172.16.11.1

inging 172.16.11.1 with 32 bytes of data:
eply from 172.16.11.1: bytes=32 time<ims
eply from 172.16.11.1: bytes=32 time-1ms
eply from 172.16.11.1: bytes=32 time-1ms
eply from 172.16.11.1: bytes=32 time-1ms

ing statistics for 172.16.11.1
Packets: Sent = 4, Received = 4, Lost = © (8% loss),
pproximate round trip times in milli-seconds:
Minimum = ems, Maximum = ims, Average = 6ms

:\Users\Admin>ping 172.16.11.254

inging 172.16.11.254 with 32 bytes of data:
eply from 172.16.11.254: bytes=32 time<ims TTL=128
eply from 172.16.11.254: bytes=32 time<ims
eply from 172.16.11.254: bytes=32 time<ims
eply from 172.16.11.254: bytes=32 time<ims TTL=128

ing statistics for 172.16.11.254:
Packets: Sent = 4, Received = 4, Lost = © (8% loss),
pproximate round trip times in milli-second:
Minimum = @ms, Maximum = ems, Average = 6ms

:\Users\Adnin>ping 172.16.16.254

inging 172.16.10.254 with 32 bytes of data:
equest timed out.
equest timed out.
equest timed out.
equest timed out.




