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Switch 1
Current configuration : 2109 bytes
!
version 12.2
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname S1
!
!
!
no ip domain-lookup
!
!
spanning-tree mode pvst
spanning-tree extend system-id
!
interface FastEthernet0/1
 switchport mode trunk
!
interface FastEthernet0/2
 switchport access vlan 5
 shutdown
!
interface FastEthernet0/3
 switchport access vlan 5
 shutdown
!
interface FastEthernet0/4
 switchport access vlan 5
 shutdown
!
interface FastEthernet0/5
 switchport access vlan 5
 shutdown
!
interface FastEthernet0/6
 switchport access vlan 5
 switchport mode trunk
 shutdown
!
interface FastEthernet0/7
 switchport access vlan 5
 shutdown
!
interface FastEthernet0/8
 switchport access vlan 6
 shutdown
!
interface FastEthernet0/9
 switchport access vlan 6
 shutdown
!
interface FastEthernet0/10
 switchport access vlan 6
 shutdown
!
interface FastEthernet0/11
 switchport access vlan 6
 shutdown
!
interface FastEthernet0/12
 switchport access vlan 6
 shutdown
!
interface FastEthernet0/13
 switchport access vlan 6
 shutdown
!
interface FastEthernet0/14
 switchport access vlan 6
!
interface FastEthernet0/15
 switchport access vlan 7
 shutdown
!
interface FastEthernet0/16
 switchport access vlan 7
 shutdown
!
interface FastEthernet0/17
 switchport access vlan 7
 shutdown
!
interface FastEthernet0/18
 switchport access vlan 7
 shutdown
!
interface FastEthernet0/19
 switchport access vlan 7
 shutdown
!
interface FastEthernet0/20
 switchport access vlan 7
 shutdown
!
interface FastEthernet0/21
 switchport access vlan 8
 shutdown
!
interface FastEthernet0/22
 switchport access vlan 8
 shutdown
!
interface FastEthernet0/23
 switchport access vlan 8
 shutdown
!
interface FastEthernet0/24
 switchport access vlan 8
 shutdown
!
interface GigabitEthernet0/1
 switchport mode trunk
!
interface GigabitEthernet0/2
 shutdown
!
interface Vlan1
 no ip address
 shutdown
!
interface Vlan5
 mac-address 0060.2f16.3501
 ip address 192.168.5.10 255.255.255.0
!
ip default-gateway 192.168.1.1
!
!
!
!
line con 0
!
line vty 0 4
 login
line vty 5 15
 login
!
!
!
!
End

Switch 2
Current configuration : 2111 bytes
!
version 12.2
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname S2
!
!
!
no ip domain-lookup
!
!
spanning-tree mode pvst
spanning-tree extend system-id
!
interface FastEthernet0/1
 switchport mode trunk
!
interface FastEthernet0/2
 switchport access vlan 5
 switchport mode access
!
interface FastEthernet0/3
 switchport access vlan 5
 shutdown
!
interface FastEthernet0/4
 switchport access vlan 5
 shutdown
!
interface FastEthernet0/5
 switchport access vlan 5
 shutdown
!
interface FastEthernet0/6
 switchport access vlan 5
 switchport mode trunk
 shutdown
!
interface FastEthernet0/7
 switchport access vlan 5
 shutdown
!
interface FastEthernet0/8
 switchport access vlan 6
 shutdown
!
interface FastEthernet0/9
 switchport access vlan 6
 shutdown
!
interface FastEthernet0/10
 switchport access vlan 6
 shutdown
!
interface FastEthernet0/11
 switchport access vlan 6
 shutdown
!
interface FastEthernet0/12
 switchport access vlan 6
 shutdown
!
interface FastEthernet0/13
 switchport access vlan 6
 shutdown
!
interface FastEthernet0/14
 switchport access vlan 6
 shutdown
!
interface FastEthernet0/15
 switchport access vlan 7
 shutdown
!
interface FastEthernet0/16
 switchport access vlan 7
 shutdown
!
interface FastEthernet0/17
 switchport access vlan 7
 shutdown
!
interface FastEthernet0/18
 switchport access vlan 23
 shutdown
!
interface FastEthernet0/19
 switchport access vlan 7
 shutdown
!
interface FastEthernet0/20
 switchport access vlan 7
!
interface FastEthernet0/21
 switchport access vlan 8
 shutdown
!
interface FastEthernet0/22
 switchport access vlan 8
 shutdown
!
interface FastEthernet0/23
 switchport access vlan 8
 shutdown
!
interface FastEthernet0/24
 switchport access vlan 8
 shutdown
!
interface GigabitEthernet0/1
 shutdown
!
interface GigabitEthernet0/2
 shutdown
!
interface Vlan1
 no ip address
 shutdown
!
interface Vlan5
 mac-address 0001.63ba.b401
 ip address 192.168.5.11 255.255.255.0
!
ip default-gateway 192.168.1.1
!
!
!
!
line con 0
!
line vty 0 4
 login
line vty 5 15
 login
!
!
!
!
End


Brach 1
Current configuration : 1897 bytes
!
version 15.1
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname Branch1
!
!
!
!
ip dhcp excluded-address 192.168.5.1 192.168.5.10
ip dhcp excluded-address 192.168.6.1 192.168.6.10
ip dhcp excluded-address 192.168.7.1 192.168.7.10
ip dhcp excluded-address 192.168.8.1 192.168.8.10
!
ip dhcp pool VLAN5
 network 192.168.5.0 255.255.255.0
 default-router 192.168.5.1
 dns-server 209.165.200.25
ip dhcp pool VLAN6
 default-router 192.168.6.1
 dns-server 209.165.200.25
ip dhcp pool VLAN7
 default-router 192.168.7.1
 dns-server 209.165.200.25
ip dhcp pool VLAN8
 default-router 192.168.8.1
 dns-server 209.165.200.25
!
!
!
no ip cef
no ipv6 cef
!
!
!
!
license udi pid CISCO1941/K9 sn FTX1524DF9C-
!
!
!
!
!
!
!
!
!
no ip domain-lookup
!
!
spanning-tree mode pvst
!
!
!
!
!
!
interface GigabitEthernet0/0
 no ip address
 duplex auto
 speed auto
 shutdown
!
interface GigabitEthernet0/1
 no ip address
 duplex auto
 speed auto
!
interface GigabitEthernet0/1.5
 encapsulation dot1Q 5
 ip address 192.168.5.1 255.255.255.0
!
interface GigabitEthernet0/1.6
 encapsulation dot1Q 6
 ip address 192.168.6.1 255.255.255.0
!
interface GigabitEthernet0/1.7
 encapsulation dot1Q 7
 ip address 192.168.7.1 255.255.255.0
!
interface GigabitEthernet0/1.8
 encapsulation dot1Q 8
 ip address 192.168.8.1 255.255.255.0
!
interface GigabitEthernet0/1.9
 encapsulation dot1Q 9
 ip address 192.168.9.1 255.255.255.0
!
interface Serial0/0/0
 no ip address
 clock rate 2000000
 shutdown
!
interface Serial0/0/1
 ip address 192.168.1.1 255.255.255.0
 clock rate 2000000
!
interface Vlan1
 no ip address
 shutdown
!
router rip
 network 192.168.1.0
 network 192.168.5.0
 network 192.168.6.0
 network 192.168.10.0
 network 209.165.200.0
!
ip classless
!
ip flow-export version 9
!
!
!
!
!
!
!
!
line con 0
!
line aux 0
!
line vty 0 4
 login
!
!
!
End

Branch 2
Current configuration : 822 bytes
!
version 15.1
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname Branch2
!
!
!
!
!
!
!
!
no ip cef
no ipv6 cef
!
!
!
!
license udi pid CISCO1941/K9 sn FTX1524DRJO-
!
!
!
!
!
!
!
!
!
no ip domain-lookup
!
!
spanning-tree mode pvst
!
!
!
!
!
!
interface GigabitEthernet0/0
 no ip address
 duplex auto
 speed auto
 shutdown
!
interface GigabitEthernet0/1
 no ip address
 duplex auto
 speed auto
 shutdown
!
interface Serial0/0/0
 ip address 192.168.10.2 255.255.255.0
!
interface Serial0/0/1
 no ip address
 clock rate 2000000
 shutdown
!
interface Vlan1
 no ip address
 shutdown
!
router rip
 network 192.168.1.0
 network 192.168.10.0
!
ip classless
!
ip flow-export version 9
!
!
!
!
!
!
!
!
line con 0
!
line aux 0
!
line vty 0 4
 login
!
!
!
End


HQ
Current configuration : 871 bytes
!
version 15.1
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname HQ
!
!
!
!
!
!
!
!
no ip cef
no ipv6 cef
!
!
!
!
license udi pid CISCO1941/K9 sn FTX1524M2Q2-
!
!
!
!
!
!
!
!
!
no ip domain-lookup
!
!
spanning-tree mode pvst
!
!
!
!
!
!
interface GigabitEthernet0/0
 ip address 209.165.200.30 255.255.255.248
 duplex auto
 speed auto
!
interface GigabitEthernet0/1
 no ip address
 duplex auto
 speed auto
 shutdown
!
interface Serial0/0/0
 ip address 192.168.10.1 255.255.255.0
 clock rate 2000000
!
interface Serial0/0/1
 ip address 192.168.1.2 255.255.255.0
!
interface Vlan1
 no ip address
 shutdown
!
router rip
 network 192.168.1.0
 network 192.168.10.0
 network 209.165.200.0
!
ip classless
!
ip flow-export version 9
!
!
!
!
!
!
!
!
line con 0
!
line aux 0
!
line vty 0 4
 login
!
!
!
end
