Risk Assessment



	Site
	University of Wales - Single Two Storey Detached Domestic Building With Loft Room
	Assessment Number
	003

	Task / Activity
	Installation of windows – domestic properties

	Date Conducted
	10.04.2020
	Date Reviewed
	
	
	

	Assessment Team 
	Assessors
	

	1

Hazard
	2

Hazard

Effect
	3  At Risk 


	4 Severity


	5 Probability


	6 Risk Rating
	7

Required Control Measures

(minimum requirements)
	8 Severity
	9 Probability
	10 Risk Rating
	11 Acceptable?  
	12

Further site/job specific controls
	13 Completed

	Falls from height
	Death, broken bones etc.
	E
	5
	4
	20
	· Only external sealant will be applied from scaffolding.

· Ensure scaffold is erected by competent person and view hand-over certificate (see separate RA for scaffolding)

· Ensure scaffolding is inspected by competent person at designated intervals.

· Ensure employees are instructed not to tamper with or alter scaffold and to report any defects.

· Ensure employees are trained and competent.
· Ensure access ladders are suitable, inspected and clamped off.
· Ensure employees use tool belts to carry hand tools.

· Ensure ladders are only used for access purposes (3 points of contact at all times).
· Ensure employees are equipped with suitable safety boots.

· NEVER use additional items (steps etc.) to gain extra height on working platform.
· Report any suspected scaffold defects immediately to the Site Manager.
	
	
	
	
	· Reinforce with tool-box talks.

· Scaffold to be provided by Declan Thomas construction.
· Scaffold must be fully enclosed with hand rail, intermediate rail, toe board and gates.

· Weather and wind speed to be checked daily and no work undertaken if site manager feels weather conditions affect the safety of the workforce.

· Ongoing scaffold inspections to be carried out by Declan Thomas.

· Ensure external sealant work is undertaken from scaffold platform and not a ladder.

.
	

	Falling material and objects
	Head injuries
	A
	3
	3
	9
	· Windows to be fitted internally to reduce risk of falling objects.
· Scaffold to be erected during operation with brick nets in place.

· Exclusion zone to be created under windows being replaced with barriers.

· Condition of opening to be checked for loose material / rendering etc. This will carefully be removed by hand.

· Windows to be securely bolted into position at the earliest opportunity.

· Waste to be carefully carried through the property to the ground floor for disposal.

· All operatives and site workers to wear hard hats.

· All operatives to abide by Declan Thomas Site Rules.
	
	
	
	
	Reinforce with tool-box talks.
	

	Use of hand tools
	Cuts, bruises etc.
	E
	2
	2
	4
	· Ensure hand tools are fit for purpose and well maintained.
· Ensure tools are visually inspected prior to use and that any defective equipment is withdrawn from service.

· Ensure tools are kept clean and sharp.

· Ensure employees are equipped with and wear suitable gloves, impact eye protection, steel toe capped safety boots and hard hats.

· Ensure tools are not left unattended at any time.

· Ensure tools are transported in a tool belt or box, never in pockets.
	
	
	
	
	Reinforce with tool-box talks.
	

	Use of power tools
	Entanglement, electric shock etc.
	
	
	
	
	· Ensure that tools supplied are suitable and adequate for the job.

· Ensure employees are trained and competent in the use of the equipment.

· Ensure all equipment is visually checked prior to use and defects reported before use.

· Ensure only battery rechargeable or 110v equipment used.

· Ensure electrical equipment is PAT tested.

· Ensure all guards and safety devices are in place before use.

· Ensure no loose clothing / jewellery / long hair is worn.

· Ensure drill bits are sharp and of the correct size.

· Ensure walls / ceilings etc. are scanned for the presence of cables or pipes prior to fixing.

· Ensure employees wear suitable safety boots, hard hat, impact eye protection, ear defenders and an approved respirator.

· See vibration, noise and asbestos categories.
	
	
	
	
	Reinforce with tool-box talks.
	

	Electricity / overhead cables
	Electric shock, burns, fire and explosion.
	A
	5
	3
	15
	· Ensure that all electrical tools and equipment are visually inspected prior to use and any defects reported prior to use.

· Ensure equipment is PAT Tested.

· Ensure only battery rechargeable or 110v equipment used on site.

· Ensure employees are trained and competent.

· Ensure that service plans are obtained where available and that walls / ceilings etc. are scanned for cables and wires prior to any fixing work.

· Ensure workers attend briefing from E-ON on cable safety.

· Ensure that any power cables are isolated prior to work in the vicinity.

· Ensure cables are isolated and properly sheathed and covered by E-ON competent engineers.

· Ensure that no tools or equipment are leant against cables and no work undertaken next to or above cables.

· Ensure safe distance is marked and exclusion zone maintained.

· Ensure E-ON guidelines and procedures are followed.
	
	
	
	
	Reinforce with tool-box talks.
	

	Hazardous substances including dust
	Broken bones, cuts, bruises
	A
	3
	3
	9
	· Ensure material safety data sheets are obtained for substances used etc.
· Ensure COSHH Risk assessment is carried out for using hazardous substances.

· Ensure employees trained in safe use of chemicals.

· Ensure employees are issued with, and use suitable approved chemical resistant gloves.

· Ensure good hygiene practices are maintained and hand washes / wipes are available on site.

· Ensure first aid kit is available.

· Ensure no substances are left unattended on site at any time.

· Ensure employees use and replacing windows.
· NO asbestos work to be carried out.
	
	
	
	
	Reinforce with tool-box talks.
	

	Asbestos Containing Materials
	Asbestos related diseases, lung cancer etc.
	A
	5
	1
	5
	· No asbestos reported to be present.

· View asbestos management plan and register to confirm this.

· Ensure work is stopped immediately if any asbestos is suspected.

· Ensure that trained, competent and licensed company is appointed to remove any suspected asbestos.

· Ensure employees are trained in asbestos awareness.
	
	
	
	
	
	

	Manual Handling
	Sprains, strains, broken bones etc.
	E
	3
	4
	12
	· Ensure that a minimum of three operatives are available at all times.
· Ensure glass is handled by two operatives with specialist handing gloves and wrist protectors.
· Ensure employees are trained in manual handling.

· Ensure new windows are protected by cardboard or similar prior to transporting them.

· Ensure employees are equipped with approved PPE including steel toe cap safety boots, suitable gloves and wrist protectors.
· Where practical to do so utilise mechanical aids (Separate RA required).
	
	
	
	
	
	

	Authorised by

The Responsible Manager
	Signed:
	Dated:
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	E - Employees
	1
	No Injury
	1
	Very Unlikely
	1 – 5
	LO W
	A - Acceptable
	

	C - Contractors
	2
	Minor Injury
	2
	Unlikely
	6 - 14
	MEDIUM
	M - More Analysis Required
	

	V - Visitors
	3
	+3 Day Absence
	3
	Likely
	15 - 25
	HIGH
	U – Unacceptable Risk
	

	P - Public
	4
	Major Injury 
	4
	Very Likely
	
	
	
	

	A - All
	5
	Death
	5
	Virtually Certain
	
	
	
	



