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/* Main.c file generated by New Project wizard

* Created:  Tue May 13 2025
* Processor: PICI6FE774

* Compiler: CCs for PIC

o

#include <16F877A.h>
int val[] = {xco, OxF9, 0xA4, 0xBO, x99, 0x92, OxB2, OxfS, OxBe, @x90}
void main()
{
while(TRUE);
- {
1 (v=0,1>10,v++1);
| {
output port_D(v);

delay-ns 200 ;
¥

)—
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* Created:  Tue May 13 2025
* Processor: PICI6FE774
* Compiler: CCs for PIC
R4

#include <16F877A.h>

void main()

=N
while(TRUE);
=1
£ (input_co (high));
=]
output pin_B(high);
3
else:
R
output pin_b(low);
b
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