SWITCH
SHOW RUNNING-CONFIGURATION:
S1# show running-config
Building configuration...

Current configuration : 1609 bytes
!
! Last configuration change at 00:41:18 UTC Tue Mar 2 1993
!
version 15.2
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
service password-encryption
!
hostname S1
!
boot-start-marker
boot-end-marker
!
enable secret 5 $1$NllY$9q7emM19iiaHCofcqdApS.
!
no aaa new-model
system mtu routing 1500
!
!
!
!
!
!
!
no ip domain-lookup
!
!
!
spanning-tree mode pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
!
!
!
interface FastEthernet0/1
!
interface FastEthernet0/2
!
interface FastEthernet0/3
!
interface FastEthernet0/4
!
interface FastEthernet0/5
!
interface FastEthernet0/6
!
interface FastEthernet0/7
!
interface FastEthernet0/8
!
interface FastEthernet0/9
!
interface FastEthernet0/10
!
interface FastEthernet0/11
!
interface FastEthernet0/12
!
interface FastEthernet0/13
!
interface FastEthernet0/14
!
interface FastEthernet0/15
!
interface FastEthernet0/16
!
interface FastEthernet0/17
!
interface FastEthernet0/18
!
interface FastEthernet0/19
!
interface FastEthernet0/20
!
interface FastEthernet0/21
!
interface FastEthernet0/22
!
interface FastEthernet0/23
!
interface FastEthernet0/24
!
interface GigabitEthernet0/1
!
interface GigabitEthernet0/2
!
interface Vlan1
 ip address 172.16.11.10 255.255.255.0
!
ip default-gateway 172.16.11.1
ip http server
ip http secure-server
!
no vstack
banner motd ^CPlease only authorised people^C
!
line con 0
 password 7 070C285F4D06
 login
line vty 0 4
 password 7 01100F175804
 login
 transport input telnet
line vty 5 15
 password 7 01100F175804
 login
 transport input telnet
!
end

S1#


SHOW IP INTERFACE BRIEF:
S1#show ip interface brief
Interface              IP-Address      OK? Method Status                Protocol
Vlan1                  172.16.11.10    YES manual up                    up
FastEthernet0/1        unassigned      YES unset  down                  down
FastEthernet0/2        unassigned      YES unset  down                  down
FastEthernet0/3        unassigned      YES unset  down                  down
FastEthernet0/4        unassigned      YES unset  down                  down
FastEthernet0/5        unassigned      YES unset  up                    up
FastEthernet0/6        unassigned      YES unset  up                    up
FastEthernet0/7        unassigned      YES unset  down                  down
FastEthernet0/8        unassigned      YES unset  down                  down
FastEthernet0/9        unassigned      YES unset  down                  down
FastEthernet0/10       unassigned      YES unset  down                  down
FastEthernet0/11       unassigned      YES unset  down                  down
FastEthernet0/12       unassigned      YES unset  down                  down
FastEthernet0/13       unassigned      YES unset  down                  down
FastEthernet0/14       unassigned      YES unset  down                  down
FastEthernet0/15       unassigned      YES unset  down                  down
FastEthernet0/16       unassigned      YES unset  down                  down
FastEthernet0/17       unassigned      YES unset  down                  down
FastEthernet0/18       unassigned      YES unset  down                  down
FastEthernet0/19       unassigned      YES unset  down                  down
FastEthernet0/20       unassigned      YES unset  down                  down
FastEthernet0/21       unassigned      YES unset  down                  down
FastEthernet0/22       unassigned      YES unset  down                  down
FastEthernet0/23       unassigned      YES unset  down                  down
FastEthernet0/24       unassigned      YES unset  down                  down
GigabitEthernet0/1     unassigned      YES unset  down                  down
GigabitEthernet0/2     unassigned      YES unset  down                  down
S1#
ROUTER:
SHOW RUNNING-CONFIGURATION:
R1#show running-config
Building configuration...


Current configuration : 3638 bytes
!
! Last configuration change at 09:59:19 UTC Tue Dec 18 2018
!
version 16.9
service timestamps debug datetime msec
service timestamps log datetime msec
service password-encryption
platform qfp utilization monitor load 80
no platform punt-keepalive disable-kernel-core
!
hostname R1
!
boot-start-marker
boot-end-marker
!
!
enable secret 5 $1$8kaF$XCWIRpgFCwrBmHqO3pyn70
!
no aaa new-model
!
no ip domain lookup
ip admission watch-list expiry-time 0
!
!
!
!
!
!
!
!
!
!
subscriber templating
multilink bundle-name authenticated
!
!
!
crypto pki trustpoint TP-self-signed-1020466531
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-1020466531
 revocation-check none
 rsakeypair TP-self-signed-1020466531
!
!
crypto pki certificate chain TP-self-signed-1020466531
 certificate self-signed 01
  30820330 30820218 A0030201 02020101 300D0609 2A864886 F70D0101 05050030
  31312F30 2D060355 04031326 494F532D 53656C66 2D536967 6E65642D 43657274
  69666963 6174652D 31303230 34363635 3331301E 170D3138 31323138 30393439
  34375A17 0D333030 31303130 30303030 305A3031 312F302D 06035504 03132649
  4F532D53 656C662D 5369676E 65642D43 65727469 66696361 74652D31 30323034
  36363533 31308201 22300D06 092A8648 86F70D01 01010500 0382010F 00308201
  0A028201 0100ADD4 A2C20EF6 58F197EC C9593521 70F7F9DE 4EBB767D 6FD0FC74
  82D99987 54F33061 A94EFC04 FA33E1E2 0C503A48 F2EBFDB8 C2120E57 5F428611
  9C9095F3 0F56A507 08498CC2 751A6669 A57D07B1 8EA0EBE3 0A24DCB7 BD11A34A
  CB422B68 C8614504 2439368F 401C85AF 1AF44FD8 3AEA57D6 F9588E0F DBACAEA5
  0D6064E3 FBAF6F7F 284642E0 C8B58B48 6960230B 34BA3244 054448F7 EE2176CF
  9EB0EF99 A8F0592E 061D2022 9FCAA8A2 EDF03E15 365EE8B6 819FCC13 052393F2
  368A5C59 9E21AAE7 75B4BFDC 320EE53B 02FCB302 40A48D72 B0D7FB05 53FF6A0E
  080921F8 545F360F C7078155 103EED54 4A3BFA0F 2A296F48 6E299C1B 1EC16B01
  739C41EE 5D810203 010001A3 53305130 0F060355 1D130101 FF040530 030101FF
  301F0603 551D2304 18301680 1400540C 8D34631B 9292D7A6 BCA763E4 AA3CD942
  34301D06 03551D0E 04160414 00540C8D 34631B92 92D7A6BC A763E4AA 3CD94234
  300D0609 2A864886 F70D0101 05050003 82010100 508C8A3F C272DA69 D6A6BFF0
  DCAF2C1C 93970C8B 164AE3B9 499AF246 B8E784EB 6D31D80C 8AD143C4 DAF71C9A
  1C6B9438 79126B9F 0EFBD065 002BC9EA B859599C BC0B0B70 087C623E FAA94FAE
  98B5AB48 F445C495 D0935D0A 1B334625 F53542AD 058B619C 11740E11 4EA01A3E
  F00AEF59 C107E8AF 6BACEDBE 05C46F75 2844EA1D 31A693D3 FD343095 49BA3B96
  7CABC10B A440BC21 C2CAE63D 16836E7B 322733E2 065E5005 D7167253 0AAA4408
  E3F6ED4D D3A8AC69 15DC881F C33AC1A0 DCC28886 8907A9AA A481F791 8AA02A6F
  1E061E81 B4460283 C9CEB0CB F2AF1FA4 CE09199B 14A2DA3A 2D524700 8630E8BA
  51B6C5FF FD228584 070E422D EB8BEEEE 65D0BAED
        quit
!
license udi pid ISR4221/K9 sn FGL224190DM
no license smart enable
diagnostic bootup level minimal
!
spanning-tree extend system-id
!
!
!
!
redundancy
 mode none
!
!
!
!
!
!
!
!
interface GigabitEthernet0/0/0
 description THIS INTERFACE IS CONNECTED WITH PC12
 ip address 172.16.10.1 255.255.255.0
 negotiation auto
!
interface GigabitEthernet0/0/1
 description THIS INTERFACE IS CONNECTED WITH S1
 ip address 172.16.11.1 255.255.255.0
 negotiation auto
!
interface Serial0/1/0
 no ip address
 shutdown
!
interface Serial0/1/1
 no ip address
 shutdown
!
ip forward-protocol nd
ip http server
ip http authentication local
ip http secure-server
!
!
!
!
!
!
control-plane
!
banner motd ^C Please stay far from here^C
!
line con 0
 password 7 01100F175804
 login
 transport input none
 stopbits 1
line vty 0 4
 password 7 104D000A0618
 login
line vty 5 15
 password 7 104D000A0618
 login
!
!
!
!
!
!
end

R1#



SHOW IP INTERFACE BRIEF:
R1#show ip interface brief
Interface              IP-Address      OK? Method Status                Protocol
GigabitEthernet0/0/0   172.16.10.1     YES manual up                    up
GigabitEthernet0/0/1   172.16.11.1     YES manual up                    up
Serial0/1/0            unassigned      YES unset  administratively down down
Serial0/1/1            unassigned      YES unset  administratively down down
R1#




PING FROM PC-A TO 172.16.10.254:
C:\Users\Admin>ping 172.16.10.254

Pinging 172.16.10.254 with 32 bytes of data:
Reply from 172.16.10.254: bytes=32 time<1ms TTL=127
Reply from 172.16.10.254: bytes=32 time<1ms TTL=127
Reply from 172.16.10.254: bytes=32 time<1ms TTL=127
Reply from 172.16.10.254: bytes=32 time<1ms TTL=127

Ping statistics for 172.16.10.254:
    Packets: Sent = 4, Received = 4, Lost = 0 (0% loss),
Approximate round trip times in milli-seconds:
    Minimum = 0ms, Maximum = 0ms, Average = 0ms

C:\Users\Admin>




[bookmark: _GoBack]PING FROM PC-B TO 172.16.11.254:
C:\Users\Admin>ping 172.16.11.254

Pinging 172.16.11.254 with 32 bytes of data:
Reply from 172.16.11.254: bytes=32 time<1ms TTL=127
Reply from 172.16.11.254: bytes=32 time<1ms TTL=127
Reply from 172.16.11.254: bytes=32 time<1ms TTL=127
Reply from 172.16.11.254: bytes=32 time<1ms TTL=127

Ping statistics for 172.16.11.254:
    Packets: Sent = 4, Received = 4, Lost = 0 (0% loss),
Approximate round trip times in milli-seconds:
    Minimum = 0ms, Maximum = 0ms, Average = 0ms

C:\Users\Admin>


