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S1#show running-config
Building configuration...

Current configuration : 1602 bytes
!
! Last configuration change at 01:28:16 UTC Mon Mar 1 1993
!
version 15.2
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
service password-encryption
!
hostname S1
!
boot-start-marker
boot-end-marker
!
enable secret 5 $1$3rv3$jiGO5DDscWu4Q.iBrJjOA1
!
no aaa new-model
system mtu routing 1500
!
!
!
!
!
!
!
no ip domain-lookup
!
!
!
spanning-tree mode pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
!
!
!
interface FastEthernet0/1
!
interface FastEthernet0/2
!
interface FastEthernet0/3
!
interface FastEthernet0/4
!
interface FastEthernet0/5
!
interface FastEthernet0/6
!
interface FastEthernet0/7
!
interface FastEthernet0/8
!
interface FastEthernet0/9
!
interface FastEthernet0/10
!
interface FastEthernet0/11
!
interface FastEthernet0/12
!
interface FastEthernet0/13
!
interface FastEthernet0/14
!
interface FastEthernet0/15
!
interface FastEthernet0/16
!
interface FastEthernet0/17
!
interface FastEthernet0/18
!
interface FastEthernet0/19
!
interface FastEthernet0/20
!
interface FastEthernet0/21
!
interface FastEthernet0/22
!
interface FastEthernet0/23
!
interface FastEthernet0/24
!
interface GigabitEthernet0/1
!
interface GigabitEthernet0/2
!
interface Vlan1
 ip address 172.16.11.10 255.255.255.0
!
ip default-gateway 172.16.11.1
ip http server
ip http secure-server
!
no vstack
banner motd ^CAuthorised access only^C
!
line con 0
 password 7 110A1016141D
 login
line vty 0 4
 password 7 1511021F0725
 login
 transport input telnet
line vty 5 15
 password 7 1511021F0725
 login
 transport input telnet
!
End


S1#show ip int brief
Interface              IP-Address      OK? Method Status                Protocol
Vlan1                  172.16.11.10    YES manual up                    up
FastEthernet0/1        unassigned      YES unset  down                  down
FastEthernet0/2        unassigned      YES unset  down                  down
FastEthernet0/3        unassigned      YES unset  down                  down
FastEthernet0/4        unassigned      YES unset  down                  down
FastEthernet0/5        unassigned      YES unset  up                    up
FastEthernet0/6        unassigned      YES unset  up                    up
FastEthernet0/7        unassigned      YES unset  down                  down
FastEthernet0/8        unassigned      YES unset  down                  down
FastEthernet0/9        unassigned      YES unset  down                  down
FastEthernet0/10       unassigned      YES unset  down                  down
FastEthernet0/11       unassigned      YES unset  down                  down
FastEthernet0/12       unassigned      YES unset  down                  down
FastEthernet0/13       unassigned      YES unset  down                  down
FastEthernet0/14       unassigned      YES unset  down                  down
FastEthernet0/15       unassigned      YES unset  down                  down
FastEthernet0/16       unassigned      YES unset  down                  down
FastEthernet0/17       unassigned      YES unset  down                  down
FastEthernet0/18       unassigned      YES unset  down                  down
FastEthernet0/19       unassigned      YES unset  down                  down
FastEthernet0/20       unassigned      YES unset  down                  down
FastEthernet0/21       unassigned      YES unset  down                  down
FastEthernet0/22       unassigned      YES unset  down                  down
FastEthernet0/23       unassigned      YES unset  down                  down
FastEthernet0/24       unassigned      YES unset  down                  down
GigabitEthernet0/1     unassigned      YES unset  down                  down
GigabitEthernet0/2     unassigned      YES unset  down                  down


R1#show running-config
Building configuration...


Current configuration : 3609 bytes
!
! Last configuration change at 13:27:37 UTC Wed Apr 12 2000
!
version 16.9
service timestamps debug datetime msec
service timestamps log datetime msec
service password-encryption
platform qfp utilization monitor load 80
no platform punt-keepalive disable-kernel-core
!
hostname R1
!
boot-start-marker
boot-end-marker
!
!
enable secret 5 $1$QdDE$aVvD2/owphcK8Wurt5Knr.
!
no aaa new-model
!
no ip domain lookup
ip admission watch-list expiry-time 0
!
!
!
!
!
!
!
!
!
!
subscriber templating
multilink bundle-name authenticated
!
!
!
crypto pki trustpoint TP-self-signed-1020466531
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-1020466531
 revocation-check none
 rsakeypair TP-self-signed-1020466531
!
!
crypto pki certificate chain TP-self-signed-1020466531
 certificate self-signed 01
  30820330 30820218 A0030201 02020101 300D0609 2A864886 F70D0101 05050030
  31312F30 2D060355 04031326 494F532D 53656C66 2D536967 6E65642D 43657274
  69666963 6174652D 31303230 34363635 3331301E 170D3030 30343132 31323334
  31305A17 0D333030 31303130 30303030 305A3031 312F302D 06035504 03132649
  4F532D53 656C662D 5369676E 65642D43 65727469 66696361 74652D31 30323034
  36363533 31308201 22300D06 092A8648 86F70D01 01010500 0382010F 00308201
  0A028201 0100BD9E 12FAC2B7 0AA5B870 7CB8770B 69CB9378 2C730FC8 ADBAF6F3
  6C84657F 2A1393D6 A98FB64B D75680AF DD7CF454 40632946 3C3A96D4 32CAFDDC
  B190E3F2 CC76638D 57A0444B 762A1A07 82CF08C1 541A6E94 2FAE47FE A311B63A
  F4A25790 5772405D 317B342A 00CA8101 62A2051C EF67F2BA 7EF7E618 1D78BD6A
  8EC65C1D 00956C09 71D388F6 3D45CDD6 3CD3B386 4BEAD6F1 682CD760 D9CF13E7
  38F1C5FA F4B30052 1B2C688A 18E345FC AD986695 68CF6CC1 0D4AE31D 374FB8B3
  32BAEA07 A7B42E63 39D3B7D9 1DB4194B 99016EF0 086116EF 5DA66575 A83027F5
  BE940517 015C71FE E96BB460 1AA9B407 5751E119 318F30EF B6696B69 F3AA4F24
  D59B63CD 24A50203 010001A3 53305130 0F060355 1D130101 FF040530 030101FF
  301F0603 551D2304 18301680 14704AD5 6128FD41 565D3247 C062D091 0C8C1D97
  25301D06 03551D0E 04160414 704AD561 28FD4156 5D3247C0 62D0910C 8C1D9725
  300D0609 2A864886 F70D0101 05050003 82010100 3167AEBA 99436C2F AF2A8731
  13A4EA74 7D7EDEA3 904C7688 22052E56 CDB3C2FF FEB63785 71FAEE7E 9F673E88
  E5DCFF11 7154BBF6 2B1CDC64 961AFD29 47622D44 BC45200D 78B515CD 4B4B1FCD
  E2EF5184 F2FE570D 095877EF BCEDB612 D2FE92AF 59C74025 38007798 B3A13063
  CBB3E45E 24906970 01E34855 254A7BAA 56CAFBBA 81738363 B66C7A0C 31ABC585
  46F3ECD0 5FC11E1B 2B31874C CFA16E8A 1DC69814 88D9150F 0FDD8B84 21A02B53
  1A243FAF 08B2C762 0C1AF202 91A93394 06FA611A E3925F93 F321F06F B57EB1E5
  DB51D973 200FA31B 92693AD7 9EC8B527 FACDD984 5DCEC040 83E83245 8A20F000
  78C08FE1 B65CF7BC E46CCF47 2D65AF7E A5CB2A86
        quit
!
license udi pid ISR4221/K9 sn FGL224190DM
no license smart enable
diagnostic bootup level minimal
!
spanning-tree extend system-id
!
!
!
!
redundancy
 mode none
!
!
!
!
!
!
!
!
interface GigabitEthernet0/0/0
 description "Connected to Pc-b"
 ip address 172.16.10.1 255.255.255.0
 negotiation auto
!
interface GigabitEthernet0/0/1
 description "Connected to S1"
 ip address 172.16.11.1 255.255.255.0
 negotiation auto
!
interface Serial0/1/0
 no ip address
 shutdown
!
interface Serial0/1/1
 no ip address
 shutdown
!
ip forward-protocol nd
ip http server
ip http authentication local
ip http secure-server
!
!
!
!
!
!
control-plane
!
banner motd ^CUnauthorised access is prohibited^C
!
line con 0
 password 7 14141B180F0B
 login
 transport input none
 stopbits 1
line vty 0 4
 password 7 05080F1C2243
 login
line vty 5 15
 password 7 05080F1C2243
 login
!
!
!
!
!
!
End


R1#show ip int brief
Interface              IP-Address      OK? Method Status                Protocol
GigabitEthernet0/0/0   172.16.10.1     YES manual up                    up
GigabitEthernet0/0/1   172.16.11.1     YES manual up                    up
Serial0/1/0            unassigned      YES unset  administratively down down
Serial0/1/1            unassigned      YES unset  administratively down down

Ping Pc-A
C:\Users\Admin>ping 172.16.10.254
Pinging 172.16.10.254 with 32 bytes of data:
Reply from 172.16.10.254: bytes=32 time<1ms TTL=127
Reply from 172.16.10.254: bytes=32 time<1ms TTL=127
Reply from 172.16.10.254: bytes=32 time<1ms TTL=127
Reply from 172.16.10.254: bytes=32 time<1ms TTL=127

Ping statistics for 172.16.10.254:
    Packets: Sent = 4, Received = 4, Lost = 0 (0% loss),
Approximate round trip times in milli-seconds:
    Minimum = 0ms, Maximum = 0ms, Average = 0ms

Pc-B ping 
C:\Users\Admin>ping 172.16.11.254

Pinging 172.16.11.254 with 32 bytes of data:
Reply from 172.16.11.254: bytes=32 time<1ms TTL=127
Reply from 172.16.11.254: bytes=32 time=1ms TTL=127
Reply from 172.16.11.254: bytes=32 time<1ms TTL=127
Reply from 172.16.11.254: bytes=32 time=1ms TTL=127

Ping statistics for 172.16.11.254:
    Packets: Sent = 4, Received = 4, Lost = 0 (0% loss),
Approximate round trip times in milli-seconds:
    Minimum = 0ms, Maximum = 1ms, Average = 0ms
