	Activity to be Assessed
	Assessment Number
	

	Roof Construction
	10002
	

	Persons undertaking or affected by the activity
	

	
	

	
	Y
	Employees
	Y
	Contractor
	Y
	Public
	Y
	Service User
	

	
	

	
	Y
	Other: Principal Designer and Principle Contractor 
	

	Identified Hazards and Associated Risks
	Likelihood
	Severity
	Risk Level
	

	1
	Unsafe access and egress.
	3
	4
	12
	

	2
	Falling objects.
	3
	4
	12
	

	3
	Slips, trips and falls from roof edges and openings.
	3
	5
	15
	

	4
	Unsafe weather.
	3
	2
	6
	

	5
	Unsafe transportation of materials from the ground to scaffolding.
	4
	3
	12
	

	Existing Control Measures / Additional Control Measures Required
	

	1
	To prevent unsafe access and egress, ladders should be used and fixed to the scaffold at the appropriate opening. Stair towers and fixed or mobile scaffold towers should be used. All openings should have a gate to prevent them from staying open when not in use. Where scaffolding is not available, then mobile access equipment should be used in strict accordance with the Lifting Operations and Lifting Equipment Regulations 1998 (LOLER) and a separate risk assessment for this must be carried out.
	

	2
	To prevent objects from falling from height, guardrails and toeboards must be used in the scaffolding. All tools and materials on the scaffolding should be secured where possible to prevent them falling on people below. Debris nets or catch platforms can be installed to help catch falling objects.
	

	3
	Slips, trips and falls from roof edgings and openings can be avoided installing scaffolding to prevent people falling from the edge. Edge protection must be fit to the eaves of the roof, once constructed. A secure double guardrail and toeboard must be fit around the edge. Workers must regularly check for anything in their path that could cause a slip, trip or fall and remove that hazard of safe to do so. If it is not safe to do so, they should should stop work immediately, notify their colleagues and notify the site manager. Work will only then commence once the hazard has been dealt with.
	

	4
	Weather can be unpredictable but it would be best practice to monitor the weather and keep updated about any predicted changes. The construction of the roof is to take place in May so the weather should be mild/warm and dry. However, the location of the construction is near the coast so high winds and rain is a high possibility. If the weather is too adverse to safely carry out work at height then the work must be delayed until that weather changes.
	

	5
	To prevent unsafe transportation of materials from the ground to scaffolding the Work at Height Regulations 2005 (WAHR) must be followed. Unstable or unbalanced loads must not be carried up a ladder. Also, the Manual Handling Operations Regulations 1992 must be followed. Where possible, lifting aids should be used, such as forklifts. These must be used by competent person with the relevant and valid certification. This must be done in strictly in accordance with the Lifting Operations and Lifting Equipment Regulations 1998 (LOLER).
	

	Reassessment of Activity Hazards 
	Likelihood
	Severity
	Risk Level
	

	1
	Unsafe access and egress.
	1
	3
	3
	

	2
	Falling objects.
	2
	2
	4
	

	3
	Slips, trips and falls from roof edges and openings.
	2
	4
	8
	

	4
	Unsafe weather.
	3
	1
	3
	

	5
	Unsafe transportation of materials from the ground to scaffolding.
	1
	2
	2
	

	Name  Lee Thomas

Position  Principle Designer
	Signed L. Thomas


	   Date of Completion: 19.04.2020
	

	Reviews
	Key
	
	

	Review Date: 
	Likelihood
	Severity
	Severity of Injury
	5
	5Y
	10R
	15
	20
	25

	Reviewed by: 
	1   very     unlikely

2   unlikely

3   likely

4   very likely

5   certainty
	1   nuisance

2   minor

3   medical treatment

4   major

5   fatal
	
	4
	4
	8
	12
	16
	20

	Review Date :
	
	
	
	3
	3
	6G
	9
	12
	15

	Reviewed by:
	
	
	
	2
	2
	4
	6Y
	8
	10Y

	Review Date :
	
	
	
	1
	1
	2
	3
	4
	5G

	Reviewed by:
	
	
	
	0
	1
	2
	3
	4
	5

	Review Date :
	
	
	
	Likelihood of Injury
	

	Reviewed by:
	
	
	
	Low Risk
	
	Medium Risk
	
	High Risk
	


