THERMODYNAMICS EXAM 2016-17


1. QUESTION FOUR / Closed System: (15 marks)

An insulated rigid tank initially contains 0.7 kg of helium at 27C and 350 kPa. A paddle wheel with a power rating of 0.015 kW is operated within the tank for 30 min. Determine,
a) The final temperature of the helium gas.	[10]
b) The final pressure of the helium gas.	[5]

Tank filled with helium









Assumptions:
· Helium can be considered as an ideal gas.
· Constant specific heat values and gas constant can be found in Table A-2.



2. QUESTION FIVE  / Open system, steady-flow process:  (15 marks)

A house has an electric heating system that consists of a 300 W fan and an electric resistance heating element placed in a duct. Air flows steadily through the duct at a rate of 0.6 kg/s and experiences a temperature rise of 7C. The rate of heat loss from the air in the duct is estimated to be 305 W. Determine the power rating of the electric resistance heating element.
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Assumptions:
· Air can be considered as an ideal gas.
· Constant specific heat values can be found in Table A-2.
· Kinetic and potential energy changes are negligible. 


3. QUESTION SIX  / Open system, unsteady-flow process:  (20 marks)

An air conditioning system is to be filled from a rigid container that initially contains 5 kg of saturated liquid R-134a at 24C. The valve connecting this container to the air-conditioning system is now opened until the mass in the container is 0.25 kg, at which time the valve is closed. During this time, only liquid R-134a flows from the container. Thus, at the final state the container encloses a saturated liquid - vapour mixture. Presuming that the process is isothermal (that is constant temperature) while the valve is open, determine,
a) The final quality of the remaining liquid-vapour mixture of the R-134a in the container.	[10]
b) The total heat transfer. 	[10]
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Assumptions:
· Kinetic and potential energy changes are negligible.
· There are no work interactions involved.
· The system is isothermal therefore T2 = T1.
· Specific enthalpy of the exit is .
· You will need to use Table A-11.
· In a saturated liquid-vapour mixture, the mass fraction of vapour is called the quality and is expressed as:

Quality may have values between 0 (saturated liquid) and 1 (saturated vapour). It has no meaning in the compressed liquid or superheated vapour regions. In the saturated mixture region, the average value of any intensive property y is determined from:

where f stands for saturated liquid, g for saturated vapour and y stands for v, u or h.
· [bookmark: _GoBack]For specific volume, 
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B 5-113 A hair dryer consumes 1200 W of electric power when running. The inlet volume flow rate and the
exit velocity of air are to be determined.

Assumptions 1 This is a steady-flow process since there is no change with time. 2 Air is an ideal gas with
constant specific heats at room temperature. 3 Kinetic and potential energy changes are negligible. 4 The
power consumed by the fan and the heat losses are negligible.

Properties The gas constant of air is 0.287 kPa.m*/kg K (Table A-1). The constant pressure specific heat of
air at room temperature is ¢, = 1.005 kJ/kg-K (Table A-2)

Analysis We take the hair dryer as the system. which is a control volume since mass crosses the boundary.
There is only one inlet and one exit, and thus 7y = i1, = 71 . The energy balance for this steady-flow system
can be expressed in the rate form as
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Substituting. the mass and volume flow rates of air are determined to be
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] Analysis We take the tank as the system, which is a control volume since mass crosses the boundary.

" Noting that the microscopic energies of flowing and nonflowing fluids are represented by enthalpy / and

internal energy u, respectively, the mass and energy balances for this uniform-flow system can be

expressed as
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The initial state properties of R-134a in the tank are

v, =0.0008261m* kg
u, =84.44kJ/kg (Table A-11)

h, =84.98 kI/kg
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