IOAN ALEXANDRU BLAJ    

PART 3




    Using ping command, verify end-to-end connectivity:
From PC-1, ping PC-2 & LP-A. Is it successful? 	YES					 From PC-1, ping default gateway. Is it successful? 			YES		 From PC-2, ping 172.16.0.1. Is it successful?         YES		 From PC-1, ping 172.16.0.254. Is it successful?                  NO				



Issue the shutdown command on R1 G0/1, and then re-issue the following commands to verify that HSRP is working as expected:
From PC-2, ping 172.16.0.1. Ping should not be successful        NO	 From PC-2, ping default gateway. Is it successful? 	YES	  From PC-2, ping 209.165.200.225. Is it successful? 		YES		

