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Materials Elements and Cost Comparisons

This is a brief study to investigate estimated cost differences/savings between a selection of the following elements –
Foundations
Specified design to date incorporates a steel sheet piled perimeter with CFA piles to support the main structures. Alternate proposal for a Secant piled perimeter supporting wall with a reduced number of CFA piles within to add foundation support.
Original build total -			£64,116,386
Alternate foundations build total -	£63,819,926
Difference (saving) -			£296,460
Roof
Specified design to date incorporates a Landscaped (extensive) Green Roof. Alternate proposal is to use a Zinc Standing Seam Roof covering.
Original build total -			£64,116,386
Alternate roof build total -		£63,691,571
Difference (saving) -			£424,815





Rugby Pitch
Specified design to date incorporates a Lano Sports Artificial Pitch. Alternate proposal is to use a Natural Winter Sports grade grass.
Original build total -			£64,116,386
Alternate pitch build total -		£63,882,289
Difference (saving) -			£234,097
Skydiving Wind Tunnel
Specified design to date incorporates a Skydiving Wind Tunnel. This is a simple comparison to look at the cost saving if this element omitted.
Original build total -			£64,116,386
Build total without wind tunnel -	£61,594,477
Difference (saving) -			£2,521,909

A total of these savings shown is £3,477,281 and will bring the Cost Estimate Build Total to £60,639,105  (£2720/m2).
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