1. The vice needs to be mountable in a CNC milling machine using a standard T-slot system. Research current T-slot clamping and apply the most suitable method to your vice body. 
2. Design the jaws to hold a 20mm steel tube. Allowing a row of 6mm vertical holes to be drilled. 
3. Add a method of quickly referencing new tubes into the correct position. 
4. [bookmark: _GoBack]Produce a full set of production drawings including an exploded view and bill of materials. 
