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ommand Prompt

Microsoft Windows [Version 16.6.18362.418]
(c) 2019 Microsoft Corporation. All rights reserved.

:\Users\Adnin>ping 141.246.11.16

Pinging 141.246.11.16 with 32 bytes of data:
transmit failed. General failure.
: transmit failed. General failure.
transmit failed. General failure.
transmit failed. General failure.

Ping statistics for 141.246.11.16:
Packets: Sent = 4, Received = ©, Lost = 4 (166% loss),

:\Users\Admin>
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