[bookmark: _GoBack]Limits & Fits Lecture – Formative Exercise 

Develop a fully dimensioned technical drawing of ‘Block C’ below. Calculate and specify the large hole to have a precision clearance and the small hole to have an interference fit.
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