IPV4 AND IPV6 Design activity
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2.1 IP Addressing table 
From the topology diagram, complete the IP Address table below. For LAN and IPv4 addresses, assign the first usable address to the router interface, the second usable address to the switch, and last usable addresses to the PCs. For IPv6, use the first, second, third, and fourth addresses to meet your addressing requirements.(10 marks)
	Device
	Interface
	IP Address 
	Subnet mask
	IPv6 Address 
	IP Default Gateway
	IPV6 Default Gateway

	R1
	Gi 0/1
	
	
	
	
	

	
	Gi0/0
	
	
	
	
	

	
	Lo1
	
	
	
	
	

	
	Lo2
	
	
	
	
	

	R2
	Gi0/1
	
	
	
	
	

	
	Gi0/0 
	
	
	
	
	

	
	Lo3
	
	
	
	
	

	AS1
	VLAN 1
	
	
	
	
	

	AS2
	VLAN1
	
	
	
	
	

	PC1
	NIC
	
	
	
	
	

	PC2
	NIC
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