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[bookmark: _Toc92083620]Abstract
This report is focused on comparing the simulation of a closed loop control system with its mathematical model and using the latter to validate the simulation. This has been done by modelling the simulation in MATLAB and Simulink of the Plant and then tuning a P.I.D. controller to bring the plant under control within the specifications. The values from the controller were then input into a Single Transfer Function which is representative of the whole simulation. The results of both were then compared and the Simulation model was validated.
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[bookmark: _Toc92083622]Introduction
This report will be looking at a control system for the angular positioning system of a Close-In-Weapon-System (CIWS) turret.
The aim is to use MATLAB and Simulink to simulate the control system (controller, plant, and feedback) and use this model to bring it under control in under two seconds and with an overshoot of less than 5%. Using this information, a Single Transfer Function can then be created. These two can then be compared to validate the Model
The Simulation and the Single Transfer Function are both modelled in MATLAB’s Simulink (see Figure 1). All screenshots and results within this report are taken from MATLAB and Simulink [1]
[bookmark: _Toc92083623]What is a control system?
Control systems are used in all sorts of processes and according to Karl and Richard [2], a controller utilises feedback to compare the output to the desired system behaviour and makes corrections to achieve this. 
There are two types of systems: Open and Closed loop systems. The difference between a closed loop and open loop system is that closed loop utilise feedback and therefore is controlled. Control systems are used in all manors of situations, both military and civilian. An example of a control system most people would be familiar with would be Central Heating used in houses. It is a closed loop system meaning it uses feedback, this comes in the form of a Thermostat. The system will heat the house up to the temperature indicated on the Thermostat and will cut off the heat when this is reached. If the temperature drops below the indicated temperature, then the heating will be turned back on.
[bookmark: _Toc92083624][bookmark: _Ref92131808][bookmark: _Ref92131881][bookmark: _Ref92131885][bookmark: _Ref92131888]P.I.D. control systems
P.I.D stands for Proportional, Integral and Derivative. A P.I.D. controller is a feedback controller which uses the sum of all three of these actions according to Dormindo and Visioli [3]. 
The Proportional aspect is as the name implies, proportional to the current value of the control error, this does mean that as the difference between the output and the input tends towards 0, the correction of the proportional aspect will also tend to 0 meaning they will never meet, also known as a steady-state error.
The Integral aspect uses the integration of previous control error values to attempt to eliminate the steady-state error. If not tuned correctly this can cause overshoot as when the signal approaches 0 the Integral of the errors will shrink which will reduce the rate of change.
The Derivative aspect uses a derivative of the change in error to predict the system behaviour. This utilises the rate of change of the error which can be used to flatten or dampen the curve and reduce overshoot. 
[bookmark: _Toc92083625]What is a CIWS?
According to David Alexander [4] a Close-In-Weapons-System (CIWS) is a defence platform, typically naval, which is designed to engage small, fast-moving targets such as missiles, fast jets, small boats etc. which have gotten too close to the ship. CIWS usually use a gatling gun with a high fire rate but are typically quite short ranged. Speed and accuracy of target acquisition is of the utmost importance for any CIWS as the faster it can get on target the more likely it is to take the target out safely. There are several examples of CIWS currently in service around the world: Raytheon’s Phalanx and Thales’ Goalkeeper.
[bookmark: _Toc92083626]Simulation setups
[bookmark: _Toc92083627]Requirement for the System:
The control system for this report is required to bring the process under control within two seconds and with only a 5% overshoot. Table 1 shows the unique values for this specific CIWS.
	a
	b
	c

	4
	2
	3


[bookmark: _Toc92083678][bookmark: _Ref91541948][bookmark: _Ref92146047]Table 1 - Unique Values
The time requirement of two seconds means that the turret is required to get from wherever angle it starts at, to facing the target within that time limit. The maximum angle the turret will need to rotate though will be 180°. This considers that the turret will have inertia and will not be able to move instantaneously. 
The overshoot requirement of 5% is the level of accuracy for where the turret is pointing. A CIWS needs to be accurate to shoot its target down.
The values for a, b, and c represent a multitude of factors such as the mass of the turret, its diameter, the power of the motor used to turn the turret, internal friction etc. All these factors need to be accounted for to control the system and are represented in the transfer function of the plant (Equation 1)

[bookmark: _Ref91748827][bookmark: _Toc92083673]Equation 1 - Plant Transfer Function
[bookmark: _Toc92083628]Controller
The P.I.D. controller is represented by Equation 2. When this is applied to the Plant (Equation 1) it becomes Equation 3. Equation 3 shows what is also known as the Forward Transfer Function which excludes the feedback in the system.

[bookmark: _Ref92082955][bookmark: _Ref92082960][bookmark: _Toc92083674]Equation 2 - P.I.D. Controller Function

[bookmark: _Ref92083325][bookmark: _Toc92083675]Equation 3 - Controlled Plant Equation
[bookmark: _Toc92083629]Single Transfer Function

[bookmark: _Ref91816199][bookmark: _Toc92083676]Equation 4 - Single Transfer Function
In Equation 4, as there is no feedback function H = 1. Taking Equation 3 as G, this then expands out to Equation 5. This equation is comprised of all the components of the Controller (Kp, Ki, Kd & N), Plant (a, b, c), and the Feedback.

[bookmark: _Ref92004041][bookmark: _Ref92004046][bookmark: _Toc92083677]Equation 5 - Overall Transfer Function (Expanded)
[bookmark: _Toc92083630]Modelling the Process
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[bookmark: _Ref91748604][bookmark: _Ref91748600][bookmark: _Toc92083661]Figure 1 - PID circuit
[bookmark: _Toc92083631]Step
The step, or input, is simply representing an input which might be sent from the targeting system. The value will represent the angle which the turret needs to turn to.
[bookmark: _Toc92083632]Adder
The Adder takes the value from the Input and subtracts the feedback from this. This is how the feedback is incorporated as if the Output of the plant is greater than the Input the Input from the Adder to the System will now reflect this (this can be seen in Figure 3).
[bookmark: _Toc92083633]PID
This represents the Controller; this attempts to compensate for any changes to the system as described above on Page 3.
A controller needs to be “Tuned” to achieve the desired effect. For this report, Simulink has been used to tune the controller to acquire the values in Table 2. 
	kp
	70.5889

	ki
	23.2987

	kd
	45.1512

	N
	1304.7178


[bookmark: _Toc92083679][bookmark: _Ref92083062]Table 2 - P.I.D. Gain values
[bookmark: _Toc92083634]Plant
The plant is represented by the Transfer Function in Equation 1. This uses the 3 values in Table 1
[bookmark: _Toc92083635]Results
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[bookmark: _Ref92069491][bookmark: _Toc92083662]Figure 2 - Step Input
Figure 2 shows the step input, this is used for both the Simulation and the Single Transfer Function. It represents the signal which would be sent from the targeting system.
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[bookmark: _Ref92069643][bookmark: _Toc92083663]Figure 3 - Input after feedback
Figure 3 shows the input signal after being combined with the feedback signal. Between seconds 1 and 2 it can be observed to go negative; this shows the turret has overshot slightly and is then brought back to (close to) 0.
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[bookmark: _Toc92083664]Figure 4 - Output from Controller
XXX
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[bookmark: _Toc92083665]Figure 5 - Output from Plant
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[bookmark: _Toc92083666]Figure 6 - Single Transfer Function output
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[bookmark: _Ref92004077][bookmark: _Toc92083667]Figure 7 - Difference between Simulation and Single TF
The comparison between the Simulation and the Single Transfer Function (Equation 5) can be seen in Figure 7. This is the subtraction of the Single Transfer Function from the Simulation Output, and the difference is at most 4.5*10-16 which is negligible.
[bookmark: _Toc92083636]Pole-Zero diagram
Pole-Zero diagrams are used to show if a system is stable or not, it plots all the roots for a transfer function. Poles (denoted as X on the graph) are where the graph tends towards infinity i.e., the denominator tends to zero. Zeros (denoted as O on the graph) are where the graph tends towards zero i.e., the numerator tends to zero. xxx
The Zeros are not pertinent to this report as their location does not impact the stability of the system. 
There are four quadrants to the graphs XXX
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[bookmark: _Toc92083668]Figure 8 - Pole-Zero - Plant TF
	Poles

	-0.2500 + 0.8292i

	-0.2500 - 0.8292i


Table 3 - Plant Pole values
XXX
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[bookmark: _Toc92083669]Figure 9 - Pole-Zero - Controller TF
	Poles
	Zeros

	-1304.7
	-1.0884

	
	-0.4736


Table 4 - Controller Poles and Zeros values
XXX
[image: Graphical user interface

Description automatically generated]
[bookmark: _Toc92083670]Figure 10 - Pole-Zero - Single TF
	Poles
	Zeros

	-1293.3
	-1.0884

	-10.1
	-0.4736

	-1.3
	

	-0.4
	


Table 5 - Single TF Pole and Zero values
XXX
[bookmark: _Toc92083637]Nyquist Diagram
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[bookmark: _Toc92083671]Figure 11 - Nyquist Plot - Forward TF
XXX
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[bookmark: _Toc92083672]Figure 12 - Bode Diagram - Forward TF
XXX
[bookmark: _Toc92083639]Discussion
XXX
While using Simulink to tune the P.I.D. controller, the response time managed to get down to less than 4*10-3 seconds which would be physically impossible. This would also mean the controller would be closer to instability.
From Figure 7 it is possible to see that the difference between the Simulation and the Single Transfer Function if probably from rounding errors when taking the values for the P.I.D. controller
[bookmark: _Toc92083640]Conclusion
It can be concluded in this report that the Single Transfer Function does validate the Simulation of the Controller, Plant and Feedback system. Figure 7, showing the difference between the two to be close to 0 is evidence for this. 
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