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ANSWER ALL QUESTIONS


1. 
a. Identify the advantages and disadvantages that Static Routing has over Dynamic Routing.						(10 Marks)

b. Identify the advantages and disadvantages of Dynamic Routing.
(10 Marks)

2. 
a. Describe the process of Legacy Inter-VLAN Routing.	(10 Marks)

b. What implementation on Inter-VLAN routing is typically used now?  Describe its operation.							(10 Marks)


3. Redundancy increases the availability of the network topology by protecting the network from a single point of failure, such as a failed network cable or switch. When physical redundancy is introduced into a design, loops and duplicate frames occur.  
a. What algorithm prevents this?  				(2 Marks)
b. How does it do it?						(8 Marks)
c. What are the port roles, give a brief description of each.  Use a diagram to help explain your answer.						(10 Marks)

4. 
a. What is HSRP?						(5 Marks)
b. Describe how it operates. Include a diagram			(15 Marks)

5. 
a. [bookmark: _GoBack]What is EtherChannel?					(4 Marks)
b. Create a diagram to show the typical configuration of EtherChannel.
(6 Marks)
c. Identify and describe the advantages of EtherChannel.	(10 Marks)
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