Switch:

[image: ][image: ][image: ][image: ][image: ][image: ][image: ][image: ][image: ]



Router:
[bookmark: _GoBack][image: ][image: ][image: ][image: ][image: ][image: ][image: ]
image7.PNG
FastEthernetd/d unass igned
FastEthernetd/5 unassigned
FastEthernetd/6 unassigned
FastEthernetd,? unassigned
FastEthernetd/8 unassigned
FastEthernetd/9 unassigned
FastEthernet0/10 unassigned
FastEthernetB/11 unassigned
FastEthernet0/12 unassigned
FastEthernet0/13 unassigned
FastEthernet0/14 unassigned
FastEthernet0/15 unassigned
FastEthernet0/16 unassigned
FastEthernet0/17 unassigned
FastEthernet0/18 unassigned
FastEthernet0/19 unassigned
FastEthernet0,28 unassigned
FastEthernetd/21 unassigned
FastEthernetd/22 unassigned
FastEthernet0/23 unassigned
FastEthernet0,/24 unassigned
GigabitEthernet8, 1 unassigned
GigabitEchernet8/2 unassigned
siufl
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ommand Prompt

Autoconfiguration IPv4 Address.

Subnet Mask .
Default Gateway .

. DHCPV6 TAID . .
DHCPYV6 Client DUID.
DNS Servers .

NetBIOS over Tcpip.

Ethernet adapter Ethernet:

Connection-specific DNS Suffix
Description .

Physical Address.

DHCP Enabled. S
Autoconfiguration Enabled .
Link-local IPv6 Address .
1Pv4 Address.

Subnet Mask .

Default Gateway .

. DHCPv6 TAID . .

DHCPYV6 Client DUID.

DNS Servers .

NetBIOS over Tcpip.

C:\Users\Admin>

: 169.254.216.167 (Preferred)
255.255.0.0

: 469893196
00-01-00-01-23-4E-83-51-6C-0D-92-BF-B9-DO.
Feco!
Fec0:0:0:FFFF::2%1
Fece!
: Enabled

Intel(R) Ethernet Connection (2) I219-1M
8C-9D-92-BF-89-D8

: No

Yes

Fego: :esef:3c54:7ch3: C25a%14(Preferred)

: 172.16.11.254(Preferred)

255.255.255.6

172.16.11.1

: 168598930
©6-01-00-01-23-4E-83-51-6C-9D-92-BF -B9-D8
feco
Fec0:0:0: FFFF::2%1
feco
: Enabled
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Command Prompt

Jicrosoft Windows [Version 16.6.17763.678]
(c) 2018 Microsoft Corporation. All rights reserved.

Jc: \Users\admin>ping 172.16.10.254

pinging 172.16.16.254 with 32 bytes of data:
[Reply from 172.16.16.254: bytes=32 time<ims
[Reply from 172.16.16.254: bytes-32 time<ims TTL=-127
[Reply from 172.16.16.254: bytes-32 time<ims TTL=-127
[Reply from 172.16.16.254: bytes-32 time<ims TTL=-127

ping statistics for 172.16.16.254;
Packets: Sent = 4, Received = 4, Lost = © (8% loss),
approxinate round trip times in milli-seconds:
Minimum = @ms, Maximum - ems, Average = 6ms

Jc: \users\admin>




image10.PNG
banner motd “Clnauthorized access is prohibited?"C

line con
aceuora’? 10408000618
login

£ransport input none
stowbits 1

Line vty @

passuord " asevs2180500
ogin

line vty 5 15

passuord 7 630752180508
ogin

end
Rifishow ip interface brief
Any interface listed with OK? value "NO” does not have a valid configuratil

Interface IP-ddress OK? Method Status Pr}

e itBthomot0/8/0  172.16.10.1  YES manual up w)
GigabitEthernot@/8/1 172.16.11.1  YES manual up w)
Serialo/1/0 unassigned  NO unset doun ol
Sorialo/1/1 unassigned  NO unset doun ol

Ri#l
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COM? - Tera Term VT -

File Edit Setup Control Windo

x Type “show 2 for a list of subcommands
Rifishou running-config

Building configuration. ..

Current configuration : 3554 hytes

Last configuration change at 20:57:01 UIC Sun Apr ? 2013

version 16.9
service timestanps debug datetime msec

service timestanps log datetime msec

service password-encryption

platforn qfp utilization monitor load 80

no platforn punt-keepalive disable-kernel-core

ostnane Ri

oot-start-marker
hoot-end-marker

enable secret 5 $1$hUBISEFq1uNiPAZoT8r98gxRxyl

no asa new-nodel

no ip domain lookup,
ip admission watch-list expiry-time 0
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~Tera Term VT

Setup Control Window Help

no ip domain lookup
ip admission watch-list expiry—time O

subscriber templating
nultilink bundle-name authenticated

crypto pki trustpoint TP-self-signed—1783363698
enrollnent selfsigned

subject-nane on=105-S1¢-Signed-Cort if icate-1783363698
revocation-check none

rsakeypair TP-self-signed—1783363698

crypte pki certificate chain TP-self-signed-1783363698
certificate self-signed 01
30820330 30820218 030201 02020101 300DAGE9 20864886 F7ODBLGL O5050030
31312F30 2DB6A3IS5 B4A31326 494F532D 53656C66 2D636967 GE6L642D 43657274
69666963 6174652D 31373833 33363336 39383GIE 170D3133 30343037 32303435 S
35315017 ©D333030 31303139 30303830 305A3031 312F302D 06035584 03132649
4F532D53 656C662D 5369676E 65642D43 65727469 66696361 74652D31 37383333
36333639 38308201 22300D06 B92A8648 S6F7ADDL 01010500 0382010F 0308281
©AB28281 B190BOIE 9D29E431 36CEIFBD 969EDAID CFFZEDAY 07456276 SE481DAL
7D9F343F 339CD7BY C283F959 7FCFE97F SDFBAFSA 2B6DFCFF 1SF3828B 2065ECFD
6579CEB4 2018ASCF SBCD?790D 7CSFFBE@ 4DBS6444 0274BE9E B3123Fii 9E2F219F
3A6FL8C8 BI5CAS99 9EZ34F88 2FFB5932 8C1C8352 48BCSAZ1 2DEF@570 EGAB3CA4
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m ~Tera Term VT

File Edit Setup Contro

6579CEB
3A6FL8CE
43452765
32FDASAL
23D2B33B
CBECAFFC
CS7E7BLY
301F8663
F6301D86
308D8689
8024573
798CB8SE
1E@63007
34F82FCI
7F7D68EF
F46FO016
3D56B4F7
E@FAZ7DF

2018A8CF
B15CAB99
0OE2D135
4ABIBFED
7BDDSE?8
BF4DFEA4
B2D58203
55102364
03551 DAE
20864886
BIFSCE2E
AGFAFA45
46DIEACA
8EB65DCI
B415E977
ANIAZE2F
FEEDBB3F
EF514806

quit

license udi pid ISR4221/K? sn FGL2235928E
no license smart enable
diagnostic bootup level minimal

Window
SBCD?796D
9E234F88
C3C65B74
98768FCS
CE463A2E
6312C4E3
01808103
18301680
04168414
F7008161
7C95B362
824F7210
20671281
EF@SDIFE
19296887
16215F36
oDA18BC3
3943B1BC

Help
7CSFFBED
2FFB5932
E4CFAE@D
29338559
CS7B7E2F
75C1AECE
53305130
144CCF1D
4CCFLD78
05050003
F8ASBFGF
FOBAASCE
CA8378AD
OE3E{1A5
5DC9215E
AFCF1349
21B16E78
ACEALFG5

spanning-tree extend system-id

redundancy
mode none

4DB86444
8C1C8352
57064009
60604648
E5799B15
91DEA3E2
OFB6355
70FSEQZE
FSEO2EC6
82016100
24999CaE
E1D8BSFD
A78E4F3F
827BA043
E57222E5
464E52F7
75406D30
DE3B6DAS

0274BESE
48BCBAZ1
FDSGDBGE
4305E000
23629C57
AB152A04
1p138161
C6833557
83355797
OEBZEQ2F
0894E352
ABBE98DA
45D2D351
54582479
CESF938B
A2CEL6C8
3AC8IDFF

B3123F11
2DEF8570
94909088
576E2ABD
78ASEB63
3BAD3DSE
FFo4g530
97ACI18E
ACI18BEA
7B7CD6D4
BID63AE?
83BABDC?
9AF4CALE
4042043
8273411F
FC4985B7
1A6B784B

9E2F219F
EGAB3CA4
EEEOAESE
5S5DECAEY
859C59EC
BFSFSABL
030161 FF
OASBBOSE
SBEOSEF6
2CD5A264
F99FDIEZ
B550E6CF
50C7354C
6E66635E
538378F1
A31F2981
7918B70E
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redundancy
mode none

interface GigabitEthernetd/0/8
description connected to pob

ip address 172.16.18.1 255.255.255.0
negotiation aute

interface GigabitEthernetB/B/1
description connected to s1

ip address 172.16.11.1 255.255.255.0
 negotiation auto

interface Seriald/1/8

interface Seriald/1/1

p foruard-protocol nd
ip http server

ip http authentication local
ip http secure-server

control-plane
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COM? - Tera Term VT

Edit Setup Control Windo

terface Seriald/i/1

Fforvard-protocol nd
htep server

http authentication local
http secure-server

control-plane

Banner motd “Clinauthorized access is prohibited!

line con
aceuora’? 10408000618
login

£ransport input none
stowbits 1

Line vty @

passuord " asevs2180500
ogin

line vty § 15

passuord 7 630752180508
ogin
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ommand Prompt

C:\Users\Admin>ipconfig /all

windows IP Configuration

Host Name . LN261-NETLAB
Primary Dns Suffix’

Node Type . Hybrid

Ip Routing Enabled. No

WINS Proxy Enabled. No

Ethernet adapter Ethernet:

Connection-specific DNS Suffix
Description .

Physical Address.

DHCP Enabled. .
Autoconfiguration Enabled .
Link-local IPv6 Address .
1Pv4 Address.

Subnet Mask .

Default Gateway .

DHCPYV6 TATD . .

DHCPYV6 Client DUID.

DNS Servers .

Intel(R) Ethernet Connection (2) I219-1M
88-D7-F6-C2-A5-9F

+:0C7:27d4:1CF5:467e%3 (Preferred)
: 172.16.10.254 (Preferred)

255.255.255.6

172.16.16.1

: 243849266
©6-01-00-01-23-50-D6-8D-88-D7-F6-C2-A5-OF
: fece:

feco
NetBIOS over Tcpip. . . . . . . . : Enabled

Ethernet adapter Npcap Loopback Adapter:
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S1#shou running—conf ig
Building configuration

Current configuration : 1472 hytes

0:58 UTC Mon Mar 1 1993

Last configuration change at 0

version 15.2

no service pad

service timestanps debug datetime msec
service tinestanps log datetime msec
o service password-encryption

hostnane S1

poot-start-marker
boot-end-narker

n0 aaa new-model
systen ntu routing 1560
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ntrol  Windo

o ip domain-lookup

spanning-tree mode pust
spanning-tree extend systen-id

vlan internal allocation policy ascending

interface FastEthernetB/1

nterface FastEthernetB,/2
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FastEthernetd/3
FastEthernet/4
FastEthernetd/s
FastEthernetd/6
FastEthernetd,?
FastEtherneta/s

FastEthernetd,9

FastEthernetd/10
FastEthernetd/11
FastEthernetd/12
FastEthernetd/13

FastEthernet0/14
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FastEthernetd 19
FastEthernetd/15
FastEthernetd/16
FastEthernetd/17
FastEthernetd/18
FastEthernetd/19
FastEthernetd 20

interface FastEthernetd 21

interface FastEthernetd 22

interface FastEthernetd 23
FastEthernetd 24

GigabitEthernet8/1
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8 File  Edit

interface GigabitEthernetB/2

ip address 172.16.11.10 255.255.255.0

p default-gatevay 172.16.11.1
ip http server
ip http secure-server

o ustack
hanner motd “Clnauthorized access is prohibited?”C

Line con @
line vty 8 4

< passuord cisco
login

line vty § 15
password cisco
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File Edit Setup Nindow Help
Silichow ip interface brief

Interface IP-fddress ? Method Status
Ulani 172.16.11.18 manual up
FastEthernetd /1 unassigned unset  down
FastEthernetd,2 unassigned unset  down
FastEthernetd,3 unassigned unset  down
FastEthernetd/d unassigned unset  down
astEthernetd 5 unassigned unset  down
FastEthernetd/6 unassigned unset up
FastEthernetd/? unassigned unset  down
FastEthernetd/8 unassigned unset  down
FastEthernetd/s unassigned unset  down
FastEthernet0/10 unassigned unset  down
FastEthernetB/11 unassigned unset doun
FastEthernet0/12 unassigned unset  down
FastEthernetd/13 unassigned unset  down
FastEthernet0/14 unassigned unset  down
FastEthernet0/15 unassigned unset  down
FastEthernet0/16 unassigned unset  down
FastEthernet0/17 unassigned unset  down

FastEthernetd/18 unassigned unset  down
FastEthernetd/19 unassigned unset  down
FastEthernitE/ZE unassigned unset  down





