	Device
	Error
	Correction

	 RA
	IP interface and subnet mask is incorrect on G0/0. Tunnel address removed to prevent overlap error.
 
 
 
	interface Tunnel 0
no ip address
int g0/0
ip address 172.31.0.1 255.255.255.0

	RA 
	 Incorrect IP address on tunnel0
 
 
 
	 interface Tunnel 0
ip address 192.168.1.1 255.255.255.252

	 RA
	 Incorrect Static route
 
 
 
	no ip route 172.31.1.0 255.255.255.0 64.103.211.2

Ip route 172.31.1.0 255.255.255.0 192.168.1.2

	 RB
	Incorrect tunnel source port
	tunnel source Serial0/0/0

	RB
	 Incorrect tunnel destination address
 
 
 
	tunnel destination 209.165.122.2 



