Sarah Rule
1810755 – 1810755@student.uwtsd.ac.uk
Lab 7 – Basic Routing Configuration

1. Name of the IOS image that the router is running? 

[image: ]

2. Non-volatile random-access memory (NVRAM) does the router have? 

[image: ]

3. How much Flash memory does the router have? 

[image: ]


4. What is the boot process for the router on the next reload? 

[image: ]

5. How are passwords presented in the output?

[image: ]

Passwords are shown as encrypted and not in plain text. 

6. What code is used in the routing table to indicate a directly connected network? 

The code that indicates that a connection is directly connected is the letter ‘C’. 

7. How many route entries are coded with a C code in the routing table? 

[image: ]
There are 2 route entries coded with ‘C’ in the above routing table. 

8. What command changed the status of the Gigabit Ethernet ports from administratively down to up?  

The ‘no shutdown’ command changes the status of the Gigabit Ethernet ports from administratively down to up. 
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Configuration register is 0x2102
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nable password 7 0822455DOA16130308180D1739
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Router>show version
Cisco I0S Software, C2900 Software (C2900-UNIVERSALKS-M), Version 15.1(4)M4, RELEASE SOFTWARE (£c2)
Technical Support: BETp://wi.CisSco.com/techsupport

Copyright (c) 1986-2012 by Cisco Systems, Inc.

Compiled Thurs 5-Jan-12 15:41 by pt_team
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255K bytes of non-volatile configuration memory.
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Router>show flash

System flash directory:
File Length Name/status

3 33591768 c2900-universalkS-mz.SPA.151-4.M4.bin

2 28282 sigdef-category.xml

1 227537  sigdef-defaulc.xml
(33847587 bytes used, 221896413 available, 255744000 total]
249856K bytes of processor board System flash (Read/Write)
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