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I- IPv4 Addressing Table
	Specification
	Subnet A
	Subnet B

	Subnet IP address
	192.168.202.0
	192.168.202.128

	Subnet mask (slash notation)
	  /26
	/25

	Subnet mask (dotted decimal)
	255.255.255.192
	255.255.255.128

	1st Host IP address
	192.168.202.1
	192.168.202.129

	Last Host IP address
	192.168.202.62
	192.168.202.254

	Number of usable hosts per subnet
	62
	126

	Broadcast address
	192.168.202.63
	192.168.202.254



II- IPv4 Address assignment
	Device
	IP address
	Subnet Mask
	Gateway

	PC-A
	192.168.202.62
	255.255.255.192
	192.168.202.1

	R1-G0/0/0
	192.168.202.129
	255.255.255.128
	192.168.202.129

	R1-G0/0/1
	192.168.202.1
	255.255.255.192
	192.168.202.1

	S1
	192.168.202.2
	255.255.255.192
	192.168.202.1

	PC-B
	192.168.202.254
	255.255.255.28
	192.168.202.129



III- IPv6 Addressing Table
	Assigned to Interface
	IPv6 Subnet Address
	Prefix Length

	R1-G0/0/1
	2001:db8:acad:0001::0
	/64

	R1-G0/0/0
	2001:db8:acad:0002::0
	/64



IV-IPv6 Address assignment
	Device
	IPv6 address
	Prefix Length
	Gateway

	R1-G0/0/0
	2001:db8:acad:0002::1
	/64
	FE80::1

	R1-G0/0/1
	2001:db8:acad:0001::1
	/64
	FE80::1

	S1
	2001:db8:acad:0001::2
	/64
	2001:db8:acad:0001::1



Task 2: Device Configuration 
1) Hostname 

[image: O imagine care conține text

Descriere generată automat]
2) Encrypted privileges EXEC password 
[image: O imagine care conține text

Descriere generată automat]

3) Secure the console access password


4) Minimum length passwords


5) Create an administrative user 


6) Configure an MOTD banner 


7) Encrypt all passwords 


8) Disable IP domain lookup 


9) Enable synchronous logging 


10) Configure router’s interfaces 


11) Configure switch’s management (SVI) interface 









Task 3: Verify Network connectivity 


	From
	To
	Protocol
	IP Address
	Ping Results

	PC-A
	R1 G0/0/0
	IPv4
	
	

	tftttttttPC-A
	R1 G0/0/0
	IPv6
	
	

	PC-A
	R1 G0/0/1
	IPv4
	
	

	PC-A
	R1 G0/0/1
	IPv6
	
	

	PC-A
	S1 VLAN 1
	IPv4
	
	

	PC-A
	S1 VLAN 1
	IPv6
	
	

	PC-A
	PC-B
	IPv4
	
	

	PC-A
	PC-B
	IPv6
	
	

	PC-B
	R1 G0/0/0
	IPv4
	
	

	PC-B
	R1 G0/0/0
	IPv6
	
	

	PC-B
	R1 G0/0/1
	IPv4
	
	

	PC-B
	R1 G0/0/1
	IPv6
	
	

	PC-B
	S1 VLAN1
	IPv4
	
	

	PC-B
	S1 VLAN1
	IPv6
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