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[bookmark: _Hlk54105057]Project: FOGS
[bookmark: h.1kmozguib79q]Site address:
Plot E3b 
South Of Fabian Way  
Langdon Road 
Swansea Docks 
Swansea SA1 8QY 
Date of works: TBC
Description of activity
· Erecting the steel frame.

Involves:
· The steel frame arriving on site from the factory
· Cranes being used to move the heavy steels into place
· Connecting the steel beams on columns together
· Use of power tools
· Operatives working at heights 

[bookmark: h.ygmyk6vg3h9j]Supervision and Personnel
· Site Manager - TBC
· Jehu Supervisor – TBC
· Health and Safety advisor – TBC
· Site Engineer - TBC
[bookmark: h.ocmnip9mxfv8]Training
· All operatives are adequately trained to carry out required tasks.
· All site operatives must hold the relevant CSCS certification.
· Additional health and safety training given if required.  
· Additional training can be given to operatives working at height.
· Steel erecting training to be carried out
· Toolbox talks to be given regarding tools used to join the steels.

[bookmark: h.r46xzs9m3ioz]Legislation
· Health and Safety Work Act 1974 (UK. Gov, 1974)
· The Management of Health and Safety at Work Regulations 2006 (HSE, 2006)
· Workplace (Health, Safety and Welfare) Regulations 1992 (UK. Gov F, 1992)
· The Personal Protective Equipment at Work Regulations 2002 (UK. Gov E, 2002)
· The Construction (Design and Management) Regulations 2015 (UK. Gov D, 2015)
· The Working from Height Regulations 2005 (UK. Gov C. 2005)
· The Control of Vibration at Work Regulations 2005 (UK. Gov B, 2005)


[bookmark: h.2cpfsm4rqcx7]While working
[bookmark: h.ddte95cmjn8g]Before any work commences, the Site Manager must ensure all operatives on site have the correct qualifications to erect steel frames and if required, give a toolbox talk on any power tools being used. Crane slingers and operatives moving the steels are to be aware of the site layout and any pedestrians or other trades on site and ensure extra caution when moving. Operatives working at heights are to ensure any additional PPE such as harness and shock absorber is used if guard rails are not in place. All operatives on site are to be aware of potential falling objects and are not to work in those areas of risk. All operatives are to be aware of the correct manual handling techniques and should not attempt to lift heavy items without the use of a crane.
PPE requirements
· Hard hats
· Safety boots
· Hi-vis vest
· Safety gloves
· Safety glasses
· Additional High Vis for working on rail lines.
· Harness for operatives working at height
· Hearing protection
[bookmark: h.jjom1h6ke549]Welfare
Welfare arrangements are supplied by the principal contractor.
These should be in line with Schedule 2 of the Construction Design & Management Regulations 2015 (CDM). All sites are to have a minimum amount of welfare facilities available for workers, which include the following:

· Toilets
· Washing facilities
· Drinking water
· Changing rooms and lockers
· Heating
· Rest facilities
[bookmark: h.zai7l19dxpwv]First aid
· Refer to the onsite safety notice board for all first aid information. 

· The first aid box is adequate to the size of the site and will be checked regularly to ensure it is in the correct state.

· The Principal Contractor should nominate an appointed person to take care of first-aid arrangements. 

· The number of appointed first aiders shall be dependent on the number of employees but is yet TBC.
[bookmark: h.ye0kne5onkgh]Emergency procedures
· The Principal Contractor will ensure that the existing site emergency procedures are followed and that relevant information is given to operatives during the site induction given by the Assistant Manager or when changes are made to procedures.

· The closest hospital is: Morriston Hospital, Heol Maes Eglwys, Cwmrhydyceirw, Morriston SA6 6NL
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