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METHOD STATEMENT 
(Piling) 
 
THE PILING WORKS 
 
The work comprises the construction of 300mm diameter piles. 
 
The piles are designed by South Wales Piling Limited for loading specified by the design Engineers. 
 
The pile layout will confirm to and be design around Activ Leisure Ltd Drawings
 
Pile construction details are to standard details.  
 
The piling platform (PPL) and commencing surface (CSL) level is existing ground level.   
 
MANAGEMENT AND PERSONNEL 
 
The works will be managed from the office in Swansea. 
Telephone: 	XXXXX XXX XXX 	 	 	 
E-mail  info@activleisure.co.uk
 
The Management Team: 
Contracts Manager – Jon Langstone 
Project Manager – Chris Atkinson 
Commercial Manager – Jenny Stroud 
Quantity Surveyor – Tobias Adamson 
Design Manager – Cameron Evans 

Crew Members will be allocated nearer the contract start date.

The minimum training / competence achievement for the crew appropriate to their designation are: NVQ / CSCS / SSSTS 
 
Records for each crew member will be provided on request. 
 
Not more than one member of the crew may be a trainee in his designated role. 
 
PERSONAL PROTECTIVE EQUIPMENT 
 
The following personal protective equipment will be used at all times: 
· Safety Helmet
· Protective Footwear 
· Gloves to
· Hi Viz Vest
· Light Eye Protection  

. 



SITE HAZARDS 
 
The piling rig is a self-erecting hydraulic type, has a mast height of 25 – 30m and will operate at all times with it’s mast between its tracks  
 
With due regard to any rules restricting rig operation, As Principal Contractor we will demark that area in which work is restricted. 
 
Any Buried services will be located and then diverted or protected by the Principal Contractor prior to piling. 
 
There are no overhead cables or the like which restrict rig movement. 
 
Project Management will issue a Permit To Work and Permit to Dig before any piling activity commences. 
 

MAIN CONTRACTOR’S ATTENDANCE 
 
Principal Contractors’ attendance includes the following principal items: 
 
· Provision of welfare facilities 
· Identification, diversion or protection of services 
· Protection of adjoining roadways 
· Traffic management 
· Provision and maintenance of access and piling platform(s) 
· Certification of the design and construction of the working platform(s) 
· Pile setting out and level control.

MATERIALS 
 
Concrete will be ready mixed and supplied from a plant registered under the QSRMC or similar accreditation scheme. 
 
Reinforcement will be supplied from a CARES registered supplier. 
 
Reinforcement cages will be fabricated on site. 
 

SEQUENCE OF PILE CONSTRUCTION 
 
The sequence of piling will be determined on site by the Piling Foreman to a planned sequence designed to avoid damage to newly constructed piles, existing construction and services. 
 




CONSTRUCTION TECHNIQUE 
 
The piling rig will be set up centrally over the pile position. 
 
A lead casing will be positioned centrally over the pile position.  
 
At commencement of driving, small hammer drops shall be employed until the plug has been compacted and the casing is stable. 
 
The lead casing will be checked for position and verticality as installation proceeds. 
 
The pile will be further driven until it attains its specified set or depth. 
 
Upon reaching final set or depth the driving hammer will be withdrawn and the internal depth of the pile measured and recorded.  
 
This casing is permanent and will not be extracted; it remains part of the permanent works. 
 
Concrete will be placed centrally into dry casings.  Special measures are required where concrete is to be placed under water or where grout is to be used.  Such measures are outside the scope of this method statement. 
 
Short reinforcement cages may be inserted after concreting.  Otherwise reinforcement will be inserted prior to concreting or during the concreting operation when the level of the concrete is at its highest level consistent with cage installation. 
 
QUALITY 
 
The Piling Foreman will notify his Manager of any departure from this statement.
 
ON-SITE TRAINING 
 
The Principal Contractor will provide induction training to all personnel on their arrival.  The induction is to include site emergency procedures. 
 
The Piling Foreman will brief all operatives prior to commencement of piling works. 
 
Toolbox talks will be carried out as reasonably required by the Principal Contractor. 











 
RECORD OF BRIEFING 
 
I confirm that I have read and understood this method statement and associated risk assessments.  I agree to work in accordance with the systems of work as described and as directed by the Company. 
 
	Name 
	Signature 
	Date 
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